[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered.
· The contract will be awarded to the lowest-cost technically compliant bid/item.
· The quantities mentioned below are required unless there is a variation within a specified range with proper justification. The LRC reserves the right to increase or decrease the quantities.
· The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.  
· In the event of any discrepancy between the unit price and the total price, LRC reserves the right to rely on the unit price as stated in the financial bid, rather than the total price without going back to the supplier. The unit price must be provided with no more than two decimal places.
· Only one option is allowed for biding 
· Sample/datasheet for each item must be submitted with the bid and labelled reference to each item number (please refer to annex 3)
· LRC reserves the right to award the items per LOT.
	LRC To Complete
	Bidder to Complete 

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT rated at 11%, but inclusive Labor, packing, packaging, Bank Transfer Fees, Delivery and all other fees 
	VAT (%)
	Unit Price in USD, inclusive VAT, Labor, packing, packaging, Bank Transfer Fees, Delivery and all other fees
	Total Price in USD, inclusive VAT, Labor, packing, packaging, Bank Transfer Fees, Delivery and all other fees
	Lead time of delivery for any quantity from the date of each purchase order 

	1.1
	Safety Warning Triangle
	Pc
	200
	
	
	
	
	

	1.2
	Snow Chain for Tires (195/80R15)
	Set
	75
	 
	 
	 
	
	

	1.3
	Snow Chain for Tires (265/75R16)
	Set
	55
	 
	 
	 
	
	

	1.4
	Safety Cone Medium Size
	Pc
	80
	
	
	
	
	

	1.5
	Safety Cone Large Size
	Pc
	130
	
	
	
	
	

	1.6
	Safety Cone Foldable
	Pc
	230
	
	
	
	
	

	1.7
	Booster Jump Starter Portable
	Pc
	60
	
	
	
	
	

	1.8
	Cable Jumper
	Set
	70
	
	
	
	
	

	1.9
	Working Gloves
	Set
	200
	
	
	
	
	

	1.10
	Screwdriver Cross Head
	Pc
	120
	
	
	
	
	

	1.11
	Screwdriver Flat Head
	Pc
	120
	
	
	
	
	

	1.12
	Plier
	Pc
	120
	
	
	
	
	

	1.13
	Spanner 10mm
	Pc
	120
	
	
	
	
	

	1.14
	Tow Cable / Recovery Strap (5m)
	Cable
	60
	
	
	
	
	

	1.15
	Ring Anchor Shackles
	Pc
	60
	
	
	
	
	

	1.16
	Siren
	Unit
	10
	
	
	
	
	

	1.17
	Tire Puncture Repair Kit
	Set
	50
	
	
	
	
	

	1.18
	Tire Sealer & Inflator
	Set
	100
	
	
	
	
	

	1.19
	Hydraulic Car Jack + Tire Inflator 12V
	Pc
	147
	
	
	
	
	

	1.20
	Magnet Mount Light Bar
	Pc
	135
	
	
	
	
	

	1.21
	Vehicle Jack (Scissor Type)
	Set
	130
	
	
	
	
	

	1.22
	Wheel Spanner
	Pc
	120
	
	
	
	
	

	1.23
	Fire Extinguisher (2 kg)
	Pc
	150
	
	
	
	
	

	1.24
	Car Drying Towel
	Set
	130
	
	
	
	
	

	1.25
	Ratchet Straps 5 Tons
	Set
	70
	
	
	
	
	

	1.26
	Ratchet Straps 1 Ton
	Set
	60
	
	
	
	
	

	1.27
	Socket and Tool Set (137 pcs)
	Set
	105
	
	
	
	
	

	1.28
	12 pcs 3/8" Ratchet Handle With Socket Set
	Set
	27
	
	
	
	
	

	1.29
	13 mm spanner
	Pc
	110
	
	
	
	
	

	1.30
	Cutter
	Pc
	110
	
	
	
	
	

	1.31
	Heavy-duty plastic tool bag to store all the equipment
	Box
	120
	
	
	
	
	

	
	Total 
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ANNEX 3: DETAILED SPECIFICATIONS 

I. [image: ]Safety Warning Triangle 
Type: Foldable reflective warning triangle
Material: Durable plastic with reflective surface
Color: Red with high-visibility reflective coating
Dimensions: Side length 40–45 cm
Visibility: Minimum 150 meters
Construction: Foldable design with stable support stand
Features: Weather resistant (heat, UV, water), lightweight, compact storage case,
Sample is required
II. Snow Chain for Van/Ambulance 
[image: ]Type: Ladder or Diamond pattern 
Material: Heavy duty steel
Link thickness: 5 mm minimum
Pattern: Full chain coverage
Tensioning: Manual or ratchet system
Finish: Rust Resistant
Supply: Set of two chains
Compatible with size: 195/80R15/Van 
Sample is required
III. Snow Chain for SUV
Type: Ladder or Diamond pattern 
Material: Heavy duty steel
Link thickness: 5 mm minimum
Pattern: Full chain coverage
Tensioning: Manual or ratchet system
Finish: Rust Resistant
Supply: Set of two chains
Compatible with size: 265/75R16/SUV
Sample is required
IV. [image: ]Safety cones Medium Size:
Type: Traffic / Safety Cone 
Height: Minimum 500 mm 
Material: Flexible PVC or durable rubber base 
Color: High-visibility orange 
Reflective Bands: two white reflective bands (high-intensity grade) 
Base: Weighted or wide anti-slip base for stability 
Weather Resistance: UV resistant, suitable for outdoor use 
Features: Impact-resistant, stackable design for storage 
Sample is required


V. [image: Why Every Vehicle Should Have a Collapsible Safety Cone Kit » OTW Safety]Safety cones Foldable:
Type: Traffic / Safety Cone 
Height: 30 - 40 cm 
Material: Flexible PVC or durable rubber base 
Color: High-visibility orange 
Reflective Bands: two white reflective bands (high-intensity grade) 
Base: Weighted or wide anti-slip base for stability 
Weather Resistance: UV resistant, suitable for outdoor use 
Features: Impact-resistant, stackable design for storage, storage bag.
Sample is required

[image: ]
VI. Safety cones Big Size:
Type: Traffic / Safety Cone 
Height: Minimum 70 - 75 cm
Material: Flexible PVC or durable rubber base 
Color: High-visibility orange 
Reflective Bands: two white reflective bands (high-intensity grade) 
Base: Weighted or wide anti-slip base for stability 
Weather Resistance: UV resistant, suitable for outdoor use 
Features: Impact-resistant, stackable design for storage 
Sample is required
VII. [image: ]Booster Jump Starter Portable size.
Battery Cell Composition: Lithium

Voltage: 12v
Vehicle Service Type: Passenger car, motorcycle, Van, Truck
Battery Capacity: 2000 – 3000 Milliamp Hours
Amperage 1000Amps
About this item
· Start Dead Batteries - Safely jump start a dead battery in seconds with this compact, yet powerful, 1000-amp lithium battery jump starter - up to 20 jump starts on a single charge - and rated for gasoline engines up to 6.0-liters and diesel engines up to 3.0-liters.
[image: ]In The Box - Ultra Safe Portable Car Jump Starter, Heavy Duty Booster Clamps, 12-Volt Car Charger, Micro USB Charging Cable, Microfiber Storage Bag, User Guide, 1-Year Warranty, and Designed in the USA or EU or similar quality.
Datasheet is required

VIII. Cable Jumper
Cable Gauge: 4 to 6 gauge 
Length: 4 to 7.5 meters 
Cables: Pure copper 
Clamps: Heavy-duty, preferably coated to prevent rust and improve grip
Amperage Rating: 400 to 800 amps 
Clamps: Strong spring-loaded clamps for a secure connection, Color-coded (red for positive, black for negative) for safety and ease of use
Compatibility: Suitable for various vehicle types, including cars, trucks, SUVs, and motorcycles
Carrying Case includes a storage bag or case for easy transport and organization.
Safety Features: Insulated handles to protect against electric shock.
Sample is required

IX. [image: ]Working Gloves
Nitrile-coated work gloves.
Seamless nylon/polyester liner.
Good grip in dry and oily conditions
Color: Blue
Elastic knitted wrist cuff.
Available in sizes M, L.
Suitable for general handling, warehouse, transport, and maintenance work.
Sample is required.

X. Screwdriver Cross Head
Type: Phillips (Crosshead) Screwdriver 
[image: ]Size: PH2 (Medium) 
Shaft Material: Heat-treated chrome vanadium steel. 
Tip: Magnetic crosshead tip 
Shaft Finish: Corrosion-resistant finish. 
Handle: Ergonomic anti-slip rubber grip 
 Overall Length: 200–250 mm 
Features: High-torque design, durable construction, comfortable grip for prolonged use
Application: Suitable for vehicle maintenance, mechanical repairs, and general workshop use. 
Sample is required.

XI. Screwdriver Flat Head
Type: Slotted (Flat Head) Screwdriver 

[image: ]Blade Size: 6 mm (Medium) 
Shaft Material: Heat-treated chrome vanadium steel. 
Tip: Magnetic flat-head tip 
Shaft Finish: Corrosion-resistant finish. 
Handle: Ergonomic anti-slip rubber grip 
Overall Length: 200–250 mm 
Features: High-torque design, durable construction, comfortable grip for prolonged use 
Application: Suitable for vehicle maintenance, mechanical repairs, and general workshop use.
Sample is required







XII. Plier
Type: Combination Pliers 
[image: ]Size: 8 inches (200 mm) 
Material: Drop-forged, heat-treated chrome vanadium steel 
Finish: Corrosion-resistant finish 
Jaws: Serrated gripping jaws with integrated wire cutter 
Grip: Ergonomic anti-slip handle for secure handling 
Features: Heavy-duty construction, smooth pivot action, high gripping, and cutting performance 
Application: Suitable for vehicle maintenance, mechanical repairs, gripping, twisting, bending, and cutting wires and small components.
Sample is required

XIII. [image: ]Spanner
Type: Ratchet combination spanner (open-end + ring ratchet) 
Size: 10 mm 
Material: Chrome Vanadium (Cr-V) steel 
Finish: Mirror polish or chrome plated, corrosion-resistant 
Ratchet Mechanism: 72-tooth (or higher) fine ratcheting system. 
Direction: Reversible ratchet (forward/reverse switching) 
 Head Angle: Offset ring head (typically 15°) 
Design: Slim profile for access to tight engine compartments 
Strength: Heat-treated for high torque resistance 
Application: Suitable for vehicle maintenance, mechanical assembly, and confined space fastening tasks.
Sample is required

XIV. Spanner
[image: TTI 13mm Metric Ring & Open End Combination Spanner TCSM13 | Total Tools]Type: Ratchet combination spanner (open-end + ring ratchet) 
Size: 13 mm 
Material: Chrome Vanadium (Cr-V) steel 
Finish: Mirror polish or chrome plated, corrosion-resistant 
Ratchet Mechanism: 72-tooth (or higher) fine ratcheting system. 
Direction: Reversible ratchet (forward/reverse switching) 
 Head Angle: Offset ring head (typically 15°) 
Design: Slim profile for access to tight engine compartments 
Strength: Heat-treated for high torque resistance 
Sample is required

XV. [image: ARB 4x4 Accessories ARB705LB Orange 30' x 2 3/8" Snatch Strap Recovery, 1  Pack, Towing Straps & Ropes - Amazon Canada]Tow Cable / Recovery Strap – 5m. 
Type: Recovery strap (tow cable)
Length: 5 meters
Material: High-strength polyester webbing
Width: 70–80 mm
Minimum Breaking Strength: ≥ 12,000 kg
Construction: Reinforced eye loops with protective sleeves
Features: Low stretch, weather resistant, high visibility
Compatibility: Suitable with rated shackles and recovery points
Sample is required

XVI. Ring Anchor Shackles (Bow / D-Shackle)
[image: ]Type: Screw pin bow shackle (D-ring)
Material: Drop-forged high-strength steel
Pin Diameter: 16–19 mm
Working Load Limit (WLL): ≥ 4.75 tons
Breaking Strength: ≥ 20,000 kg
Construction: One-piece forged body with threaded screw pin
Features: Corrosion resistant, suitable for towing and recovery
Compatibility: Use only with rated recovery points and straps
Sample is required
XVII. Siren Specifications
[image: ]100 Siren with PA noise canceling microphone
Siren Tones, PA, Radio rebroadcast and air horn
Library of selectable siren tones
Horn ring transfer and park kill
(4) programmable inputs, plus dedicated inputs for park, horn, and ignition
Convergence network configuration software allows for easy customization of the siren
Five-year Warranty minimum.
Siren with self-contained controls 100W.
Specifications
Power 100W
Input voltage 11 – 28 VDC
Nominal output voltage 64V peak to peak.
Standby Current <0.1A
Max input current 10A 
Frequency range 182 to 1600 hz
Operating temperature -40 to +80 Degree Celsius
Height 6.4cm
Length 15.2cm
· Width 20.5cm
· can be powered via the vehicle’s power center or directly from the vehicle’s battery.
· Origin: Manufactured in Europe, USA.
Datasheet is required.










XVIII. Tire Puncture Repair Kit
[image: ]Type: Manual tire repair kit (for tubeless tires) 
Includes: 
Insertion tool 
Probe tool 
Repair plugs (at least 5 pcs) 
Adhesive (glue) 
Cutter or Blade
Function: Temporary repair of small punctures 
Easy to use (no electricity required) 
Packed in a small portable case 
Instructions included 
Suitable for cars, SUVs, and light trucks
Sample required

XIX. Tire Sealer & Inflator – Specifications
[image: ]Type: Aerosol tire sealer and inflator (2-in-1).
Capacity: 400–450 ml per can.
Seals small tire puncture and inflate the tire instantly.
Provides temporary emergency repair to allow the vehicle to reach a workshop.
Seals puncture up to approximately 4–5 mm.
Fast operation within a few minutes.
Works without removing the tire.
No tools or jack required.
Easy connection to tire valves via hose/nozzle.
Simple one-step application.
Suitable for cars, light vehicles, and vans.
Compatible with tubeless tires only.
Contains a sealant and compressed gas formula.
Non-corrosive and safe for rims and tires.
Supplied in an aerosol can with hose/nozzle.
Properly sealed and suitable for storage in vehicles.
Minimum shelf life of 2–3 years.
Flammable aerosol.
Clear instructions and safety warnings printed on the can.
Sample required.

XX. [image: ]Hydraulic Car Jack + tire inflator 12V
Type: Electric Hydraulic Car Jack
Capacity: 5 Ton
Voltage: 12V DC
Lifting Range: 150mm – 450mm (15–45cm)
Power Source: Car cigarette lighter / Battery clamp
Functions: Lifting + Tire Inflator + LED Lighting
Safety Features: Overload protection, anti-slip head
Suitable Vehicles: Sedan, SUV, MPV, pickup, light truck
Datasheet is required.

XXI. Magnet Mount Light Bar Specifications
Features
[image: ]Low-profile 15” mini-light bar
Unique edge cruise lighting available in dual color model
(25) flash patterns
Multi voltage 12/24v
Magnet mount
Five-year warranty
Blue light only

Specifications
Operating voltage 12/24 vdc
Current draw 2.0 A @ 12VDC/ 1.0A @ 24 VDC
Operating temperature -40 to +65 degrees Celsius 
Length 37.2 cm
Width 21.5cm
Height 5.4
Origin: Manufactured in Europe, USA.
Datasheet is required 

XXII. [image: ]Vehicle Jack (Scissor Type)

Type: Compact scissor jack, suitable for in-vehicle storage.
Capacity: Minimum lifting capacity of 2 tons (suitable for SUV weight).
Operation: Manual, with crank/handle provided.
Construction: Heavy-duty steel, rust- and corrosion-resistant finish.
Safety: Wide base plate for stability on uneven or soft surfaces.
Storage: Compact and lightweight design for storage inside the vehicle
Sample is Required

XXIII. [image: ]Wheel Spanner

Type: Cross spanner.
Material: Hardened, corrosion-resistant steel.
Size: suitable for SUV’s and sedan
Durability: Strong enough for repeated use without bending.
Socket Sizes: 17, 19, 21, 23mm. 
Sample is Required
[image: C:\Users\LRC\Desktop\iStock-518534038.jpg]
XXIV. Car drying towel

Microfiber
90x60cm 
Thickness 600-1000 GSM
Sample is Required

XXV. [image: ]Ratchet straps 5 tons
Ratchet straps with claw hook
5tons x10m
Color Blue
Material: Heavy duty
Suitable for outdoor use
Sample is Required

XXVI. Ratchet straps 1 ton
[image: ]Type: Retractable ratchet tie-down strap
Load Capacity: 1 Ton (1,000 kg minimum breaking strength)
Working Load Limit (WLL): Minimum 300–500 kg
Strap Width: 25 mm
Material: High-strength polyester webbing
Finish: Zinc-plated or powder-coated metal components
UV Resistance: Yes, suitable for outdoor use.
Abrasion Resistance: High durability for repeated use
Operation: One-hand tightening and automatic retraction system
Application: Securing light cargo in vans, pickups, and small trucks
Safety: Designed for safe transport load securing applications
Sample required
XXVII. Socket and Tool set 137pcs.
Sockets
10 × 1/2″ drive standard sockets (18–32mm)
[image: ]9 × 3/8″ drive standard sockets (10–19mm)
12 × 1/4″ drive standard sockets (4–13mm)
Deep sockets for 1/2, 3/8, and 1/4″ drives
Ratchets & Drive Tools
3 × 72-tooth reversible ratchets (1/4, 3/8, 1/2)
Extension bars for all drive sizes
Universal joints and socket handles
Flexible and offset handles.
Screwdriver Bits (33pcs Cr-V)
Phillips, Posidrive, Slot, Hex
Torx and Torx with hole
Square and M-type bits
Hand Tools
15 × Combination spanners (6–21mm)
9 × Hex key set (1.5–10mm)
Combination pliers (7″)
Long nose pliers (6″)
Locking pliers (10″)
Machinist hammer – 300g
Screwdrivers and nut driver
Sample is Required

XXVIII. [image: ]12Pcs 3/8″ Ratchet Handle with Socket Set
10pcs metric CrV sockets: 8,10,11,12,13,14,16,17,18,19mm
1pc CrV extension bar:75mm
1pc two-component ergonomic ratchet handle, 72T, CrV, quick release
Packing: plastic hanger with color label
Sample is Required

XXIX. Cutter
[image: Buy Utility Knife Paper Cutter-Big E2061 at Hardwarepasal.com || Online  Shopping in Kathmandu Nepal]Heavy-duty 18 mm utility cutter. 
Ergonomic high-impact plastic body with reinforced metal blade guide. 
Replaceable 18 mm SK5 high-carbon steel snap-off blade (0.5 mm thickness). 
Secure sliding blade locking mechanism for safe operation. 
Suitable for cutting cardboard, paper, plastic, packaging materials, and other general-purpose applications
Sample is required


XXX. Heavy-duty plastic tool bags to store all the equipment. 
Heavy-duty durable plastic protective equipment case (rigid shell design) 
Made from high-impact resistant polypropylene (PP) or similar engineering plastic. 
Shockproof and crush-resistant structure for protection of sensitive tools and equipment 
[image: Black Shockproof Tool Box ABS Plastic Hard Carry Case Safety Equipment  Instrument Portable Tool Box Impact Resistant Tool Case Foam Buy cheaply on  Joom]Ergonomic top handle for secure and comfortable carrying. 
Reinforced locking latches for safe closure and transport security 
Stackable design for efficient storage and transport optimization 
Ribbed external frame for added strength and durability. 
Resistant to dust, moisture, and light water exposure (splash-resistant) 
Suitable for tools, electronics, and field equipment storage 
Available in multiple sizes for different equipment storage requirements
Sample is required.
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HEAVY-DUTY JUMP-START CABLES
- PRODUCT SPECIFICATIONS

« Cable Gauge: 4106 AWG (Pure Copper
Conductors)

« Length: 4107.5 meters (Selectable optons)

« Amperage Rating: 4000 800 AMPS

= Clamps: Strong,spring-loadd, heavy-cuty
clamps with insulated handlos. Plated for
rustpreventon.

= Clamp Coloring: Red (1) fo Posiive,
Black () for Negative.
« Compatiily: Suitable forcars, trucks,
SUV, and motorcycis.

« Safety Features: Insulated handies protect
againstelectric shock.

= Canying Case: Includes a durable Zppered
storage bag for easy tansport and
organization.
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