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Tender reference: 2026-069
[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered.
· The contract will be awarded to the lowest-cost technically compliant complete lot or complete bid. 
· The quantities mentioned below are required unless there is a variation within a specified range with proper justification. The LRC reserves the right to increase or decrease the quantities.
· The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.  
· In the event of any discrepancy between the unit price and the total price, LRC reserves the right to rely on the unit price as stated in the financial bid, rather than the total price without go back to the supplier. The unit price must be provided with no more than two decimal places.
· Only one option is allowed for biding 
· The bidder shall price each of the three distribution-line schedules separately. All unit rates shall include labor, materials, equipment, transport, testing, permits, overheads, incidental works, and all obligations necessary for the complete execution and handover of the works.
LOT 1:  Al Ain Village 
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1
	General 
	 
	 
	 
	 
	 
	 

	The Contractor shall carry out all general works required for the successful execution of the project, including mobilization and demobilization, site inspections, topographic survey and setting out, preparation and submission of shop drawings and as-built drawings, coordination with relevant stakeholders, obtaining necessary approvals and permits, and provision of all labor, equipment, materials, transportation, supervision, health and safety measures, and temporary works required for the completion of the contract. All works shall be carried out in accordance with the specifications, drawings, and Engineer's instructions.

	1.1
	Topographic Survey and Setting Out Works
	LS
	1
	 
	 
	 
	 

	1.2
	Preparation and Submission of Shop Drawings and As-Built Drawings
	LS
	1
	 
	 
	 
	 

	2
	Pipeworks
	 
	 
	 
	 
	 
	 

	2.1
	Pipes 
	Lm
	220
	 
	 
	 
	 

	2.2
	Asphalt Cutting 
	Lm
	220
	 
	 
	 
	 

	2.3
	Trench Excavation 
	Lm
	220
	 
	 
	 
	 

	2.4
	Sand bedding and surrounds
	Lm
	220
	 
	 
	 
	 

	2.5
	Laying of HDPE Pipe 
	Lm
	220
	 
	 
	 
	 

	2.6
	Backfilling of Trenches Including Compaction and Testing
	Lm
	220
	 
	 
	 
	 

	3
	Road Reinstatement 
	 
	 
	 
	 
	 
	 

	3.1
	Supply and placement of  asphalt to reinstate the road surface over trench areas, 10 cm thickness. Works include surface preparation, priming, laying of base and wearing courses, mechanical compaction, and finishing to restore road conditions to original or as specified by the local authority.
	m2
	88
	 
	 
	 
	 

	4
	Valves and Piping Works 
	 
	 
	 
	 
	 
	 

	4.1
	Connection of a 63 mm OD HDPE pipeline to an existing 6-inch ductile iron pipeline, including all necessary saddles, fittings, adaptors, excavation, tie-in works, testing, and reinstatement, complete in all respects.
	Piece
	1
	 
	 
	 
	 

	4.2
	SB-01 & SB02 - Supply and installation of a 2-inch gate valve complete with a round ductile iron surface box, including connection to a 63 mm OD HDPE pipe. The works shall include all necessary fittings, supports, sealing gaskets, chamber adjustments, alignment, anchoring, pressure testing, and reinstatement of disturbed areas.
	Piece
	2
	 
	 
	 
	 

	4.3.1
	2-inch bronze gate valve, PN16 with wash-out extension pipe inside Manhole
	Piece
	1
	 
	 
	 
	 

	4.3.2
	2-inch bronze check valve, PN16
	Piece
	1
	 
	 
	 
	 

	4.3.3
	2-inch bronze gate valve, PN16 for isolation
	Piece
	1
	 
	 
	 
	 

	4.3.4
	Pressure gauge Ø 100 glycerine-filled, stainless-steel case, pressure range 0–16 bar, bottom outlet with isolating valve
	Piece
	1
	 
	 
	 
	 

	4.3.5
	150 cm × 150 cm C25 manhole constructed of precast or cast-in-situ reinforced concrete
	Piece
	1
	 
	 
	 
	 

	4.4.1
	DN50 Air Release Valve complete with isolation gate valve PN16
	Piece
	1
	 
	 
	 
	 

	4.4.2
	150 cm × 100 cm C25 manhole constructed of precast or cast-in-situ reinforced concrete T10 @20 double layer  
	Piece
	1
	 
	 
	 
	 

	5
	Testing and commissioning of potable water pipes
	
	
	 
	 
	 
	 

	5.1.1
	Testing and commissioning of  63 mm OD Pipes
	Lm
	220
	 
	 
	 
	 

	 
	Total for Lot 1 Excluding VAT
	 
	_____________ USD

	 
	V.A.T 11%
	 
	 

	 
	Total for Lot 1 including VAT
	 
	_____________ USD

	 
	Lead time of Delivery and Implementation 
	 
	 













LOT 2:  Al Jame3 Line
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1
	General 
	 
	 
	 
	 
	 
	 

	The Contractor shall carry out all general works required for the successful execution of the project, including mobilization and demobilization, site inspections, topographic survey and setting out, preparation and submission of shop drawings and as-built drawings, coordination with relevant stakeholders, obtaining necessary approvals and permits, and provision of all labor, equipment, materials, transportation, supervision, health and safety measures, and temporary works required for the completion of the contract. All works shall be carried out in accordance with the specifications, drawings, and Engineer's instructions.

	1.1
	Topographic Survey and Setting Out Works
	Ls
	1
	 
	 
	 
	 

	1.2
	Preparation and Submission of Shop Drawings and As-Built Drawings
	Ls
	1
	 
	 
	 
	 

	2
	Pipeworks
	 
	 
	 
	 
	 
	 

	2.1
	Pipes 
	Lm
	1000
	 
	 
	 
	 

	2.2
	Asphalt Cutting 
	Lm
	1000
	 
	 
	 
	 

	2.3
	Trench Excavation 
	Lm
	1000
	 
	 
	 
	 

	2.4
	Sand bedding and surrounds
	Lm
	1000
	 
	 
	 
	 

	2.5
	Laying of HDPE Pipe 
	Lm
	1000
	 
	 
	 
	 

	2.6
	Backfilling of Trenches Including Compaction and Testing
	Lm
	1000
	 
	 
	 
	 

	3
	Road Reinstatement 
	 
	 
	 
	 
	 
	 

	3.1
	Supply and placement of  asphalt to reinstate the road surface over trench areas, 10 cm thickness. Works include surface preparation, priming, laying of base and wearing courses, mechanical compaction, and finishing to restore road conditions to original or as specified by the local authority.
	m2
	400
	 
	 
	 
	 

	4
	Valves and Piping Works 
	 
	 
	 
	 
	 
	 

	4.1
	Connection of a 63 mm OD HDPE pipeline to an existing 2 inch HDPE pipeline, including all necessary saddles, fittings, adaptors, excavation, tie-in works, testing, and reinstatement, complete in all respects.
	Piece
	1
	 
	 
	 
	 

	4.2
	SB-01 & SB02 - Supply and installation of a 2-inch gate valve complete with a round ductile iron surface box, including connection to a 63 mm OD HDPE pipe. The works shall include all necessary fittings, supports, sealing gaskets, chamber adjustments, alignment, anchoring, pressure testing, and reinstatement of disturbed areas.
	Piece
	2
	 
	 
	 
	 

	4.3.1
	2-inch bronze gate valve, PN16 with wash-out extension pipe inside Manhole
	Piece
	4
	 
	 
	 
	 

	4.3.2
	Pressure gauge Ø 100  PN 16 with glycerine, bottom outlet with isolating valve
	Piece
	1
	 
	 
	 
	 

	4.3.3
	150 cm × 150 cm C25 manhole constructed of precast or cast-in-situ reinforced concrete
	Piece
	1
	 
	 
	 
	 

	4.4.1
	2-inch bronze gate valve, PN16 with wash-out extension pipe inside Manhole
	Piece
	1
	 
	 
	 
	 

	4.4.2
	150 cm × 100 cm C25 manhole constructed of precast or cast-in-situ reinforced concrete T10 @20 double layer  
	Piece
	1
	 
	 
	 
	 

	5
	Testing and commissioning of potable water pipes
	 
	 
	 
	 
	 
	 

	5.1.1
	Testing and commissioning of  63 mm OD Pipes
	Lm
	1000
	 
	 
	 
	 

	 
	Total for Lot 2 Excluding VAT
	 
	_____________ USD

	 
	V.A.T 11%
	 
	 

	 
	Total for Lot 2 including VAT
	 
	_____________ USD

	 
	Lead time of Delivery and Implementation 
	 
	 




LOT 3:  Al Fekha, Saydeh Line
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1
	General 
	 
	 
	 
	 
	 
	 

	The Contractor shall carry out all general works required for the successful execution of the project, including mobilization and demobilization, site inspections, topographic survey and setting out, preparation and submission of shop drawings and as-built drawings, coordination with relevant stakeholders, obtaining necessary approvals and permits, and provision of all labor, equipment, materials, transportation, supervision, health and safety measures, and temporary works required for the completion of the contract. All works shall be carried out in accordance with the specifications, drawings, and Engineer's instructions.

	1.1
	Topographic Survey and Setting Out Works
	Ls
	1
	 
	 
	 
	 

	1.2
	Preparation and Submission of Shop Drawings and As-Built Drawings
	Ls
	1
	 
	 
	 
	 

	2
	Pipeworks
	 
	 
	 
	 
	 
	 

	2.1
	Pipes 
	Lm
	900
	 
	 
	 
	 

	2.2
	Asphalt Cutting 
	Lm
	900
	 
	 
	 
	 

	2.3
	Trench Excavation 
	Lm
	900
	 
	 
	 
	 

	2.4
	Sand bedding and surrounds
	Lm
	900
	 
	 
	 
	 

	2.5
	Laying of HDPE Pipe 
	Lm
	900
	 
	 
	 
	 

	2.6
	Backfilling of Trenches Including Compaction and Testing
	Lm
	900
	 
	 
	 
	 

	3
	Road Reinstatement 
	 
	 
	 
	 
	 
	 

	3.1
	Supply and placement of  asphalt to reinstate the road surface over trench areas, 10 cm thickness. Works include surface preparation, priming, laying of base and wearing courses, mechanical compaction, and finishing to restore road conditions to original or as specified by the local authority.
	m2
	360
	 
	 
	 
	 

	4
	Valves and Piping Works 
	 
	 
	 
	 
	 
	 

	4.1
	Connection of a 63 mm OD HDPE pipeline to an existing 4 inch HDPE   pipeline, including all necessary saddles, fittings, adaptors, excavation, tie-in works, testing, and reinstatement, complete in all respects.
	Piece
	1
	
	
	
	

	4.2
	2-inch bronze gate valve, PN16 for isolation
	Piece
	2
	 
	 
	 
	 

	4.3
	Pressure gauge Ø 100  PN 16 with glycerine, bottom outlet with isolating valve
	Piece
	1
	 
	 
	 
	 

	4.3.1
	150 cm × 150 cm C25 manhole constructed of precast or cast-in-situ reinforced concrete
	Piece
	1
	 
	 
	 
	 

	4.3.2
	SB-01 - Supply and installation of a 2-inch gate valve complete with a round ductile iron surface box, including connection to a 63 mm OD HDPE pipe. The works shall include all necessary fittings, supports, sealing gaskets, chamber adjustments, alignment, anchoring, pressure testing, and reinstatement of disturbed areas.
	Piece
	1
	 
	 
	 
	 

	4.4.1
	2-inch bronze gate valve, PN16 with wash-out extension pipe inside Manhole
	Piece
	1
	 
	 
	 
	 

	4.4.2
	150 cm × 100 cm C25 manhole constructed of precast or cast-in-situ reinforced concrete T10 @20 double layer  
	Piece
	1
	 
	 
	 
	 

	5
	Testing and commissioning of potable water pipes
	 
	 
	 
	 
	 
	 

	5.1.1
	Testing and commissioning of  63 mm OD Pipes
	Lm
	900
	 
	 
	 
	 

	 
	Total for Lot 1 Excluding VAT
	 
	_____________ USD

	 
	V.A.T 11%
	 
	 

	 
	Total for Lot 1 including VAT
	 
	_____________ USD

	 
	Lead time of Delivery and Implementation 
	 
	 






ANNEX 3: DETAILED SPECIFICATIONS 

As per: 2026-069 Terms of Reference -Al Ain & Fakeha Water Supply Tender 


Supplier: Sign & Stamp ____________________________                                                                                                                                                               Page 1 of 19
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