National tender application pack V0.3Lebanese Red Cross 

Tender reference: 2026-082
[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered.
· The contract will be awarded to the lowest-cost technically compliant complete lot or complete bid. 
· The quantities mentioned below are required unless there is a variation within a specified range with proper justification. The LRC reserves the right to increase or decrease the quantities.
· The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.  
· In the event of any discrepancy between the unit price and the total price, LRC reserves the right to rely on the unit price as stated in the financial bid, rather than the total price without go back to the supplier. The unit price must be provided with no more than two decimal places.
· Only one option is allowed for biding 
· The bidder shall price each of the three distribution-line schedules separately. All unit rates shall include labor, materials, equipment, transport, testing, permits, overheads, incidental works, and all obligations necessary for the complete execution and handover of the works.
LOT 1:  Zahle PHC
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	[bookmark: RANGE!A3:D63]Division 1
	 
	 
	 
	 

	1
	Preliminaries & General Requirements
	 
	 
	 
	 

	1.1
	Mobilization & Demobilization
	LS
	1
	 
	 
	 
	 

	1.2
	Site Establishment 
	LS
	1
	 
	 
	 
	 

	1.3
	Temporary Utilities
	LS
	1
	 
	 
	 
	 

	1.4
	Temporary Fencing & Signage
	LS
	1
	 
	 
	 
	 

	1.5
	Traffic Management and Safety Barriers
	LS
	1
	 
	 
	 
	 

	1.6
	Insurance Accident and liability
	LS
	1
	 
	 
	 
	 

	1.7
	Health & Safety Measures
	LS
	1
	 
	 
	 
	 

	1.8
	Site Cleaning & Waste Management
	LS
	1
	 
	 
	 
	 

	1.9
	Dismantling of existing elements and return to initial condition
	LS
	1
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 2
	 
	 
	 
	 

	2
	Constructions
	 
	 
	 
	 

	2.1
	Partitions 
	m²
	70
	 
	 
	 
	 

	2.2
	False Ceilings
	m²
	181
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 3 
	 
	 
	 
	 

	3
	Finishing
	 
	 
	 
	 

	3.1
	Painting for existing walls
	m²
	450
	 
	 
	 
	 

	 
	Painting for Gypsum new walls
	m²
	250
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 4 
	 
	 
	 
	 

	4
	Sanitary
	 
	 
	 
	 

	4.1
	Sanitary fixtures
	No.
	8
	 
	 
	 
	 

	4.2
	Vanity top  (Kitchen)
	No.
	1
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 5
	 
	 
	 
	 

	5
	Aluminum Works
	 
	 
	 
	 

	5.1
	Aluminum Doors
	No.
	11
	 
	 
	 
	 

	5.3
	Aluminum Partitions
	m²
	15
	 
	 
	 
	 

	5.4
	Aluminum Windows
	m²
	19
	 
	 
	 
	 

	5.5
	Repair and reuse existing aluminum
	m²
	24
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 6
	 
	 
	 
	 

	6
	Flooring
	 
	 
	 
	 

	5.1
	Floor Polishing
	m²
	300
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 7
	 
	 
	 
	 

	7
	HVAC Works
	 
	 
	 
	 

	7.1
	Split AC Units, 9000 BTU
	No.
	7
	 
	 
	 
	 

	7.2
	Split AC Units, 18000 BTU
	No.
	1
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 8
	 
	 
	 
	 

	8
	Furniture
	 
	 
	 
	 

	8.1
	Benche
	No.
	3
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 9
	 
	 
	 
	 

	9
	Dental Clinic
	 
	 
	 
	 

	9.1
	Wooden raised Platform
	m²
	24
	 
	 
	 
	 

	9.2
	Specialized works 
	LS
	1
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 10
	 
	 
	 
	 

	10
	Electrical Works
	 
	 
	 
	 

	10.1
	Lighting Points (60*60)
	LS
	1
	 
	 
	 
	 

	10.2
	CCTV System
	LS
	1
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD

	Division 11
	 
	 
	 
	

	11
	Wooden Elements
	 
	 
	 
	 

	11.1
	Existing wooden windows
	U
	18
	 
	 
	 
	 

	Division Total
	 
	 
	 
	_________________ USD






	Divisions
	Items by Trade
	Total
Exc (VAT)
	Total
(Inc VAT)

	Division 1
	Preliminaries & General Requirements
	
	

	Division 2
	Constructions
	
	

	Division 3
	Finishing
	
	

	Division 4
	Sanitary
	
	

	Division 5
	Aluminum Works
	
	

	Division 6
	Flooring
	
	

	Division 7
	HVAC Works
	
	

	Division 8
	Furniture
	
	

	Division 9
	Dental Clinic
	
	

	Division 10
	Electrical Works
	
	

	Division 11
	Wooden Elements
	
	

	Grand Total                           












ANNEX 3: DETAILED SPECIFICATIONS 

As per: 2026-082 Terms of Reference

 
	Item No
	Items by trade 
	Description of works
	Unit
	Qty

	Division 1

	1
	Preliminaries & General Requirements

	1.1
	Mobilization & Demobilization
	Contractor's mobilization/demobilization:  removal of personnel, equipment, tools, and temporary facilities upon completion of works
	LS
	1

	1.2
	Site Establishment 
	Contractor’s site setup, including necessary working areas, storage areas, site camp facilities (if required), and general site arrangements.
	LS
	1

	1.3
	Temporary Utilities
	Provision, connection, maintenance, and removal of temporary water, electricity, lighting, communication, and other utilities required for the execution of works.
	LS
	1

	1.4
	Temporary Fencing & Signage
	Provision and maintenance of temporary fencing, warning signs, safety notices, and protection measures for the work area.
	LS
	1

	1.5
	Traffic Management and Safety Barriers
	Provision and maintenance of traffic control measures, barriers, access control, and safe circulation arrangements where required.
	LS
	1

	1.6
	Insurance Accident and liability
	Provision of all required insurance coverage, including workers’ compensation, contractor’s liability, and third-party liability insurance.
	LS
	1

	1.7
	Health & Safety Measures
	Provision and implementation of all necessary occupational health and safety measures throughout the execution of the works, including scaffolding, traffic management measures, safety barriers and warning signs, personal protective equipment (PPE) for all workers, safe access and working platforms, provision of drinking water, and all other safety and welfare requirements necessary to comply with applicable safety regulations and Engineer’s instructions.
	LS
	1

	1.8
	Site Cleaning & Waste Management
	Continuous cleaning of the work areas, collection, transportation, and disposal of construction waste and debris to approved disposal locations.
	LS
	1

	1.9
	Dismantling of existing elements and return to initial condition
	Removal of temporary facilities, fencing, utilities, and protection measures, including cleaning and reinstatement of affected areas upon completion.

	LS
	1

	Division 2

	2
	Constructions

	2.1
	Partitions 
	Supply, delivery, assembly, and precise installation of a 10 cm thick heavy-duty moisture-resistant gypsum board partition wall. 
2. Material Specifications:
Gypsum Board Enclosure: Moisture-Resistant (MR) / Waterproof-grade gypsum plasterboards. Double-layer application on both faces of the partition wall using 12.5 mm thick MR boards (yielding a total skin thickness of 25 mm per side to achieve the required structural durability and a total wall profile of ~10 cm).
Metal Framing System:
Hot-dip galvanized steel studs and floor/ceiling tracks (runners), sized to match the overall 10 cm partition depth. Heavy-duty structural metal framework installed with vertical studs and horizontal bridging channels positioned at maximum 40 cm centers (on-center spacing) both horizontally and vertically to form a reinforced grid.
3. Accessories & Fasteners: Corrosion-resistant, self-tapping drywall screws spaced at required centers per manufacturer guidelines for double-layer installation.Heavy-duty mechanical masonry anchors/plugs to securely fasten tracks to floor slabs, soffits, and adjacent perimeter walls. Fiberglass mesh joint tape embedded in specialized waterproof joint compound, finished flush and sanded smooth for immediate priming/painting or tiling.Perimeter Sealing: Acoustic and moisture-resistant elastomeric sealant applied along floor, ceiling, and perimeter wall tracks to prevent moisture ingress and sound transmission.
4. Execution & Quality Control: Partition walls must be installed strictly squared and leveled,  Floor and ceiling tracks must be securely aligned prior to board installation.
	m²
	70

	2.2
	False Ceilings
	Supply and install plastic suspended false ceiling 60x60 including supporting grid system, hangers, trims, and all necessary accessories, complete in all respects, where all metallic framing is in galvanized steel
	m²
	181

	Division 3 

	3
	Finishing

	3.1
	Painting for existing walls
	Supply and apply acrilyc based paint to all existing walls, with half high rubber paint skirting, including:
Light sanding where required to ensure proper adhesion.
Local application of wall putty only where necessary to repair surface imperfections, cracks, holes, or uneven areas, including sanding to achieve a smooth finish.
Application of additional finishing layers of high-quality anti-graffiti oil-based paint, minimum 3 coats or as required by the Engineer, in white or approved neutral color, ensuring uniform coverage. (First coat as undercoat)
Protection of floors and adjacent surfaces by covering the complete area with protective sheets prior to painting works.
Including all required materials, tools, equipment, and skilled manpower to complete the works to the Engineer’s satisfaction.
	m²
	450

	 
	Painting for Gypsum new walls
	Supply and apply acrilyc based paint to all new walls, with half high rubber paint skirting, including:
Light sanding where required to ensure proper adhesion.
Local application of wall putty only where necessary to repair surface imperfections or uneven areas, including sanding to achieve a smooth finish.

Application of additional finishing layers of high-quality anti-graffiti oil-based paint, minimum 3 coats or as required by the Engineer, in white or approved neutral color, ensuring uniform coverage. (First coat as undercoat)
Protection of floors and adjacent surfaces by covering the complete area with protective sheets prior to painting works.
Including all required materials, tools, equipment, and skilled manpower to complete the works to the Engineer’s satisfaction.
	m²
	250

	Division 4 

	4
	Sanitary

	4.1
	Sanitary fixtures
	Supply and installation of a wall mounted porcelain washbasins oval/rectangular shape (50 cm) (made in Europe) of suitable height to be determined on site (European manufacturer) including:
[b] water connection (PPR, concealed) & sewer connection (PVC, concealed)
[c] cast iron anti-corrosion painted brackets
[d] all necessary materials, accessories , requirements and manpower to make it properly serviceable
mixers, siphons, valves, connections to water supply and drainage networks, and all necessary accessories, complete in all respects.
Supply and installation of a wall mounted porcelain washbasins oval/rectangular shape (50 cm) (made in Europe) of suitable height to be determined on site (European manufacturer) including:
[a] stainless steel P-trap high quality


	No.
	8

	4.2
	Vanity top  (Kitchen)
	Supply and Install countertop & bassin for kitchen including
in premium natural granite slab (3cm thickness), polished with honed edges (standard), with cutout for sink as described below.
Edge Profile: 4cm half bullnose
Color: Client's selection from approved samples
Treatment: Stain-resistant sealant application (2 coats)
-Stainless steel, undermount, single-bowl bassin (50×45cm, 18-gauge, satin finish)
Mixer tap with a Single-lever pull-down sprayer and Ceramic cartridge (drip-free)
with all accessories including but may not be limited to :
Sink strainer with overflow protection
Angle valves (chrome-plated brass). 
Color and design as approved by engineer
	No.
	1

	Division 5

	5
	Aluminum Works

	5.1
	Aluminum Doors
	Supply and install aluminum SIDEM 2000 profile doors (w 90cm, h200cm) with 6mm thick single glass panels, including frames, hinges, locks, handles, sealing, and all necessary accessories, complete as per approved shop drawings, with a matching sliding insect screen with a multi-rail sliding system engineered for smooth, silent, and low-friction track operation. 
	No.
	11

	5.3
	Aluminum Partitions
	Supply and install aluminum SIDEM 2000 profile partition of 3m height, consisting of 1.50 m aluminum sheet at bottom and 1.50 m 6mm glass above, including framing system, fixing, sealing, and all necessary accessories, complete in all respects.
	m²
	15

	5.4
	Aluminum Windows
	Supply and install aluminum SIDEM 2000 profile windows (1m x 2m) with 6mm thick double glass panels, including frames, hinges, locks, handles, sealing, and all necessary accessories, complete as per approved shop drawings, with a matching sliding insect screen with a multi-rail sliding system engineered for smooth, silent, and low-friction track operation.
	m²
	19

	5.5
	Repair and reuse existing aluminum
	Dismantling, repairing and relocating 2 existing aluminum partitions; including all accecerries if needed (new location as per drawing)
	m²
	24

	Division 6

	6
	Flooring

	5.1
	Floor Polishing
	Clean and Rub the Existing Floor Tiles and Skirting Rehabilitate any type of flooring tiles and skirting (marbels, mosaic, etc...) works includes all materisals and labors and the following steps:     
- Preparing and saftty
- Cleaning and structural repairing
- Grinding and leveling
- Progressive honing
- High Gloss Polishing
- Penetration sealing.
A trial mockup (one by type of floor tiles) will be performed by the contractor prior to proceed with the complete item. Proposed location and results should be pproved by the client. 
	m²
	300

	Division 7

	7
	HVAC Works

	7.1
	Split AC Units, 9000 BTU
	Supply & Installation of 9,000 BTU Inverter Split AC Units
220V, 50Hz, non-flammable refrigerant (R32/R290)
Includes 3m copper piping (Ø6.35mm + Ø9.52mm) with insulation
Complete installation with electrical wiring, drainage, and mounting System. Including testing & commissioning (vacuum and pressure testing
refrigerant charging and performance verification
	No.
	7

	7.2
	Split AC Units, 18000 BTU
	Supply & Installation of 18,000 BTU Inverter Split AC Units
220V, 50Hz, non-flammable refrigerant (R32/R290)
Includes 3m copper piping (Ø6.35mm + Ø12.70mm) with insulation
Complete installation with electrical wiring, drainage, and mounting System. Including testing & commissioning (vacuum and pressure testing
refrigerant charging and performance verification
	No.
	1

	Division 8

	8
	Furniture

	8.1
	Benche
	Supply and install waiting room benches in upholsted galvanized steel, complete with all necessary accessories and fixing.
	No.
	3

	Division 9

	9
	Dental Clinic

	9.1
	Wooden raised Platform
	Supply and install removable wooden raised floor system in dental clinic areas, including supporting structure, panels, finishing, openings where required, and all necessary accessories, complete in all respects. The system shall allow future accessibility and flexibility for installation, maintenance, and modification of dental clinic infrastructure and equipment.
	m²
	24

	9.2
	Specialized works 
	Preparation and execution of all required infrastructure for dental clinic, including but not limited to drainage, water supply, electrical outlets, medical equipment connections, and all related works, complete in all respects (as per attached drawings and requirements).
	LS
	1

	Division 10

	10
	Electrical Works

	10.1
	Lighting Points (60*60)
	Supply and install all internal electrical works including LED lighting fixtures 30 (60cm*60cm), switches 20, sockets 50, wiring, Data 11,conduits,Cabinet 1 ,Electrical panel 2,cicuit breaker 24,distribution, and all necessary accessories, complete as per specifications and drawings.
	LS
	1

	10.2
	CCTV System
	Supply and install indoor and outdoor CCTV system 10 cameras, cabling, recording unit, accessories, and all necessary components for proper operation, complete with testing and commissioning.
	LS
	1

	Division 11

	11
	Wooden Elements

	11.1
	Existing wooden windows
	Repair and rehabilitation of 18 existing external wooden windows and doors, including sanding, fixing, replacement of damaged parts if needed, and finishing, complete in all respects.
	U
	18



Supplier: Sign & Stamp ____________________________                                                                                                                                                               Page 1 of 19
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