[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered. 
· The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.  
· In the event of any discrepancy between the unit price and the total price, LRC reserves the right to rely on the unit price as stated in the financial bid, rather than the total price without go back to the supplier. The unit price must be provided with no more than two decimal places.
· The quoted unit and/or lump-sum prices shall include all costs for the supply and complete execution of the works, including materials, labor, transportation, delivery to the LRC-designated site, installation, equipment, tools, fittings, accessories, testing, and all applicable bank transfer charges.
	LRC To Complete
	Bidder to Complete 
	

	Item # 
	Item/Milestone Required
	 UOM
	QTY
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Total Price in USD
Inclusive of VAT
	Lead Time for Delivery

	1
	Rehabilitation of the DRR Hazmieh  as detailed in the TOR and as be the BOQ
	LS
	1
	
	
	
	



	LRC To Complete
	Bidder to Complete 

	Item # 
	Item/Milestone Required as per the Specification mentioned in the BOQ
	 UOM
	QTY
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Total Price in USD
Inclusive of VAT

	1
	Site preparation and demolition
	LS
	1
	
	
	

	2
	Reinforced Concrete Jacketing
	LS
	1
	
	
	

	3. Hollow or Solid Concrete Blocks and Clostra construction
Supply and install hollow or solid concrete blocks as per drawings
Work to include all places as per the drawings, location and the Engineer instructions, Materials, Cement mortar and the use of extruded nets and reinforcement by means of metal gates and the placement of angles of galvanized. steel iron of concrete columns thickness of 4 mm every 60 cm, Labors and all items needed and instructions by the Engineer

	3.1.1
	10 cm hollow concrete blocks
	M2
	20
	
	
	

	3.1.2
	12 cm hollow concrete blocks
	M2
	20
	
	
	

	3.1.3
	15 cm hollow concrete blocks
	M2
	15
	
	
	

	3.2
	Repair of Existing Plaster Internal & External (Cracks)
	LS
	1
	
	
	

	4. Woodwork

	4.1
	Timber Kitchen Cupboards – Under-Counter and Upper Cabinets
	LM
	12
	
	
	

	4.2
	Wooden Works, Doors, Frames and Carpentry:
General Requirement: Supply and install all timber work with all related items, The joinery works should be of the first-class type and as per specifications and drawings, Work to include Material and labors, all accessories to be heavy duty (Hinged, Lock, Glass vision, as required…etc), The frame for any width (Steel, Wood…)	, Paint as follows: Anti-rust layers, Putty + one layer of undercoat, three layers of epoxy paint, remove the existing timber panels, repair the edges
The Contractor should submit shop drawings and all needed items as the Engineer instructions

	4.2.1
	New internal timber Doors 
	U
	12
	
	
	

	4.2.2
	Rehabilitate the Existing Timber Doors:
	U
	12
	
	
	

	5. Aluminum Doors and Windows
Fabricate, supply and install aluminum works as manufactured by SIDEM 2000 first choice with all necessary accessories as per the drawings and the Engineer instructions, cost to include all doors and windows: Single glass 6 mm clear on both sides, Double glass 6-12-6 mm clear on both sides, and outer Glass should be Tempered), Section width 12.5 cm and thickness 2 mm, Hinges and locks, Joint Filler, Mosquito Screen, Mesh
All items needed as per the Engineer instructions, All as specified and base on an approved shop drawings after exact dimensions

	5.1
	New External Aluminum windows (Double Glass)
	M2
	150
	
	
	

	5.2
	New Aluminum Internal Door
	M2
	3
	
	
	

	6. Tiles

	6.1
	Install New Tiles
	M2
	300
	
	
	

	6.2
	Threshold marbles tiles (Doors, Topping, Toilets)
	LM
	10
	
	
	

	6.3
	New external Natural Stone Plinth
	LM
	200
	
	
	

	6.4
	Clean and Rub the Existing Floor Tiles and Skirting
	M2
	200
	
	
	

	7
	Ceiling Works
	M2
	40
	
	
	

	8. Paint Work

	8.1
	Paint Works for Wall and Ceilings 
	M2
	450
	
	
	

	8.2
	Outside Walls Paint (Old and New Walls and Ceilings)
	M2
	150
	
	
	

	8.3
	Paint Water Repellant Colorless Layer Unleaded on Facades and Supply a Guarantee for Five Years
	M2
	150
	
	
	

	9. Bathrooms Accessories: Supply and install all needed accessories and make good their places and their surroundings, Place all frame, cover joints (stainless steel) anti-corrosion, Install items and their contact with the surfaces, All works should be done as per the Engineer instructions, All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval

	9.1
	Paper Roller Holder
	U
	6
	
	
	

	9.2
	Soap Dispenser
	U
	6
	
	
	

	9.3
	Paper Holder Box
	U
	6
	
	
	

	9.4
	Mirror for Lavatories
	U
	6
	
	
	

	9.5 PIPED SYSTEMS (LIQUIDS)
Cold & Hot Water Piping Inside Building
Supply, install and test water supply system inside the building.
Pipes should be (PPR) and the price is per linear meter. Cost to include all accessories, connections, reducers, all valves as shown on the drawings, Ø20mm PRV for make-up system where applicable, water hammer arrestor hanging and embedded system, so that all piping can receive ideal standard fixtures
The Contractor should submit shop drawings for approval by the Engineer. Works should be as standard installation details

	9.5.1
	Ø 20 mm
	LM
	35
	
	
	

	9.5.2
	Ø 25 mm
	LM
	35
	
	
	

	9.5.3
	Ø 32 mm
	LM
	50
	
	
	

	9.6
	Water Tanks 2000 Litres
	U
	2
	
	
	

	9.7
	Steel tower for Water Tank
	U
	2
	
	
	

	9.8
	Western Toilets seats 
	U
	6
	
	
	

	9.9
	Semi Pedestal Wash Basin
	U
	6
	
	
	

	9.10
	Self-Close tap for wash basins
	U
	6
	
	
	

	9.11
	Kitchen Sink Accessories
	U
	3
	
	
	

	9.12
	Taps for Kitchen Sinks
	U
	2
	
	
	

	10. Drainage System inside the Building
Supply, install and test the wastewater drainage from (UPVC) pipes inside the building to outside and the pipes measured in Linear Meter with all related accessories, cleanout, elbows, vent hangers, brackets and all necessary accessories as per standard installation details
The diameter of the pipes are as follows:

	10.1.1
	Ø 110 mm / UPVC
	LM
	40
	
	
	

	10.1.2
	Ø 200 mm / UPVC
	LM
	40
	
	
	

	10.2 Floor Drain: Supply and install floor drain P.V.C. with chrome-plated brass drain cover and to be the same level as the floor and do all necessary installation and connections. This includes all civil works and connection to the proper floor pipes and as per the Engineer instructions

	10.2.1
	FD-01: Ø75 mm bottom outlet
	U
	25
	
	
	

	10.3
	Water Heating Solar Panels
	U
	2
	
	
	

	11
	Booster Pumps
	U
	2
	
	
	

	12. Basic Electrical Requirements
The Contractor should revise all the drawings and compare them with the actual site conditions and redo all the design works with the necessary calculations for all the electrical installations and works. Moreover, the Contractor should submit all needed shop drawings, subject to the client approval.
At the end of the project, the contractor should submit complete As-Built Drawings, operational and maintenance manuals for all executed works with exact dimensions & sizes for easy maintenance work in the future. All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval

	12.1
	Removal of existing electrical network
	LS
	1
	
	
	

	12.2
	Electrical Distribution Panel boards
	U
	2
	
	
	

	12.3
	Electrical Distribution Panel boards for UPS
	U
	2
	
	
	

	13.1
	Disconnecting Switches
	U
	60
	
	
	

	13.2 Electrical Sockets: Supply, install and test single socket outlet, 250 Volt, 16 Amp, special children type, with all the necessary protection. The cost includes conduits, cables, wires, and all accessories as per the drawings, specifications and Engineer instructions. All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval

	13.2.1
	16A 250V 3 pin wall mounted socket outlet

	U
	70
	
	
	

	13.2.2
	16A 250V 3pin wall mounted socket outlet UPS
	U
	70
	
	
	

	12.2.3
	RJ45 CAT6  data outlets with 5x4pairs CAT6  cables to corresponding patch panel
	U
	70
	
	
	

	13.2.4
	RJ45 CAT6  camera outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	16
	
	
	

	13.2.5
	RJ45 CAT6  access point outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	10
	
	
	

	13.2.6
	RJ45 CAT6  access control outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	2
	
	
	

	14
	Lighting Fixtures: Supply, install and test the lighting fixtures complete with all the necessary wires conduits, boxes and accessories required to provide power to each lighting fitting from LP including the earth wire as per the drawings, specifications and Engineer instructions.
The Contractor should submit samples of each lighting fixture for approval.

	14.1.1
	Led Panel Light 60X60 60W 110/220V Day light; surface mounted type.
	U
	30
	
	
	

	14.1.2
	Ceiling mounted lighting fixture, Spot Led, diameter 20 cm
	U
	16
	
	
	

	14.1.3
	Led Wall-mounted globe/hublot luminaire 20 W
	U
	5
	
	
	

	14.2
	HDMI wall outlet/link. Complete with wall plates, back boxes, conduit and accessories, and cable 15 m run.
The minimal requirement for the HDMI: version 2.1 compatible, supported resolution/refresh rate up to 8K at 60 Hrz, HDCP compatibility 2.2 to 2.3, cable’s construction hybrid optical fiber plus coper conductor.
	U
	5
	
	
	

	14.3
	Electrical outlet for electrical Powered door
	U
	2
	
	
	

	14.4
	Outlet for ventilation/exhaust fan.
	U
	6
	
	
	

	14.5
	Empty provisional outlet point
	U
	20
	
	
	

	15. Video surveillance CCTV & Network video recorder (NVR)

	15.1
	Video surveillance CCTV
	U
	16
	
	
	

	15.2
	Network video recorder (NVR)
	U
	1
	
	
	

	16
	Chipboard Panels
	M2
	950
	
	
	

	Total Amount TTC:
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ANNEX 3: DETAILED SPECIFICATIONS / TERMS OF REFERENCE AND BOQ

Subject: Rehabilitation and Upgrade Works at Beirut Hazmieh Station for DRR
The Lebanese Red Cross is seeking expressions of interest from qualified and experienced contractors for the implementation of rehabilitation, renovation, and upgrade works at a new office in Hazmieh in Beirut.

A. [bookmark: _Toc238047604]Project Overview
[bookmark: _Toc238047605]As part of the Lebanese Red Cross (LRC) commitment to improving the operational capacity, safety, resilience, and functionality of its facilities, the organization intends to undertake rehabilitation and upgrading works at the Beirut Hazmieh Station for Disaster Risk Reduction (DRR).
The project aims to renovate and upgrade the existing facility through a series of architectural, civil, mechanical, electrical, and plumbing works to improve working conditions, enhance the station’s operational capacity, strengthen preparedness and response capabilities, and ensure compliance with the operational requirements of the DRR 
B. Main Scope of Works
The project shall include, but shall not be limited to, the following activities:
The Contractor shall provide all labor, materials, equipment, tools, transportation, supervision, testing, and all other resources necessary for the complete execution of the rehabilitation and upgrade works at the Beirut Hazmieh Station for Disaster Risk Reduction (DRR).
1.  Demolition and Removal Works
· Demolition and removal of selected existing walls, partitions, floor and wall finishes, sanitary fixtures, doors, windows, and any other elements indicated in the drawings or instructed by the Engineer.
· Removal, transportation, and disposal of debris and waste materials to authorized dumping sites in accordance with local regulations.
· Protection of existing structures and services that are to remain operational during the execution of the works.
2.  Architectural and Finishing Works
· Supply and installation of new ceramic floor and wall tiles in kitchens and sanitary facilities.
· Construction of new partitions
· Surface preparation, repairs, finishing, and painting works where required.
· Making good all disturbed surfaces following completion of the works.
· Demolition and Reconstruction of Lintels
3. B. Doors, Windows, and Joinery Works
· Supply and installation of new aluminum windows complete with accessories and hardware.
· Supply and installation of aluminum doors and partitions where specified.
· Supply and installation of internal wooden doors, including frames where needed, ironmongery, and accessories.
· Supply and installation of wood kitchen top and cabinets and associated accessories.
4. C. Plumbing and Sanitary Works
· Supply and installation of new sanitary fittings and fixtures for all WC facilities.
· Modification, replacement, and connection of water supply and drainage networks as required.
· Supply and installation of a water storage tank complete with all necessary pipework, valves, fittings, and accessories.
· Testing and commissioning of all plumbing and sanitary systems.
5. D. Electrical Works
· Removal of obsolete electrical installations where required.
· Supply and installation of new electrical wiring and distribution systems.
· Supply and installation of electrical control and distribution panels.
· Supply and installation of lighting fixtures, switches, sockets, and related accessories.
· Testing, commissioning, and certification of all electrical installations.
6. E. Waterproofing and External Works
· Cleaning, treatment, repair, and waterproofing of external walls.
· Sealing of cracks, joints, and other areas susceptible to water infiltration.
· Execution of all associated ancillary works required to ensure a complete and durable waterproofing system.
7. F. Testing, Commissioning, and Handover
· Testing and commissioning of all installed architectural, mechanical, electrical, plumbing, and sanitary systems.
· Rectification of deficiencies identified during inspections.
· Final cleaning of the premises and handover of the facility in complete operational condition.
The scope described above is indicative and not exhaustive. The Contractor shall execute all works necessary for the proper completion and functionality of the the Beirut Hazmieh Station for Disaster Risk Reduction (DRR).
in accordance with the contract documents, technical specifications, drawings, and the Engineer's instructions.
The Contractor shall supply and install all materials, equipment, fixtures, fittings, and systems necessary for the complete execution of the rehabilitation works. All materials shall be new, of first quality, and compliant with the project specifications and approved standards.
C. [bookmark: _Toc238047606]Project Location
The project is located at: Hazmieh, Mont Lebanon, Lebanon.
D. [bookmark: _Toc238047607]Project Duration
The Contractor shall complete, test, commission, and hand over all awarded works no later than 15 December 2026.
The Contractor’s program shall account for material procurement, mobilization, surveys, approvals, permits, site access, construction works, testing, documentation, and handover.
E. [bookmark: _Toc238047608]Mandatory Site Visit
A mandatory site visit and briefing will be conducted.
Bidders who fail to attend the mandatory site visit shall be disqualified from the tender process.
The date, time, meeting point, and arrangements for the site visit as mentioned in the Invitation to Bid.
F. [bookmark: _Toc238047609]Submission Requirements
Interested contractors shall submit a complete Technical and Financial Offer containing all the documents listed below.
1. [bookmark: _Toc238047610]Priced Annex 2 Financial bid Form in accordance to the Bill of Quantities (BOQ)
The bidder shall submit a priced Annex 2 – Financial form that is fully completed, Signed and stamped covering all the requirement mentioned in the BOQ Below: 
	Item
	Description
	
	UoM
	Qty

	1
	SITE PREPARATION AND DEMOLITION
Demolishing and Removal of Debris
The works include all types of demolition and the removal of debris such but not limited to:
Existing plastering and concrete items such as foundations, columns, slabs, …etc
Tiling (floors and walls)
Toilet fixtures and pipes installation of all sizes
Counter tops, bases and sinks
Water tanks of different types
Hollow concrete block walls or concrete walls of all sizes
Proper cutting equipment to be used in opening of doors.plans and specifications Including the necessary equipment for the removal debris etc…
	هدم وتجهيز الموقع:
تكسير وإزالة أنقاض يشمل كل أنواع التكسير في الموقع ونقل الأنقاض الناتجة إلى مكب معتمد خارج المشروع وذلك على نفقة ومسؤولية المتعهد ضمن الأوقات المتفق عليها بين المهندس والإدارة والمتعهد أعمال التكسير على سبيل الذكر ولا الحصر:
ورقة اسمنتية وخرسانة مسلحة وعلى اختلاف أنواعها )أعمدة - قواعد - أرضيات - أدراج أسقف (...
بلاط أرضيات وحوائط بما فيها الطبقة اللاصقة الموجودة مهما كان نوع التشطيب
قطع الصحية للحمامات شاملة الكراسي والمغاسل والمباول وجميع القساطل مهما كانت القياسات والقواطع والواجهات، 
مجلى المطابخ مع الخزائن الموجودة، خزانات مياه على اختلاف أنواعها، حوائط من الحجر الفارغ مهما كانت القياسات والسماكات وتوسيع فتحات أبواب أو إيجاد فتحات جديدة وذلك بواسطة قص الحوائط لتأمين الفتحات وتشمل الاسعار:
استخدام المعدات اللازمة، اليد العاملة، النقليات ووسائل التحميل والنقل، إلخ
	LS
	1

	2
	Reinforced Concrete Jacketing
Remove loose concrete and Laitance. Prepare mechanical steel brush for brushing existing steel reinforcement, treat exposed steel reinforcements with two components corrosion inhibitor based on polymers, cements binders and should be lightly adhesive to metal, epoxy dowels scratch smooth concrete surface where needed to receive new concrete jacket wall, columns, beams. etc all concrete surfaces should be rough free from dust, loose materials and washed with approved high pressure water prior to casting of new concrete, materials, formwork, epoxy, dowels, labor...etc, shop drawings must be submitted prior to installation

	تقوية وحماية الخرسانة المسلحة
إزالة كافة الشوائب والأجزاء الخرسانية الغير ثابتة وطبقات التشطيب الموجودة مهما كان نوعها وسماكتها وذلك ضمن الشروط الفنية في التنفيذ مع تنظيف حديد التسليح ومعالجته بمواد خاصة عازلة للحماية من الصدأ والقيام بتنفيذ زرع حديد التسليح مع التشريك ضمن الحوائط والأعمدة باستخدام مادة الإيبوكسي اللاصقة وذلك حسب التفاصيل المرفقة بالخرائط التنفيذية والموافق عليها من جهة الإشراف وذلك لزوم الاعمدة والحوائط والجسور، وتشمل الأشغال: اليد العاملة، والمواد خرسانة وحديد تسليح، التدعيم والطوبار، إزالة الطبقة المتصدعة والغبار وكل ما يمنع التصاق الطبقة القديمة والجديدة قبل المباشرة في تنفيذ الأعمال وكل ما يلزم لتنفيذ الأعمال حسب الأصول؛ يجب تقديم الخرائط التنفيذية التفصيلية وأخذ الموافقة عليها قبل البدء بالأشغال
	LS
	1

	3. Hollow or Solid Concrete Blocks and Clostra construction
Supply and install hollow or solid concrete blocks as per drawings
Work to include all places as per the drawings, location and the Engineer instructions.
Work to include: Materials, Cement mortar and the use of extruded nets and reinforcement by means of metal gates and the placement of angles of galvanized. steel iron of concrete columns thickness of 4 mm every 60 cm.
Labors and all items needed and instructions by the Engineer
	بناء جدران من البلوك الاسمنتي المفرغ او المصمت
توريد وبناء حوائط من البلوك الاسمنتي المفرغ او المصمت على أن يكون ذو ابعاد اسمنتية منتظمة بطول 40 سنتم وسماكة حسب المطلوب وارتفاع 20سنتم وان تكون صلدة سليمة نظيفة وذات زوايا خارجية قائمة يستعمل لبناء الحوائط حسب ما هو موضح بالمخططات والتكحيل ويكون البلوك مصنوعا من الاسمنت البورتلاندي العادي والركام مكون من الحصى والرمل النظيف الخالي من الاملاح القابلة للذوبان في الماء والتى تؤثر على تماسك الخلطة
على أن تشمل أعمال مباني بلوك الاسمنت المفرغ اعمال الجلسات والعرقات والفتحات ) نوافذ وأبواب ( والجوانب من الخرسانة المسلحة Jambs) + lintels (Sills,، على أن تشمل: المواد والأكسسوارات والسقالات، المونة الإسمنتية، استعمال الشبك الممدد والتسليح بواسطة خوابير معدنية ووضع زوايا من الحديد المغلفن على الأعمدة الخرسانية سماكة 4 ملم كل 60 سنتم، اليد العاملة،  وكل ما يلزم لإنهاء الأشغال حسب الأصول

	3.1.1
	10 cm hollow concrete blocks
	بلوك اسمنتي مفرغ 10 سم 
	M2
	20

	3.1.2
	12 cm hollow concrete blocks
	بلوك اسمنتي مفرغ 12 سم
	M2
	20

	3.1.3
	15 cm hollow concrete blocks
	بلوك اسمنتي مفرغ 15 سم
	M2
	15

	3.2
	Repair of Existing Plaster Internal & External (Cracks)
Rehabilitate and repair cracked and damaged plaster indoor and outdoor, work to include:
Determine the location and remove all loose items around the area
Remove the cracked plaster layer
Install galvanized steel mesh 20 cm width at least
Clean the places with suitable materials
Fill all cracks after widening of 10cm width by tinocrete or approved equal
Apply the finish rough plaster layer
Apply the second smooth plaster layer
All needed items as per drawings and the Engineer instructions

	أعمال ترميم ورقة موجودة إسمنتية داخلية وخارجية:
ترميم ومعالجة الورقة الإسمنتية الداخلية بما فيها الشقوق والفسوخ والفجوات، وتشمل الأعمال:
تحديد الأماكن المراد إصلاحها ومعالجتها
نزع الورقة الإسمنتية الغير فنية والغير سليمة
توسعة الشروخ بحدود 10 سنتم على كامل اتجاه الشرخ
تركيب شبك معدني غير قابل للصدأ
تنظيف مكان الأعمال بالمواد اللازمة بعرض لا يقل عن 20 سنتم
تعبئة الشروخ بمادة Tinocrete أو ما يعادلها
طبقة رشة مسمارية إسمنتية
طبقة إسمنتية خشنة
طبقة إسمنتية ملساء
اليد العاملة والسقالات والمعدات والمواد اللازمة لإنهاء هذا العمل حسب المواصفات وتعليمات الجهة المشرفة
	LS
	1

	4. Woodwork

	4.1
	Timber Kitchen Cupboards – Under-Counter and Upper Cabinets
Timber Cupboard For New Kitchens
Supply and install timber under counter cupboards plastic laminate (hydrofuge) for kitchen with upper cupboards where required with all needed items for fixation (accessories, soft close, block board 22mm thick, etc..) with skirting and concrete upstand whatever the
The Contractor should submit shop drawings for approval
All needed items as per the Engineer instructions

	أعمال خشبية
خزائن خشبية لزوم المطابخ الجديدة
توريد وتصنيع وتركيب خزائن سفلية لزوم المطبخ من الخشب الفورمايكا المعالج لمنع امتصاص الرطوبة والماء (hydrofuge) وخزائن علوية حيث يلزم إنفاذاً للمواصفات والمخططات المرفقة. وتشمل الأشغال:
المواد واليد العاملة، قاعدة خرسانية مرتفعة مع نعلة مهما كانت الأطوال المطلوبة لتنفيذ المطبخ من خشب  Plastic Laminate Hydrofuge Block board 22 mm thick
الخرضوات والأكسسوارات والسكك والمفصلات (نوع تسكير تلقائي) أوروبي الصنع
وكل ما يلزم لإنهاء الأشغال حسب ارشادات المهندس المشرف
يجب على المقاول تقديم مخططات التنفيذ
	LM
	12

	4.2
	Wooden Works, Doors, Frames and Carpentry
Supply and install all timber work with all related items
The joinery works should be of the first-class type and as per specifications and drawings
Work to include: Material and labors, all accessories to be heavy duty (Hinged, Lock, Glass vision, as required…etc)
The frame for any width (Steel, Wood…)	
Paint as follows:
· Anti rust layers
· Putty + one layer of undercoat
· Three layers of epoxy paint
· remove the existing timber panels
· repair the edges
The Contractor should submit shop drawings and all needed items as the Engineer instructions
	الأعمال الخشبية والنجارة:
توريد وتنفيذ جميع الأعمال الخشبية والنجارة بكل مكوناتها وتفاصيلها؛ يجب أن تكون أعمال النجارة المطلوبة من أجود الأنواع وفقاً للخرائط والمواصفات وأن يكون الخشب جاف تماماً وخالي من العقد والشوائب وباقي العيوب، وتشمل أسعار هذه الأعمال على سبيل الذكر وليس الحصر: المواد والنقل والمعدات ، الخرضوات والبراغي والشناكل والمفصلات والغالات... جميعها شديدة التحمل وصناعة أوروبية
الصندوق الخشبي حسب المواصفات مهما كان عرض الحائط مع الحواجب حيث يلزم وفقًا للخرائط
الدهان بجميع أنواعه طبقاً للمواصفات والتفاصيل التالية:
· دهان خلف صناديق الأبواب الخشبية بمادة عازلة للحماية من الرطوبة
· فك وإزالة الأبواب بما فيها الصناديق والحواجب في الأماكن الملحوظة
· تصليح مواقع ومحيط الأبواب بواسطة الورقة حسب الأصول
وعلى المقاول تقديم خرائط تنفيذية تفصيلية لهذه الأشغال للحصول على موافقة الجهة المشرفة قبل البدء بأي أشغال

	4.2.1
	New internal timber Doors 
Supply and install flush timber door as drawings with laminated plastic facing and the door should have 10cm width frame between the plywood and fill with timber beads by tongue and groove each 5cm, and the door edges should behead wood and fixed by tongue and groove frames should be as specified. Refer to description in Item No. 4.1 
Works included, all accessories and fittings, preprinting and finishing paint sides of doors and box frames.
All works should be done as per the Engineer instructions
Single Leaf

	أبواب خشبية داخلية جديدة  
توريد وتركيب باب معاكس للأبواب الداخلية كامل خشب تجليد فورمايكا  (Laminated Plastic) حسب المواصفات المطلوبة مؤلف من برواز خشب زين بعرض 10 سنتم مركب بالفرز واللسان وتقاطيع داخلية من خشب الشوح الجيد قياس (3,5 × 8 سنتم) كل 25 سنتم عرضاً، و (3,5× 3,5 سنتم) كل 5 سنتم طولًا، مغطى على الوجهين بخشب معاكس، باب أول، سماكة 6 ملم تجليد فورمايكا (Laminated Plastic)  سميك على الجهتين ينزل بفرز في برواز خشب زين قياس (3× 4 سنتم) مع فتحة زجاجية للمراقبة
وتشمل الأشغال:
المواد والإكسسوارات كاملة، مع أعمال الدهان للصندوق وجوانب الباب مع الصندوق مع النهو تطبيق للمواصفات الفنية المرفقة والمذكورة في مقدمة البند رقم 4.2.
	U
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	4.2.2
	Rehabilitate the Existing Timber Doors:
As stated in the Preambles of Item 7.1
In addition, rehabilitate the existing timber doors.
	ترميم أبواب الخشبية الموجودة
وفق ما ذكر في مقدمة البند رقم 7.1
يضاف إليه، ترميم وتأهيل أبواب (باب + صندوق + حواجب) موجودة مهما كان قياس الفتحة وعرض الصندوق وكل ما يلزم حسب المواصفات وتعليمات الجهة المشرفة
	U
	12

	5. Aluminum Doors and Windows
Fabricate, supply and install aluminum works as manufactured by SIDEM 2000 first choice with all necessary accessories as per the drawings and the Engineer instructions, cost to include all doors and windows:
· Single glass 6 mm clear on both sides
· Double glass 6-12-6 mm  clear on both sides, and outer Glass should be Tempered)
· Section width 12.5 cm and thickness 2 mm
· Hinges and locks
· Joint Filler
· Mosquito Screen
· Mesh
All items needed as per the Engineer instructions
All as specified and base on an approved shop drawings after exact dimensions

	أعمال أبواب وشبابيك ألمنيوم
تصنيع، توريد وتركيب وحدات من الألمنيوم الكاملة نوع سيدم 2000 نوعية أولى مع زجاج والخردوات شديدة التحمل
حسب الخرائط المعدة لهذه الغاية والمواصفات وتوجيهات المهندس على ان تشمل الأسعار كافة الأعمال الشبابيك والأبواب والمواد المطلوبة لإنهاء البند:
· زجاج طبقة واحدة 6 ملم شفاف من الداخل والخارج
· الزجاج المزدوج 6 ملم بينهما فراغ 12 ملم شفاف من الداخل والخارج
· مقاطع الألمنيوم 12.5 سنتم سمك 2 ملم
· درفة حماية من البرغش
· جميع الخرضوات والمسكات والكاوتشوك والدواليب القشاطات وحشوات الفواصل
· أعمال التسكير حول وحدات الألمنيوم
وكل ما يلزم هذه الوحدات من مواد وأيدي عاملة ونقل وسقالات وسلالم، إلخ وكل ما يلزم حسب المواصفات والخرائط؛ ويشمل السعر أيضاً تحضير الخرائط التفضيلية التنفيذية لهذه الوحدات والحصول على موافقة الجهة المشرفة عليها قبل البدء بأعمال التنفيذ ويعد أخذ والتأكد أخذ المقاسات الفعلية على الموقع

	
5.1
	New External Aluminum windows (Double Glass)
Supply and install the fabricated aluminum windows with double glass (6 - 12 - 6 mm) (Outer Glass should be Tempered) 
	واجهات ألمنيوم جديدة (زجاج مزدوج)
توريد وتركيب نوافذ ألمنيوم واجهات، زجاج شفاف مزدوج (6 - 12 - 6 ملم) وفق ما ذكر في البند 5.1

	M2
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	5.2
	New Aluminum Internal Door
Supply and install aluminum door with frame and related strengthening stud, Works to include:
Materials, and accessories
Labors
All needed items as per the engineer instructions.
Repair all around the opening
	أبواب الألمنيوم الداخلية
توريد وتركيب أبواب من الألمنيوم مع إطار وتقوية حسب الأصول وكامل الخرضوات والأكسسوارات، ويشمل السعر:
· اليد العاملة
· الإكسسوارات وترميم محيط الفتحات طبقاً للمواد الموجودة وكل ما هو مطلوب طبقا" للمواصفات الفنية
PROVIDE NEW ALUMINUM PARTITION DOOR AS INDICATED
	M2
	3

	6. Tiles

	6.1.
	Install New Tiles
Supply and install tiles first choice for the new stair (treads 3cm thick - Risers 2cm thick) and landing tiling 2cm and for all floors or otherwise specified color type and quality to be submitted for approval, works to include:
· Labour, materials and installations
· Under tile fill
· Mortar
· Lining
And needed items to complete the works as per the Engineer instructions.
	تركيب بلاط جديد
توريد وتركيب بلاط لزوم أشغال أدراج جديدة (treads 3cm thick - Risers 2cm thick) وتبليط السفرة وجميع الأرضيات (سماكة 2 سنتم)؛ يتم اختيار اللون والنوعية على الموقع بناء" لإرشادات المهندس المشرف، وفقًاً للخرائط التفصيلية التنفيذية المرفقة، وتشمل الأعمال:
· المواد، اليد العاملة وتركيب؛
· النعلات وبلاط السفر وجميع أشغال النعلات
· الردم اللازم بمواد مناسبة
· المونة والروبة اللازمة وجلي بلاط
وكل ما يلزم لإنهاء الأشغال وفقاً لإرشادات جهاز الإشراف
	M2
	300

	6.2
	Threshold marbles tiles (Doors, Topping, Toilets)
Supply and install 3cm thick threshold as per the Engineer instructions
Cost to include:
· Demolition and removal of old elements where is applicable
· Fixing materials
· All materials
· All labors
All Edges must be rounded or chamfered
All needed items as per the Engineer instructions
	برطاش رخام )أبواب، فوق كراسي الحمامات، قواطع الداخلية للحمامات(
تقديم وتركيب برطاش سماكة 3 سنتم وفقًا لتعليمات المهندس وتشمل الأشغال:
· تحضير مواقع الأشغال بعد نزع القديم وترحيله إن وجد
· المواد اللاصقة اللازمة
· اليد العاملة
· المواد
احرف البرطاش يجب ان تكون مبرومة او مشطوفة
وكل ما يلزم لإنهاء الأشغال حسب المواصفات وتعليمات الجهة المشرفة 
	LM
	10

	6.3
	New external Natural Stone Plinth
Supply and install new natural stone plinth at base of windows facade as per drawings, similar to existing or according to drawing and engineer approval.
Work to include:
· Labors, equipment and support
· Natural plinth (high according to drawings) 8cm thick
· Mortar
· Lining
All needed items and as per the engineer instruction
	شعاير خارجية جديدة من الحجر الطبيعي
توريد وتركيب شعاير خارجية جديدة من الحجر الطبيعي عند أسفل شبابيك الواجهات الخارجية وحيث يلزم طبقا" للمخططات المرفقة وتعليمات المهندس المشرف وموافقته، وتشمل الأعمال
· اليد العاملة والمعدات
· شعيرة  جديدة من الحجر الصخري وطبقا" للإرتفاعات المطلوبة ضمن الخرائط بسماكة لا تقل عن 5 سم
· المونة والمواد كافة مع أعمال التكحيل والروبة
وكل ما هو مطلوب لإنهاء الأشغال حسب المواصفات وتعليمات جهة الإشراف
	LM
	200

	6.4
	Clean and Rub the Existing Floor Tiles and Skirting
Rehabilitate any type of flooring tiles and skirting (ceramic – mosaic, marble…)
Work to include:
· All materials and labors
· Grouting
· Polish and rubbing
All needed items as per the Engineer instruction as specfied
Type 1: Marble
	تنظيف وجلي بلاط الأرضيات الموجودة
إعادة تأهيل البلاط الموجود (أرضيات ,ونعلات وكافة أنواعه) سيراميك، موزاييك، رخام، إلخ....
وتشمل الأشغال:
· كافة المواد واليد العاملة
· الروبة
· الجلي والتلميع
كل ما يلزم لإنهاء الأشغال المواصفات وتعليمات المهندس المشرف
النوع 1: رخام 
	M2
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	7
	Ceiling Works
Suspended Ceilings
The suspended ceiling works to include:
· All panels
· All heavy duty hangers and accessories as specified
· Rails (hidden type)
· Special metal heavy duty suspension systems
· All needed heavy duty accessories and items to complete the works
· Works to be indicated on drawings and as per the specifications
· Works should be coordinated between the starting and the end of the floor panels and also should be coordinated with the electromechanical units in the ceiling
All works should be as instructed by the Engineer
	أعمال الأسقف
أسقف مستعارة
تشمل اعمال الاسقف المستعارة توريد وتركيب:
· جميع الالواح
· نظام التعليق والاكسسوارات  وكافة السكك الغير ظاهرة الشديدة التحمل
· الحمالات وبلاطات الاسقف بأنواعها وبالسماكات والنوعيات التي توضحها الخرائط والمواصفات
· الدهانات بانواعها وعلى أن تكون كل المواد من اجود الانواع
· التنسيق بين البدايات والنهايات وتوزيع وحدات الانارة والتكييف، ومراعاة فتحات الخدمة الضرورية لصيانة التمديدات الميكانيكية والكهربائية فوق السقف المستعار، حسب الخرائط التنفيذية المقدمة من قبل المقاول للاعتماد،
السعر يشمل كافة الأعمال والمواد المطلوبة لانهاء البند طبقاً لاصول الصناعة والمواصفات الفنية وتعليمات المهندس المشرف
	M2
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	8. Paint Work

	8.1
	Paint Works for Wall and Ceilings 
Painting include: prepare the surfaces and treat these surfaces so the surfaces be able to receive the paints, and place 3 layers of putty, The paint should be from the best quality as per specifications and as indicated in drawings, or as the instruction of the Engineer 
The pricing is fully inclusive of all materials and labor, meaning no hidden tool or supply costs
Painting include the following:
· Surface Preparation: Complete removal (scraping) of old paint, followed by sanding and cleaning after every single putty application to guarantee a perfectly smooth finish.
· Putty & Priming: Application of three coats of putty to level the surfaces, followed by a primer coat including spot-repairing (تفقيط) of any remaining minor surface defects.
· Final Painting: Application of three topcoats of paint (or spray) over a lead-free undercoat layer. It explicitly mandates Super Rubber Paint for old walls and ceilings to bridge hairline cracks and resist moisture.
Health & Eco-Standards: Strict requirement for all paint materials to be Lead-Free and Low VOC (Volatile Organic Compounds) to ensure safe indoor air quality.
	أعمال دهان الجدران والأسقف
تشمل أعمال الدهان تجهيز الأسطح ومعالجتها لتكون صالحة لاستقبال الدهانات، ووضع 3 طبقات من المعجون. يجب أن يكون الدهان من أفضل الأنواع وأجودها حسب المواصفات ومماثلاً لما هو مبين في الخرائط، أو بناءً على تعليمات المهندس المشرف.
يشمل التسعير كامل جميع المواد واليد العاملة، مما يعني عدم وجود أي تكاليف مخفية للأدوات أو التوريدات.
أعمال الدهان تشمل ما يلي:
· تجهيز الأسطح (تأسيس الأسطح): الإزالة الكاملة للدهان القديم، يليه الحف (الصنفرة) والتنظيف بعد كل طبقة معجون لضمان الحصول على ملمس ناعم تماماً.
· المعجون طبقة الأساس (البريمر): تنفيذ ثلاث طبقات من المعجون لتسوية الأسطح، يليه طبقة دهان أساس (بريمر) تشمل عملية تفقيط (Spot-repairing) لأي عيوب سطحية بسيطة متبقية.
· الدهان النهائي: تطبيق ثلاث طبقات وجه نهائي من الدهان (أو الرش) فوق طبقة دهان تحضيرية (undercoat)  خالية من الرصاص. ونوع  (Super Rubber Paint) للحوائط والأسقف القديمة لسد الشروخ الشعرية ومقاومة الرطوبة.
· المعايير الصحية والبيئية: اشتراط صارم بأن تكون جميع مواد الدهان خالية من الرصاص ومنخفضة المركبات العضوية المتطايرة (Low VOC) لضمان جودة وسلامة الهواء الداخلي.

	M2
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	8.2
	Outside Walls Paint (Old and New Walls and Ceilings)
Paint for external old and new walls, smooth touch
Work to include:
· Removal of any paint or obstacle
· Rehabilitate the surfaces and make them good
· Polyurethane where needed for cracks
· Apply 2 coats external putty
· Apply one coat of undercoat
· Apply 2 coats of external paint (Role or Brush)
· Apply one layer of external transparent paint (acrylic styrene)
· copolymer elastic water proof)
Pricing shall include all needed scafolding and materials for the best execution of the works
All works and items should be as per manufacturer and the Engineer instructions and approval,
All paint types must be lead-free and Low VOC (Volatile Organic Compounds
	أشغال طرش خارجي جديد (للحوائط والأسقف الجديدة والقديمة)
أشغال طرش خارجي للأعمال المستحدثة، ورقة إسمنتية جديدة أو الواجهات المطلوبة وفقًا لخرائط المرفقة، وتشمل الأشغال:
· قشط جميع الدهانات والعوائق عن الجدران
· تحضير الجدران لتنفيذ أشغال الدهان
· تسكير التشققات والشروخ باستخدام معجونة مرنة (Polyurethane)
· تنفيذ طبقة أساس
· تنفيذ طبقتين من المعجونة الخارجية
· تنفيذ طبقة دهان خارجية شفافة (acrylic styrene)
· تنفيذ طبقة واحدة أساس مانع للنش (copolymer)
يشمل السعر السقالات واليد العاملة ذا خبرة بهذا الاختصاص، وكل ما يلزم لإنهاء الأشغال حسب المواصفات وتعليمات الجهة المشرفة.
جميع أنواع الطلاء يجب أن تكون خالية من الرصاص (Lead free) ومنخفضة المركبات العضوية المتطايرة (Low VOC) لضمان جودة وسلامة الهواء الداخلي
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	8.3
	Paint Water Repellant  Colorless Layer Unleaded on Facades and Supply a Guarantee for Five Years
Supply and paint with Water Repellant paint after cleaning and washing all walls, and remove the existing paint and enlarge all cracks especially at the intersection of the hollow concrete blocks and reinforced concrete slabs and between columns beams and hollow concrete blocks walls (4cm width with 5cm depth) and refill these grooves with polyethylene sealant whatever their width and depth of these grooves and then paint one layer of base paint with acrylic styrene copolymer elastomeric waterproof with a fixation of 400% and dissolved by water and then apply two layers over the base paint with acrylic styrene copolymer elastomeric waterproof and dissolved with water 10% and time needed is 24 hours between each layer.
All works and items should be as per manufacturer and the Engineer instructions and approval, all paint types must be lead free and Low VOC (Volatile Organic Compounds)
	دهان مانع للنش للواجهات مع كفالة خمس سنوات
توريد وتنفيذ دهان مانع للنش شفاف أو ملون وخالٍ من الرصاص، بعد تنظيف وغسل الجدران وإزالة الدهان غير المتماسك. وتشمل الأشغال:
· تنظيف الأسطح وتوسيع الشقوق، خاصة عند التقاء جدران البلوك مع الأعمدة والجسور والأسقف، بعرض 4 سم وعمق 5 سم.
· ملء الأخاديد بمادة Polyethylene Sealant مهما كان طولها.
· تنفيذ طبقة أساس من Acrylic Styrene Copolymer Elastomeric Waterproof بمرونة 400% ومخففة بالماء.
· تنفيذ طبقتين من المادة نفسها مخففتين بالماء بنسبة 10%، بفاصل 24 ساعة بين الطبقات.
يشمل السعر السقالات والمواد واليد العاملة وكل ما يلزم حسب تعليمات المهندس المشرف. جميع الدهانات يجب أن تكون خالية من الرصاص (Lead-Free) ومنخفضة المركبات العضوية المتطايرة (Low VOC).
على المتعهد تقديم كفالة على أعمال منع النش لمدة خمس سنوات.
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	9. Bathrooms Accessories:
Supply and install all needed accessories and make good their places and their surroundings, Place all frame, cover joints (stainless steel) anti-corrosion
Install items and their contact with the surfaces
All works should be done as per the Engineer instructions
All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval 
	لوازم وأكسسوارات الحمامات
توريد وتركيب جميع لوازم الحمامات مع تثبيتها ومعالجة أماكن التركيب والتكحيل. تكون البراويز وأغطية الفواصل والأجزاء المعدنية من الستانلس ستيل المقاوم للصدأ، ويتم التنفيذ في المواقع المحددة بالمخططات وحسب المواصفات وتعليمات المهندس المشرف.
جميع الأكسسوارات يجب أن تكون صناعة أوروبا، اليابان، جنوب كوريا، أو ما يعادله من نوعيه، بعد موافقة المهندس المشرف.

	9.1
	Paper Roller Holder
Supply and install toilet paper holder, stain and rust resistant, steel 316
with all accessories and fixation (anti-rust materials) for good quality and at the places shown on drawings
All works should be done as the Engineer instructions
	حاملة ورق تواليت
توريد وتركيب حاملة ورق من ستانلس ستيل 316 مقاوم للصدأ والبقع، مع جميع الإكسسوارات ومواد التثبيت المقاومة للصدأ، في المواقع المحددة بالمخططات وحسب تعليمات المهندس المشرف.
	U
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	9.2
	Soap Dispenser
Supply and install  soap dispenser, stainless steel 316, rust and stain resistant, wall type fixation (anti-rust materials and accessories) with all needed items
All works should be done as the Engineer instructions
	علبة صابون سائل
توريد وتركيب موزع صابون جداري من ستانلس ستيل 316 مقاوم للصدأ والبقع، مع كامل لوازم ومواد التثبيت المقاومة للصدأ، حسب تعليمات المهندس المشرف.
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	9.3
	Paper Holder Box
Supply and install hand paper holder box, stainless steel 316, rust and stain resistant, with all needed works and fixation (anti-rust materials and accessories)
The box should be from a good manufacturer
All works should be done as the Engineer instructions
	حاملة مناديل ورقية
توريد وتركيب حاملة مناديل ورقية من ستانلس ستيل 316 مقاوم للصدأ والبقع، مع كامل أعمال ولوازم التثبيت حسب تعليمات المهندس المشرف.
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	9.4
	Mirror for Lavatories
Supply and install 6mm glass mirror for lavatories with colored PVC frames (60X100 cm) as show on drawings and as stated in the specifications with all needed items and accessories
The mirror should be placed on 3mm thick plywood from the back
All works should be done as per the Engineer instructions
	مرآة للمغاسل
توريد وتركيب مرآة زجاج سماكة 6 ملم بإطار PVC ملون (60*100 سنتم) حسب المخططات والمواصفات، مع كامل الإكسسوارات والتثبيت، وتركيب خلفية من الخشب سماكة 3 ملم خلف المرآة، حسب تعليمات المهندس المشرف.
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	9.5 PIPED SYSTEMS (LIQUIDS)
Cold & Hot Water Piping Inside Building
Supply, install and test water supply system inside the building.
Pipes should be (PPR) and the price is per linear meter. Cost to include all accessories, connections, reducers, all valves as shown on the drawings, Ø20mm PRV for make-up system where applicable, water hammer arrestor hanging and embedded system, so that all piping can receive ideal standard fixtures
The Contractor should submit shop drawings for approval by the Engineer. Works should be as standard installation details
	أنظمة المواسير - مياه باردة وساخنة داخل المبنى
توريد وتركيب واختبار شبكة مياه داخل المبنى من مواسير PPR، ويحتسب السعر بالمتر الطولي لكل قطر مركب. يشمل السعر جميع الوصلات والأكواع والنقاصات والمحابس المبينة على المخططات، وصمام تخفيض ضغط PRV قطر 20 ملم حيث يلزم، ومانع الصدمات المائية Water Hammer Arrestor ونظام التعليق والتثبيت، بما يؤمن ربط التجهيزات الصحية من نوع Ideal Standard.
على المقاول تقديم مخططات تنفيذية لأخذ موافقة المهندس قبل التنفيذ، وتتم الأعمال حسب تفاصيل التركيب القياسية.

	9.5.1
	Ø 20 mm
	LM
	35

	9.5.2
	Ø 25 mm
	LM
	35

	9.5.3
	Ø 32 mm
	LM
	50

	9.6
	Water Tanks 2000 Litres
Supply and install polyethylene water tank (3 layers) or more with all necessary supply and over flow connections all as per the Engineer instructions
	خزان مياه سعة 2000 ليتر
توريد وتركيب خزان مياه من البولي إيثيلين (Polyethylene) من ثلاث طبقات أو أكثر، مع جميع وصلات التغذية والفائض وكامل الملحقات، حسب تعليمات المهندس المشرف.
	U
	2

	9.7
	Steel tower for Water Tank
Supply, install, construct, steel tower for water tank complete as shown and detailed on drawings, including excavation reinforced concrete footing and support
Fixing and welding in place
Apply two layers of anti-rust paint
Epoxy paint after proper grinding and putting all access welding painting, etc.; and complete in every respect.
All works needed as per specifications and the engineers
instructions.
	سقالة معدنية لرفع خزان المياه
توريد وتصنيع وتركيب سقالة معدنية من الحديد الصناعي لرفع خزان المياه حسب المخططات، بما يشمل الحفر والقواعد الخرسانية المسلحة والدعامات والتثبيت واللحام.
تنفيذ طبقتين من دهان مانع الصدأ ودهان إيبوكسي بعد الجلخ والمعالجة، مع كامل المواد واليد العاملة وكل ما يلزم حسب المواصفات وتعليمات المهندس المشرف.
	U
	2

	9.8
	Western Toilets seats
Supply and install W.C Flush valve with cover as manufactured by Ideal Standard Item No. E876801 also the hose, or approved equal and to be 40 cm from floor finish with cover.
The work to include the installation, clean jointing, all necessary connection, angle valves and necessary accessories.
Each W.C. should be equipped with a Flushing Hose, origin as described in item # 9 or approved equal) 
	كرسي حمام إفرنجي
توريد وتركيب كرسي حمام معلق EWC-01 قياس 52 × 36 سم مع صمام طرد وغطاء، من نوع Ideal Standard E876801 أو ما يعادله المعتمد، وعلى ارتفاع 40 سم من منسوب الأرضية النهائية.
يشمل السعر التركيب والتكحيل والتنظيف وكافة توصيلات المياه والصرف ومحابس الزاوية والأكسسوارات، مع شطاف من Grohe أو Ideal Standard أو ما يعادله، حسب تعليمات المهندس المشرف.
	U
	6

	9.9
	Semi Pedestal Wash Basin
Supply and install semi pedestal wash basin similar to Ideal Standard Item No. 742001 or approved equal and fixed at 82 cm high from the floor finish. Cost to include all necessary connections, angle valves, traps and necessary accessories as specified.

	مغسلة بنصف عامود
توريد وتركيب مغسلة خزف صيني بنصف عامود من نوع Ideal Standard 742001 أو ما يعادله، قياس 55 × 45 سم، تثبت على ارتفاع 82 سم من منسوب الأرضية النهائية.
يشمل السعر جميع التوصيلات ومحابس الزاوية والسيفون والخلاط وكامل الإكسسوارات حسب المواصفات.
	U
	6

	9.10
	Self-Close tap for wash basins
Supply and install self-close taps to be fixed in the lavatory body with all required works and drain accessories including trap, and to be connected to the new water supply and drain and as instructed by the Engineer
	حنفية إغلاق ذاتي للمغاسل
توريد وتركيب حنفية إغلاق ذاتي تثبت على المغسلة، مع كامل لوازم التوصيل بشبكة المياه والصرف، بما في ذلك السيفون والأكسسوارات اللازمة، حسب تعليمات المهندس المشرف.
	U
	6

	
9.11
	Kitchen Sink Accessories
Supply and install kitchen sink accessories such as chrome trap, angle valve, mixers as specified in Item # 9
	أكسسوارات مجلى المطبخ
توريد وتركيب أكسسوارات المجلى، بما يشمل سيفون كروم، محبس زاوية، وخلاط حسب المواصفات في البند # 9.
	U
	3

	9.12
	Taps for Kitchen Sinks
Supply and install taps for kitchen sinks with all required works and drain accessories including trap and to be connected to the new water supply and drain and as instructed by the Engineer; product origin refer  to item # 9
	حنفيات مجالي المطبخ
توريد وتركيب حنفيات من نوع Grohe أو ما يعادلها لمجالي المختبر، مع كامل أعمال التوصيل بشبكتي المياه والصرف والسيفون والأكسسوارات اللازمة، حسب تعليمات المهندس المشرف.
النوعية وفق ما ورد في البند # 9.
	U
	2

	10. Waste water drainage 
Drainage System inside the Building
Supply, install and test the waste water drainage from (UPVC) pipes inside the building to outside and the pipes to be measured in Linear Meter with all related accessories, cleanout, elbows, vent hangers, brackets and all necessary accessories as per standard installation details
The diameter of the pipes are as follows:
	نظام الصرف الصحي داخل المبنى
توريد وتركيب واختبار شبكة صرف من مواسير UPVC من داخل المبنى إلى الخارج، ويحتسب السعر بالمتر الطولي شاملاً جميع الوصلات والأكواع وفتحات التنظيف والتهوية والرباطات وكامل الإكسسوارات، حسب تفاصيل التركيب القياسية.
الأقطار المطلوبة كما يلي:

	10.1.1
	Ø 110 mm / UPVC
	LM
	40

	10.1.2
	Ø 200 mm / UPVC
	LM
	40

	10.2 Floor Drain
Supply and install floor drain P.V.C. with chrome-plated brass drain cover and to be the same level as the floor and do all necessary installation and connections. This includes all civil works and connection to the proper floor pipes and as per the Engineer instructions
	مصفاية أرضية
توريد وتركيب مصفاية أرضية PVC مع غطاء من النحاس المطلي بالكروم، على مستوى تشطيب الأرضية، مع جميع أعمال التركيب والتوصيل بشبكة الصرف والأعمال المدنية اللازمة، حسب تعليمات المهندس المشرف.

	10.2.1
	FD-01: Ø75 mm bottom outlet
	U
	25

	10.3
	Water Heating Solar Panels
Supply and install solar water heating panels, size 2 m2, as specified including supports, fixations, 100 liters storage tank, control wiring, required valves, temperature sensors and all necessary accessories as required
	ألواح تسخين المياه بالطاقة الشمسية
توريد وتركيب ألواح تسخين مياه شمسية بمساحة تقارب 2 م² حسب المواصفات، شاملة الحوامل والتثبيت، خزان تخزين 100 ليتر، أسلاك التحكم، المحابس المطلوبة، حساسات الحرارة وكامل الإكسسوارات اللازمة.
	U
	2

	11
	Booster Pumps
Supply and install booster pumps as specified and scheduled: 230V, 50Hrz, 1PH, P-PW-01 (1.8m3/h; 280 Kpa)
Including pipe work connections with anti-vibration flexible connections, anti-vibration bases and mounting, isolating & check valves, Strainers test points, temperature & pressure gauges, control & power wiring, bonding and identification, thermal insulations and all related works and accessories as specified 
1 Duty/ 1 Standby complete with 18 Liters Pressure Vessel
	مضخات تقوية الضغط
توريد وتركيب مضخات الضغط حسب المواصفات والجداول؛ 230 فولت، 50 هرتز، 1 حصان،  P-PW-01 (تصريف 1.8 م³/ساعة) ضغط 280 kPa،
شاملة توصيلات المواسير المرنة وقواعد التثبيت المضادة للاهتزاز، محابس العزل وعدم الرجوع، المصافي، نقاط الفحص، مقاييس الحرارة والضغط، تمديدات القدرة والتحكم، الربط والتعريف، العزل الحراري وكامل الإكسسوارات.
مضخة تشغيل ومضخة احتياط، كاملة مع خزان ضغط سعة 18 ليتر. 
	U
	2

	13. Basic Electrical Requirements
The Contractor should revise all the drawings and compare them with the actual site conditions and redo all the design works with the necessary calculations for all the electrical installations and works. Moreover, the Contractor should submit all needed shop drawings, subject to the client approval.
At the end of the project, the contractor should submit complete As-Built Drawings, operational and maintenance manuals for all executed works with exact dimensions & sizes for easy maintenance work in the future.
All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval
	متطلبات عامة للأعمال الكهربائية
على المقاول مراجعة جميع الخرائط ومطابقتها مع واقع الفعلي للموقع، وإعادة استكمال التصاميم والحسابات اللازمة لجميع الأعمال والأنظمة الكهربائية، وإعداد وتقديم الخرائط التنفيذية التفصيلية (Shop Drawings) لاعتمادها.
عند انتهاء الأعمال، يقدم المقاول خرائط As-Built كاملة لجميع الأعمال المنفذة موضحاً عليها المواقع والأبعاد والمقاسات الفعلية، ودليلي التشغيل والصيانة لتسهيل أعمال الصيانة مستقبلاً.
جميع الأكسسوارات يجب أن تكون صناعة أوروبا، اليابان، جنوب كوريا، أو ما يعادله من نوعيه، بعد موافقة المهندس المشرف.

	12.1
	Removal of existing electrical network
Remove all the existing cables, wires, sockets, outlets, electrical panel boards, and circuit breakers then prepare the suitable location to reinstall:
Lighting fixtures
Wires and cables
Sockets and switches
Circuit breakers
Disconnecting switches
Electrical panel boards with grounding
Earth pits
Lightning protection (Air terminals, pits & down conductors)
All needed electrical works … etc
All the above should be as per the drawings, specifications and Engineer instructions
	إزالة الشبكة الكهربائية الحالية
إزالة الكابلات والأسلاك والمآخذ والمفاتيح واللوحات والقواطع الكهربائية القائمة، وتحضير المواقع المناسبة لإعادة تركيب:
· وحدات الإنارة.
· الأسلاك والكابلات والمآخذ والمفاتيح.
· القواطع ومفاتيح الفصل ولوحات التوزيع مع التأريض.
· حفر التأريض ونظام الحماية من الصواعق بما يشمل رؤوس الالتقاط والموصلات النازلة.
وجميع الأعمال الكهربائية اللازمة، حسب المخططات والمواصفات وتعليمات المهندس المشرف.
	LS
	1

	12.2
	Electrical Distribution Panel boards
Supply, install, connect and test the electrical main and sub distribution boards in perfect operating conditions as shown on drawings and specified inclusive of enclosure, all busbars, protective devices, digital meters, miniature circuit breakers (MCB) according to IEC 60947-2, and all the necessary components and requirements.
The Electrical board should include:
Main circuit breaker
Sub-main circuit breakers (office, kitchen, toilets, services, etc…)
All above requirements as per drawing and specification and subject to the opproval of the supervisor engineer.
All the above should follow the tender drawings and the Engineer instructions.
	لوحات التوزيع الكهربائية
توريد وتركيب وتوصيل واختبار لوحات التوزيع الرئيسية والفرعية بحالة تشغيل كاملة حسب المخططات والمواصفات، شاملة الغلاف، قضبان التوزيع Busbars، أجهزة الحماية، العدادات الرقمية، وقواطع MCB المطابقة للمواصفة IEC 60947-2 وكامل المكونات.
تتضمن اللوحة القاطع الرئيسي، القواطع الفرعية للمكاتب والمطبخ والحمامات والخدمات وغيرها، وجميع وسائل الحماية والأكسسوارات اللازمة.
التنفيذ حسب مخططات والمواصفات وبعد اخذ موافقة المهندس المشرف.
	U
	2

	12.3
	Electrical Distribution Panel boards for UPS
Supply and install Complete Distribution Board dedicated to UPS-backed loads (capacity for 40 points). Contractor shall state the enclosure/IP rating, busbar rating, incomer and outgoing MCB/MCCB ratings and breaking capacities, number of ways, phase arrangement, neutral and earth bars, labels, and all required accessories.
Datasheet and proposed panel schedule shall be submitted prior to execution and subject to the approval of the supervisor engineer
	لوحات التوزيع الكهربائية الخاصة  بال UPS
توريد وتركيب لوحة توزيع متكاملة مخصصة للأحمال المغذاة من نظام UPS (القدرة الإستيعابية 40 نقطة كهربائبة) . على المتعهد تحديد درجة الحماية IP، سعة قضبان التوزيع Busbars، تيارات وقدرات قطع القواطع الرئيسية والفرعية MCB/MCCB، عدد المخارج، ترتيب الأطوار، قضبان Neutral وEarth، الملصقات وجميع الملحقات.
يجب تقديم ورقة البيانات الفنية (Datasheet) وجدول اللوحة المقترح (Panel Schedule) قبل التنفيذ وأخذ موافقة المهندس المشرف.
	U
	2

	14. Electrical Work

	13.1

	Disconnecting Switches
Supply, install and test the disconnecting switches in perfect operating conditions including the conduits, boxes, wiring according to IEC-609473 with steel cover and protection degree not less than IP=55 as shown on the drawings, specifications and Engineer instructions.
10A 250V one way one gang switch
All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval
	مفاتيح فصل
توريد وتركيب واختبار مفاتيح الفصل (Disconnecting Switches) بحالة تشغيل كاملة، شاملة المواسير والعلب والأسلاك، وفق IEC 60947-3، بغطاء فولاذي ودرجة حماية لا تقل عن 55IP، حسب المخططات والمواصفات وتعليمات المهندس المشرف.
مفتاح مفرد اتجاه واحد 250 فولت 10 أمبير.
جميع الأكسسوارات يجب أن تكون صناعة أوروبا، اليابان، جنوب كوريا، أو ما يعادله من نوعيه، بعد موافقة المهندس المشرف.
	U
	60

	13.2 Electrical Sockets
Supply, install and test single socket outlet, 250 Volt, 16 Amp, special children type, with all the necessary protection. The cost includes conduits, cables, wires, and all accessories as per the drawings, specifications and Engineer instructions. All accessories should be made in Europe, USA, Japan, South Koria or equal quality, and subject to the engineer approval
	مآخذ الكهرباء
توريد وتركيب واختبار مخرج كهرباء 250 فولت 16 أمبير. يشمل السعر المواسير والكابلات والأسلاك وجميع الإكسسوارات حسب المخططات والمواصفات وتعليمات المهندس المشرف.
جميع الأكسسوارات يجب أن تكون صناعة أوروبا، اليابان، جنوب كوريا، أو ما يعادله من نوعيه، بعد موافقة المهندس المشرف.

	13.2.1
	16A 250V 3 pin wall mounted socket outlet
	U
	70

	13.2.2
	16A 250V 3pin wall mounted socket outlet UPS
	U
	70

	12.2.3
	RJ45 CAT6 data outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	70

	13.2.4
	RJ45 CAT6 camera outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	16

	13.2.5
	RJ45 CAT6 access point outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	10

	13.2.6
	RJ45 CAT6 access control outlets with 5x4pairs CAT6 cables to corresponding patch panel
	U
	2

	15. Lighting Fixtures
Supply, install and test the lighting fixtures complete with all the necessary wires conduits, boxes and accessories required to provide power to each lighting fitting from LP including the earth wire as per the drawings, specifications and Engineer instructions.
The Contractor should submit samples of each lighting fixture for approval.
	وحدات الإنارة
توريد وتركيب واختبار وتشغيل وحدات الإنارة، شاملة الأسلاك والمواسير والعلب وجميع الإكسسوارات اللازمة للتغذية من لوحة الإنارة LP، بما في ذلك سلك التأريض، حسب المخططات والمواصفات وتعليمات المهندس المشرف.
على المقاول تقديم عينات من كل نوع إنارة للاعتماد قبل التنفيذ.

	14.1.1
	Led Panel Light 60X60 60W 110/220V Day light; surface mounted type.
	U
	30

	14.1.2
	Ceiling mounted lighting fixture, Spot Led, diameter 20 cm
	U
	16

	14.1.3
	Led Wall-mounted globe/hublot luminaire 20 W
	U
	5

	14.2
	HDMI wall outlet/link. Complete with wall plates, back boxes, conduit and accessories, and cable 15 m run.
The minimal requirement for the HDMI: version 2.1 compatible, supported resolution/refresh rate up to 8K at 60 Hrz, HDCP compatibility 2.2 to 2.3, cable’s construction hybrid optical fiber plus coper conductor.
	نقطة/وصلة HDMI جدارية
توريد وتركيب نقطة HDMI جدارية، كاملة مع لوحات والعلب الخلفية والمواسير والإكسسوارات الجدار وكابل HDMI طول 15م.
	U
	5

	14.3
	Electrical outlet for electrical Powered door
Electrical door equipment include wiring, conduit, outlet/back box, isolation/termination and accessories up to door equipment connection point. Supplier to confirm connected load, voltage, interface requirement and cable size based on offered door equipment.
	مخرج كهربائي لباب المدخل:
توريد وتنفيذ مخرج كهربائي لتجهيزات أبواب المداخل، شاملاً الأسلاك والمواسير والعلبة الخلفية ووسيلة العزل/النهاية والإكسسوارات حتى نقطة توصيل الباب.
على المتعهد تحديد الحمل والجهد ومتطلبات الربط ومقطع الكابل حسب تجهيز الباب المقترح.
	U
	2

	14.4
	Outlet for ventilation/exhaust fan.
Include wiring, conduit, outlet/isolator connection provisions and accessories. Supplier to confirm fan voltage, power, starting current, local isolator requirement and final cable size.
	مخرج لمروحة تهوية/شفط
توريد وتنفيذ مخرج لمروحة تهوية أو شفط، شاملاً الأسلاك والمواسير وتجهيزات نقطة التوصيل/مفتاح العزل والإكسسوارات.
على المورد تحديد الجهد والقدرة وتيار الإقلاع والحاجة إلى مفتاح عزل محلي ومقطع الكابل النهائي.
	U
	6

	14.5
	Empty provisional outlet point
Including approved box (10x10 cm ), conduit (25 mm) route to accessible service zone or designated source, draw wire, cover plate and identification label
	نقطة احتياط فارغة
تنفيذ نقطة احتياط فارغة تشمل علبة معتمدة (20*20 سنتم) ومواسير(25 مم قطر) حتى منطقة خدمات متاحة أو مصدر محدد، مع سلك سحب وغطاء وملصق تعريف.
	U
	20

	16. Video Surveillance & recorder

	15.1
	Video surveillance CCTV
Supply, install, connect, label, test and commission a complete IP CCTV system including, fixings, frames, programming, software suites, connections and all necessary accessories for a complete and perfect operation as specified and shown on drawings and to the satisfaction of the engineer
High resolution colored CCTV dome (fixed) IP camera with auto iris, vary focal lens & PoE, ceiling mounting adapter or wall bracket.
	نظام المراقبة بالكاميرات
توريد وتركيب وتوصيل وترقيم واختبار وتشغيل نظام CCTV IP متكامل، شاملاً المواسير الصلبة ووسائل التثبيت والحوامل والبرمجة والبرامج والتوصيلات وجميع الإكسسوارات اللازمة للتشغيل الكامل حسب المخططات والمواصفات وموافقة المهندس.
كاميرا Dome IP ثابتة ملونة عالية الدقة، بعدسة متغيرة البعد البؤري وAuto Iris وPoE، تثبيت سقفي أو جداري. 
	U
	16

	15.2
	Network video recorder (NVR):
Supply and install NVR, 32 IP CCTV cameras with 10 TB storage capacity
	جهاز تسجيل شبكي NVR
توريد ,وتركيب جهاز NVR ،32 كاميرا IP CCTV، بسعة تخزين 10 TB.
	U
	1

	16
	Chipboard Panels
Supply and installation of 5 mm thick Chipboard panels, with approximate panel dimensions of 2800 mm height × 1200 mm width. The panels shall be of suitable quality for the intended application, moisture-resistant and easy to clean, with a uniform finished surface free from defects, waves, scratches, or visible imperfections.
The item shall include complete supply and installation of the panels, including surface preparation, measurement, cutting, fitting, and installation, as well as the supply and application of suitable adhesive materials specifically intended for fixing the panels to walls. The adhesive shall be recommended by the panel manufacturer and compatible with the existing wall surfaces.
The rate shall also include the supply and installation of all required accessories and finishing profiles, including, as applicable:
· H-Profiles
· Corner Profiles
· End Profiles/End Caps
· Internal and external corner profiles, panel joint profiles, Edge Trims, and all necessary fixing and ancillary materials required to provide a complete and uniform finished installation.

The rate shall include all transportation, loading, unloading, lifting, handling, cutting, installation, fixing, finishing, and final cleaning, together with all equipment, tools, and labour required to complete the works in accordance with good workmanship practices and the instructions of the Supervising Engineer. The completed installation shall be handed over fully finished and ready for use.
	ألواح الشيبورد
توريد وتركيب ألواح chipboard بسماكة  5 ملم وبأبعاد تقريبية 2800 x 1200 ملم، على ان تكون من نوعية جيدة مقاومة للرطوبة، سهلة التنظيف، وذات سطح متجانس وخالٍ من العيوب والتموجات والخدوش.
تشمل الأعمال تجهيز الأسطح، أخذ القياسات، القص والتركيب، وتثبيت الألواح على الجدران باستخدام مادة لاصقة مناسبة ومعتمدة من الشركة المصنعة ومتوافقة مع الأسطح القائمة.
كما يشمل السعر توريد وتركيب جميع الإكسسوارات وقطاعات التشطيب اللازمة، بما فيها حسب الحاجة:
· End
· Corner Profiles
· H-Profiles
· Edge Trims
· Profiles/End Caps
· وقطاعات الوصل والزوايا الداخلية والخارجية وكافة مواد التثبيت اللازمة لإنهاء الأعمال بشكل متكامل.

يشمل السعر كذلك جميع أعمال النقل والتحميل والتنزيل والمناولة والقص والتثبيت والتشطيب والتنظيف النهائي، مع كامل المعدات والأدوات واليد العاملة، وتسليم الأعمال كاملة وجاهزة للاستعمال حسب الأصول وتعليمات المهندس المشرف.

	M2
	950



All unit rates shall include labor, materials, equipment, transport, testing, permits, overheads, incidental works, and all obligations necessary for the complete execution and handover of the works.
4. [bookmark: _Toc238047611]Method Statement and Implementation Methodology
The bidder shall submit a detailed project-specific method statement describing the proposed procedures, construction methods, materials, resources, and sequence of execution.
The methodology shall cover, at minimum:
· Mobilization and site establishment.
· Site inspection, verification of existing conditions, and setting out.
· Protection of existing structures, utilities, equipment, and operational areas.
· Demolition and removal of existing walls, tiles, sanitary fixtures, doors, windows, and other designated items.
· Waste management, debris removal, and disposal of demolition materials.
· Construction of new partitions, masonry works, and associated finishing works.
· Supply and installation of floor and wall tiles in kitchens and sanitary facilities.
· Supply and installation of aluminum windows and doors.
· Supply and installation of wooden kitchen cabinets and kitchen top and accessories.
· Plumbing and sanitary works, including installation of sanitary fixtures, fittings, and the water storage tank.
· Electrical works, including wiring, distribution panels, lighting fixtures, switches, sockets, testing, and commissioning.
· Cleaning, repair, and waterproofing treatment of external walls.
· Testing, commissioning, snagging, and corrective works.
· Final cleaning, preparation of as-built documentation, and project handover.

The document shall clearly explain the relationship, coordination, and sequencing between the different activities, demonstrating how the Contractor will complete the works safely, efficiently, and within the specified contract duration while minimizing disruption to the operation of the facility.
5. [bookmark: _Toc238047613]Health, Safety, Security and Environment Plan
The bidder shall submit a project-specific Health, Safety, Security and Environment Plan describing how workers, visitors, surrounding communities, existing infrastructure, and the environment will be protected.
6. [bookmark: _Toc238047614]List of Equipment and Machinery
The Bidder shall provide a list of the principal equipment, tools, and resources proposed for the execution of the works, indicating whether each item is owned or rented.
The list shall include, as applicable, equipment and tools required for demolition, construction, finishing, waterproofing, electrical, plumbing, lifting, transportation, and material handling activities.
7. [bookmark: _Toc238047615]Previous Experience
· At least four executed rehabilitation works during the last 5 years of a minimum value of USD 100,000 each.
The following information shall be provided for each project:
· Client name.
· Contract or project name.
· Contract value.
· Project location.
· Contract period and completion date.
· Brief description of the works.
· Client contact details.
· Completion or handover certificate.
· Contract, purchase order, or other supporting evidence. 

Priority will be given to contractors with proven experience in rehabilitation and renovation works, especially projects implemented for national and international humanitarian organizations.
8. Proposed Contract Personnel
The bidder shall provide the names, positions, professional licenses, qualifications, and relevant experience of the proposed key personnel.
The proposed team shall include, at minimum:
· Project Manager: Licensed Engineer with at least five years of relevant experience in building construction, renovation, or rehabilitation projects. 
· Site Engineer: Licensed Engineer with at least five years of relevant site experience. 
· Foreman: Minimum five years of relevant supervisory experience in construction and rehabilitation works. 

Curricula vitae, professional licenses, certificates, and supporting experience documents shall be attached.
The Foreman shall be continuously present on site during the execution of the works, and the Contractor shall ensure that qualified technical personnel are available throughout the project duration.
9. [bookmark: _Toc238047616]Proposed Materials, Manufacturers and Brands
The bidder shall submit the proposed make, manufacturer, country of origin, technical specifications, standards, and data sheets for all key materials.
The Bidder shall submit the required technical data sheets and catalogues for the main materials, equipment, and systems proposed under the project. The submission shall include, at a minimum, the following:
1. Aluminum windows and doors.
2. Internal wooden doors and ironmongery.
3. Sanitary fixtures and fittings.
4. Water storage tank.
5. Waterproofing materials external walls.
6. Electrical distribution and control panels.
7. Lighting fixtures.
8. Switches, sockets, and electrical accessories.
9. Partition systems and associated materials.
10. Paint material catalogues and types.
11. Chiboard 
The submitted technical data sheets shall clearly indicate the product specifications, manufacturer, country of origin, dimensions, performance characteristics, compliance with applicable standards, and any other information required to assess the suitability of the proposed materials and equipment. The Lebanese Red Cross reserves the right to request additional documentation or samples prior to approval.
The bidder shall submit the following physical samples with the Technical Offer:
1. Floor and wall tiles proposed for the kitchen and WC areas.
2. Aluminum window profile sample.
3. Aluminum door profile samples.
4. Aluminum partition profile samples.
5. Chiboard, glue and all necessary accessories.

All samples shall be clearly labeled with the manufacturer's name, product reference, and proposed application area and relevant item number in the BOQ. The Lebanese Red Cross reserves the right to request additional samples, mock-ups, or alternative materials for review and approval prior to procurement and/or installation.
10. [bookmark: _Toc238047618]Work Program and Time Schedule
Provide a plan of works to show the duration and planned sequence of the Works including all of the activities that will be required to carry out the works including materials delivery, equipment mobilization and manpower requirements. The time schedule should take into consideration the location, access and nature of the site with specific security measures and necessary access permits.
Works shall be completed by December 15th, 2026. 
G. [bookmark: _Toc238047619] Permits and Coordination
The contractor shall be solely responsible for obtaining all necessary permits required for the execution of the works. 
H. [bookmark: _Toc238047620]Selection and Award Criteria
Mandatory Compliance / Elimination Criteria – Pass/Fail:
. Failure to comply with any of the requirements below shall result in the elimination of the bidder from further evaluation.
1. Mandatory Site Visit: Attendance at the pre-tender site visit is compulsory. The bidder shall sign the attendance provided by the client during the site visit.
2. General Experience: Minimum 4 successfully completed construction projects during the last five years.
3. Minimum Project Value: Each of the above-mentioned similar projects shall have a minimum completed contract value of USD 100,000.
4. Mandatory Material Samples: The bidder shall submit samples of tiles, chiboard , and aluminum profiles with the tender submission. Other materials samples shall be subject to on-site review and approval, as applicable.
5. Technical Data Sheets: Item-specific technical data sheets are mandatory for all proposed materials/products. The submitted data sheets shall clearly identify and describe the exact proposed relevant product and demonstrate compliance with the technical specifications. Generic or general catalogues shall not be accepted. Failure to provide the required relevant data sheets shall result in elimination.
6. Preliminary Work Program: The bidder shall submit a general work program indicating the main work phases, sequence of execution, key miles stones and estimated duration, demonstrating the bidder’s ability to complete the works within the contractual completion period.

The Technical Evaluation aims to assess the bidders’ capability, experience, understanding of requirements, and the quality of proposed design and materials.
	CRITERIAS
	Award criteria’s
	Score up to
	Max. Score
	% of overall

	Capability / competence of tenderer to perform the service required
	1. Similar experience in the field of rehabilitation and construction projects completed and handed over during the last 5 years: At least four executed similar rehabilitation projects during the last five years with the same scope of works of a minimum value of USD 100,000 each (15 pts)
2. Client Reference: References from previous NGO, humanitarian organization clients, will be considered an added advantage, particularly for similar scope and nature of works. (5 pts)
	20
	35
	35%

	
	Qualifications, skills, experience of key personnel engaged in the project, including sub-contractors, Site engineer, Project Manager, Quality Control Engineer, Foreman, Surveyor: (10 pts)
	10
	
	

	
	Available machinery and equipment: (5 pts.)
	5
	
	

	Quality / Understanding of requirements
	Proposed Methodology: (20 pts)
Bidder’s understanding of the tender: (5 pts)
	25
	35
	35%

	
	Ability to meet delivery dates & Reliability of plan proposed, October 31st , 2026: (10 pts)
	10
	
	

	TOTAL MAXIMUM GENERAL SCORING
	70%



Only technically compliant offers shall proceed to financial evaluation. The technical offer shall be evaluated out of 70 points.
A bidder must obtain a minimum technical score of 49 out of 70 points to be considered technically qualified. 
The financial score will be calculated as follows: Financial Score = (Lowest Financial Offer ÷ Bidder Financial Offer) × 30
Where:
· Lowest Financial Offer = lowest priced compliant bid
· Bidder Financial Offer = price submitted by each qualified bidder
[bookmark: _Toc238047621]GENERAL
[bookmark: _Toc238047623] ITEMS DESCRIPTION
The items descriptions provided in the Bill of Quantities may not fully detail the scope, conditions, or methods of execution. The Contractor is required to refer to this specification document, the drawings, and all other contract documents for the complete definition of the works to be executed. Each item in the Bill of Quantities shall be read in conjunction with the full set of Contract Documents. The absence of a detailed description in the BOQ shall not relieve the Contractor from the obligation to perform all works necessary for the proper and complete execution of the Contract in accordance with the specified requirements in the contract.
[bookmark: _Toc238047624] SCOPE OF WORK
As part of the Lebanese Red Cross's efforts to enhance the operational capacity, functionality, and safety of its Disaster Risk Reduction (DRR) facilities, rehabilitation and upgrade works will be implemented at the Beirut Hazmieh DRR Office, Beirut, Lebanon.
The project aims to rehabilitate and upgrade the existing DRR Office through a comprehensive package of civil, architectural, mechanical, electrical, and plumbing works to improve the working environment, enhance operational efficiency, and strengthen the office’s capacity to support Disaster Risk Reduction activities and services.
. The scope of work includes, but is not limited to, the following activities:
· Site Inspection and Measurements of the existing facility and verification of site conditions.
· Site Preparation and Demolition Works, including the removal of selected existing walls, tiles, sanitary fixtures, doors, windows, and other deteriorated elements.
· Architectural and Finishing Works, including the supply and installation of new floor and wall tiles in kitchens and WCs, , and all associated finishing works.
· Supply and Installation of kitchen top and woodenKitchen Cabinets and related accessories.
· Supply and Installation of New Doors and Windows, including aluminum windows, aluminum doors, internal wooden doors
· Plumbing and Sanitary Works, including the supply and installation of new sanitary fixtures, fittings, and a water storage tank.
· Electrical Works, including new electrical wiring, distribution and control panels, lighting fixtures, switches, sockets, testing, and commissioning.
· External Wall Treatment, including cleaning, repair, and waterproofing of external walls.
· Testing, Commissioning, and Handover of all installed systems and completed works, including final cleaning and preparation of as-built documentation.
The Contractor shall provide all labor, materials, equipment, supervision, transportation, and services necessary for the complete and satisfactory execution of the works in accordance with the contract documents and the requirements of the Lebanese Red Cross.
[bookmark: _Toc238047627]RATES AND PRICES
The Contractor shall be deemed to have inserted against each item in the Bills such rates and prices as he may deem necessary to cover the requirements of the Contract. Where neither price nor rate is entered against an item or if the term “included” or any such similar term is used it shall be deemed to have been included in the other priced items in the BOQ and measured accordingly. All rates and prices entered against any item in the BOQ shall be deemed to include all the detailed requirements of the specifications and contract.
Rates and prices shall be inserted in the unit rate column of the Bill of Quantities. Each part of the Bill of Quantities shall be totaled, and the totals carried to the Summary and Grand Summary.
[bookmark: _Toc238047628]PRE- AND POST-INSTALLATION DOCUMENT
The Contractor shall prepare and submit all relevant documentation to support the proper planning, execution, monitoring, and handover of the works. Documentation shall include, but is not limited to, the following:
· Method Statements covering all major construction, demolition, installation, and finishing activities.
· Project-specific Health & Safety Plan.
· Quality Control Plan (QCP) detailing material inspections, workmanship controls, and testing procedures.
· Site measurements and verification reports, as required.
· Shop Drawings for all relevant works, including partitions, doors, windows, staircases, electrical installations, plumbing works, heating system, waterproofing details, and other construction elements.
· Detailed calculation notes for structural, mechanical, and electrical works where required or instructed by the LRC Engineers.
· Technical data sheets for all materials, equipment, fixtures, and systems proposed under the project.
· Detailed work program showing all major activities, milestones, and the critical path.
· As-Built Drawings reflecting the actual execution of the works.
· As-Built BOQ based on the final executed quantities.
· Operation & Maintenance (O&M) Manuals for all installed equipment and systems, including the heating system, electrical panels, water tank, and other applicable installations.
· Testing and commissioning reports for all relevant systems and installations.
· Material compliance certificates, manufacturer certificates, and product warranties.
RECORDS AND “AS-BUILT” DRAWINGS
Upon completion of the works, the Contractor shall submit as-built drawings and an as-built BOQ reflecting the actual works executed on site. The as-built documentation shall clearly indicate the final dimensions, locations, specifications, and installation details of all constructed, rehabilitated, and installed elements, including partitions, doors, windows, sanitary installations, electrical systems, heating systems, waterproofing works, water tank, RC staircases, and other project components. 
[bookmark: _Toc238047629]CONSIDERATIONS AND REMARKS
The Contractor shall be responsible for submitting detailed method statements, shop drawings, calculation notes, and technical data sheets for all works and equipment to be installed, all of which must be reviewed and approved by the LRC Engineers. General requirements such as testing, commissioning, training, preparation of as-built drawings, insurance, and warranty obligations shall not be compensated separately; their costs must be deemed included within the contract and BOQ total price. Any damage to existing utilities caused during the execution of the works shall be repaired by the Contractor at their sole cost and responsibility, with no entitlement to additional payment or time extension. Furthermore, the cutting of existing trees is strictly prohibited under this contract.
[bookmark: _Toc238047630]HEALTH AND SAFETY MEASURES 
The contractor shall be required to strictly adhere to comprehensive health and safety measures throughout the project, in accordance with applicable local and international regulations and industry best practices. These measures include but are not limited to the implementation of good hygiene practices, providing appropriate Personal Protective Equipment (PPEs) to workers and visitors, establishing a robust health monitoring system, conducting regular safety monitoring activities, conduct safety training, and foster a safety-conscious environment on-site. The contractor is responsible for the effective implementation of these requirements to ensure the well-being of all personnel involved in the project. 
[bookmark: _Toc238047631]COORDINATION WITH LOCAL AUTHORITIES
The contractor is responsible for establishing effective communication and coordination channels with relevant local authorities throughout the execution of works under LRC supervision. The contractor shall obtain all necessary permits, licenses, and approvals from local authorities prior to commencing the project. This may permits required by local regulations. The contractor shall ensure compliance with all applicable laws and regulations and provide evidence of such compliance as requested by the local authorities, at no additional cost.
[bookmark: _Toc238047632]PRIVATE LANDS
The Contractor shall not enter upon or occupy with men, tools, or materials of any nature, any lands other than the working areas specified, except after consent shall have been received by him from the proper parties and a certified copy of such consent shall have been furnished to LRC Engineers. Any rentals or damages paid for occupying private lands shall be at the Contractor’s expense.
[bookmark: _Toc238047633]EXISTING SERVICES
The Contractor shall verify existing site conditions and identify any utilities or services that may be affected by the Works. Existing installations shall be protected throughout construction.
Any required relocation, modification, disconnection, reconnection, or reinstatement of existing services shall be carried out by the Contractor as necessary for the proper execution of the Works.
Any damage caused by the Contractor to existing structures, utilities, finishes, or equipment shall be repaired at the Contractor's own expense and to the satisfaction of the Engineer. All associated costs shall be deemed included in the Contract Price.
[bookmark: _Toc238047634]GOVERNMENT REGULATIONS
The Contractor shall comply with all applicable laws, regulations, and orders issued by relevant governmental, municipal, and utility authorities. The Contractor shall cooperate with the Employer in providing any information required by such authorities and shall ensure that the requirements of this clause are incorporated into any subcontract entered into for the Works.
[bookmark: _Toc238047635]FACILITIES FOR THE ENGINEER’S REPRESENTATIVE
The Contractor shall provide all necessary personal protective equipment (PPE) and safety gear for the use of authorized site visitors, including the Employer, the Engineer, their respective staff, and representatives of any relevant authorities. This provision shall ensure safe access and compliance with site safety regulations for all official visitors throughout the duration of the works.
[bookmark: _Toc238047636]ACCESS TO WORK
The Engineer and his duly appointed representatives and the Employer or his representatives or agents may at any time and for any purpose whatsoever enter and upon the work and the premises used by the Contractor. The Contractor shall provide free, proper, and safe facilities, therefore.
[bookmark: _Toc238047638]PRECAUTIONS AGAINST CONTAMINATION OF THE WORK
The Contractor shall keep the site clean, safe, and orderly at all times and shall take all necessary measures to prevent pollution, contamination, and accumulation of waste during the execution of the Works. 
[bookmark: _Toc238047639]SITE UTILITIES
The Contractor shall be solely responsible for providing all necessary site utilities, including water, drainage, and power supply, at their own expense. 
[bookmark: _Toc238047640]ACCESS TO PROPERTIES
The Contractor shall ensure that access to the facility remains safe and functional throughout the execution of the Works. Any temporary restriction of access shall be coordinated in advance with the Lebanese Red Cross. 
[bookmark: _Toc238047641]WARRANTY
The Contractor shall provide a comprehensive warranty for the completed works, materials, and installed equipment for a period of one (1) year from the date of project completion, unless a longer warranty period is specifically required for certain equipment. During this warranty period, the Contractor shall, at no additional cost to the Employer, promptly repair or replace any defects, failures, or malfunctions resulting from defective workmanship, materials, or equipment. The warranty shall cover all aspects of the project as defined in the Contract and shall extend to both visible and latent defects.
[bookmark: _Toc238047642]TESTING AND COMMISSIONING 
The Contractor shall be responsible for the testing and commissioning of all works, equipment, and systems installed under the project to ensure compliance with the contract requirements and proper operational performance.
All necessary inspections, tests, and commissioning activities shall be carried out in the presence of the Engineer or DRR representative. Any defects or deficiencies identified during testing shall be rectified by the Contractor at no additional cost.
Upon completion of the Works, the Contractor shall submit all relevant testing and commissioning reports, together with certificates, warranties, and any required documentation, confirming the successful operation and handover of the installed systems and equipment.
[bookmark: _Toc238047643]INSURANCE
[bookmark: _Toc238047644]The cost of all required insurance policies shall be deemed to be included within the contract price. This includes, but is not limited to, the insurance of the Contractor’s personnel and staff, equipment, and any liabilities related to the Employer and their representatives, in accordance with the conditions of contract and applicable laws and regulations. The insurance shall also explicitly cover risks related to war, armed conflict, civil unrest, and acts of terrorism. No separate payment shall be made under this item. The Lebanese Red Cross (LRC) shall not be held liable for any loss, damage, injury, or claim arising from inadequate, insufficient, or missing insurance coverage on the part of the Contractor. 
TRAINING 
The Contractor shall provide, at no additional cost, technical training to the Lebanese Red Cross designated personnel on the operation and maintenance of all installed systems and equipment. The training shall be conducted by qualified personnel prior to project handover and shall include the delivery of relevant operation and maintenance documentation. Attendance records shall be submitted as part of the handover package
[bookmark: _Toc238047648]TECHNICAL DOCUMENTATION AND SUBMITTALS
The Contractor shall prepare and submit at no extra cost all required technical documentation in accordance with the project specifications, timelines, and the Engineer’s instructions. This shall include, but not be limited to, the following: detailed shop drawings, as-built drawings, calculation notes, method statements, equipment datasheets, POW, and operation and maintenance (O&M) manuals.
All documents shall be submitted in both hard copy and editable digital formats, as required, and shall be subject to the Engineer’s review and approval prior to implementation. The Contractor shall ensure that all submittals are accurate, coordinated, and delivered in a timely manner to avoid any delay to the progress of the works.


























FIRST FLOOR – EXISTING FLOOR PLAN (AS-BUILT)
EXISTING SITE CONDITION
SCALE 1:100
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SECOND FLOOR – EXISTING FLOOR PLAN (AS-BUILT)
EXISTING SITE CONDITION
SCALE 1:100
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FIRST FLOOR – RENOVATION WORKS PLAN
PROPOSED WORKS
SCALE 1:100
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SECOND FLOOR – RENOVATION WORKS PLAN
PROPOSED WORKS
SCALE 1:100
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1. All dimensions are in meters.

2. This drawing shows the current
(existing) layout of the building
based on site measurement.

3. Dimensions are approximate
and to be verified on site.

4. This plan is for documentation
and reference purposes only.

EXISTING FLOOR PLAN
(AS BUILT)

SCALE 1:100

L—],qn«o~





image4.png
[S 11.6200 ~
T T 7
i T T
1 T m
i
T T
1
37800 46300 45100
o g g
8 < <
3
T
= ;
|——s.ssn| — 25900 T
—2.8500
& A3 ——=
T 15000
|
§ g
N - 6.6500 T
LEGEND:
Existing Wall
— 5.9524 54414
=== Existing Window
(As Built) g §
Existing Door = i
(As Built)
Existing Balcony /
Terrace (As Built) |
T T T
T i
NOTES: HHH HH t
1. Alldimensions are in meters. + HHH
2. This drawing shows the current AEEmaEmEmEmmaEmEEEEE| 5 HHHH

(existing) layout of the building
based on site measurement.
3. Dimensions are approximate
and to be verified on site.
4. This plan i for documentation
and reference purposes only.

SECOND FLOOR - EXISTING FLOOR PLAN

(AS BUILT)

EXISTING SITE CONDITION

Scale: 1:100

|——1.mn——|

Y





image5.png




image6.png
0086°E

B8
84

00582

88884848





image7.png
TOILET PAPER HOLDER (WITH COVER)

AISI 316 STAINLESS STEEL

Wall mounted toilet paper holder with cover, made of high quality AISI 316 stainless steel,

rust and stain resistant, satin finish.

FEATURES:

* Material : AISI 316 Stainless Steel

« Finish : Satin (Brushed)

« Corrosion and stain resistant

+ Wall mounted with concealed fixing

« With cover (lid)

* Suitable for commercial and residential use

COMPLETE WITH:

« Stainless steel screws and anchors (AISI 316)
« All necessary fixing accessories

« Ready for installation
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