National tender application pack V0.3Lebanese Red Cross 

Tender reference: 2026-100
[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered.
· The contract will be awarded to the lowest-cost technically compliant complete lot
· The quantities mentioned below are required unless there is a variation within a specified range with proper justification. The LRC reserves the right to increase or decrease the quantities.
· The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.  
· In the event of any discrepancy between the unit price and the total price, LRC reserves the right to rely on the unit price as stated in the financial bid, rather than the total price without go back to the supplier. The unit price must be provided with no more than two decimal places.
· Bids must include customs, clearance, transportation, insurance, installation, commissioning or other charges. No additional charges shall be accepted unless expressly agreed by LRC in writing.

Lot 1: Heavy-Duty Backhoe Loader(s) and USAR Attachments
	LRC to Complete (BIDDERS ARE NOTE ALLOWED TO MODIFY THE LRC SECTION)
	Bidder To Complete

	Item Number
	Item/Milestone Required
	Unit of Measurements
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Total Price in USD, inclusive VAT 
	Lead time of Delivery from the date of the purchase order 

	1
	Backhoe loader – base machine
	Piece
	1
	 
	 
	 
	 

	2
	General Purpose front bucket
	Piece
	1
	 
	 
	 
	 

	3
	Rear stick bucket
	Piece
	1
	 
	 
	 
	 

	4
	Jack hammer with complete mounting/hydraulic kit
	Piece
	1
	 
	 
	 
	 

	5
	Front lifting forks – if offered
	Piece
	1
	 
	 
	 
	 

	6
	Other mandatory accessories / equipment
	Piece
	1
	 
	 
	 
	 

	6.1
	
	
	
	
	
	
	

	6.2
	
	
	
	
	
	
	

	7
	Delivery / transportation / unloading
	Piece
	1
	
	
	
	















ANNEX 3: DETAILED SPECIFICATIONS 

The specifications below describe the required performance and configuration. Equivalent equipment may be proposed provided that the proposed model fully meets or exceeds all mandatory requirements. The supplier shall identify the exact manufacturer, model, country of manufacture and model year.
The Bidder must complete all columns highlighted in red and provide the required supporting evidence for each applicable requirement.
For each requirement, the Bidder shall:
1. Complete the Supplier Response column clearly and accurately.
2. Provide the corresponding evidence/documentation requested in the Evidence column.
3. Clearly label each supporting document/evidence using the same item number as the relevant requirement (e.g., Evidence 1.1, Evidence 1.2, etc.).
4. Ensure that all submitted evidence is properly cross-referenced to the relevant requirement.
1. General Mandatory Requirements
	No.
	Requirement
	Evidence
	Supplier Response 

	1.1
	Equipment must be brand new, unused and free from defects.
	Confirm / evidence
	

	1.2
	Manufactured in India, Europe or USA.
	Country + certificate/origin evidence
	

	1.3
	Supplier shall state manufacturer, exact model, model year and serial/chassis identification method.
	Provide details
	

	1.4
	Supplier shall provide an official manufacturer technical datasheet for the offered model.
	Attach data sheet
	

	1.5
	Supplier shall complete the Technical Compliance Matrix in Section 3.
	Completed matrix
	

	1.6
	Supplier shall identify every deviation, exception or qualification against this Bid requirements.
	Deviation schedule
	

	1.7
	All quoted equipment and attachments shall be compatible with the proposed base machine and supplied ready for operation.
	Confirm
	


2. Mandatory Technical Specifications
	No.
	Component / Feature
	Required Specification
	BIDDER TO COMPLETE
Compliance / Offered Specification
	LRC TOM COMPLETE 
Compliance / Offered Specification

	2.1
	Manufacturing Origin
	Manufactured in India, Europe or USA.
	
	

	2.2
	Rear Axle / Differential Lock
	Rear axle shall offer 100% Diff-Lock for increased traction on poor ground conditions.
	
	

	2.3
	All Wheel Drive (AWD)
	AWD engaged via front console panel switch or brake pedal during all-wheel-braking operation; capable of engagement on the move, under load, in any gear, forward or reverse.
	
	

	2.4
	Brakes
	Dual brake pedals for split braking in confined working spaces.
	
	

	2.5
	Front Loader Capacity
	Minimum working load 1500kg. and the machine must have a rated lift to full height of at least 3000 kg
	
	

	2.6
	Front Bucket
	General Purpose Bucket 
	
	

	2.7
	Rear Excavator
	Digging depth greater than 5 m with extendable dipper stick; factory-certified lifting eye on bucket linkage for slinging chains/straps.
	
	

	2.8
	Hydraulic Pump
	Variable-flow, axial-piston pump.
	
	

	2.9
	Front Bucket Accessories
	All required brackets, pins, hydraulic linkage and mounting components.
	
	

	2.10
	Rear Stick Bucket Accessories
	All required brackets, pins, hydraulic linkage and mounting components.
	
	

	2.11
	Jack Hammer
	Jack hammer complete with all required mounting components, hydraulic connections and hoses/couplings.
	
	


3. Technical Performance Specifications
	No.
	Parameter
	Required / Reference Value
	BIDDERS TO COMPLETE 
Supplier Offered Value
	LRC TO COMPLETE

	3.1
	Engine type
	Mechanical turbocharged
	 
	 

	3.2
	Rated power at 2,200 rpm (Gross SAE J1995:2014)
	≈ 69.3 kW (93 hp)
	 
	 

	3.3
	Engine power ISO 14396:2002
	≈ 68.5 kW (93 hp)
	 
	 

	3.4
	Peak net power at 2,000 rpm (SAE J1349:2011)
	≈ 66.4 kW (89 hp)
	 
	 

	3.5
	Torque rise (net)
	≈ 38% at 1,200 rpm
	 
	 

	3.6
	Maximum torque
	≈ 394 N·m at 1,400 rpm
	 
	 

	3.7
	Displacement
	Minimum 4.4 L
	 
	 

	3.8
	Hydraulic Type
	Closed center
	 
	 

	3.9
	Pump capacity
	Minimum 130 L/min
	 
	 

	3.10
	System pressure (Backhoe & Loader)
	Minimum 250 bar
	 
	 

	3.11
	Transmission
	Power shuttle; 4-speed manual
	 
	 

	3.12
	Operating weight
	Estimated 8,200–8,500 kg
	 
	 

	3.13
	Maximum operating weight / ROPS capacity
	11,000 kg
	 
	 

	3.14
	Roading length
	Between 5,700 – 5,800 mm
	 
	 

	3.15
	Transportation length
	Between 5,600 – 5,700 mm
	 
	 

	3.16
	Transportation height
	Between 3,700 – 3,800 mm
	 
	 

	3.17
	Overall width
	Between 2,300 – 2,400 mm
	 
	 

	3.18
	Cab/canopy height
	Between 2,800 – 2,900 mm
	 
	 

	3.19
	Loader bucket capacity
	Minimum 1 m³
	 
	 

	3.20
	Lift capacity at maximum height
	Minimum 3,600 kg
	 
	 

	3.21
	Tipping load at breakout point
	Between 6,200 – 6,260 kg
	 
	 

	3.22
	Dump angle at full height
	Minimum 46°
	 
	 



4. Excavator Performance
	No.
	Parameter
	Standard Stick
	Extendible Stick Retracted
	Extendible Stick Extended
	BIDDERS TO COMPLETE 
Supplier Offered Value
	LRC TO COMPLETE

	4.1
	Maximum digging depth
	Between 4,110 – 4,250 mm
	Between 4,180 – 4,280 mm
	Between 5,200 – 5,250 mm
	 
	 

	4.2
	Loading height
	Between 3,900 – 3,970 mm
	Between 3,930 – 3980 mm
	Between 4,480 – 4,500 mm
	 
	 

	4.3
	Swing arc / bucket rotation
	180° / 205°
	180° / 205°
	180° / 205°
	 
	 



5. Steering, Brakes and Axles
	No.
	Feature
	Requirement
	BIDDERS TO COMPLETE 
Supplier Offered Specification
	LRC TO COMPLETE

	5.1
	Steering
	Front wheel steering; hydrostatic power steering.
	
	

	5.2
	Service brakes
	Fully enclosed boosted hydraulic multiple discs; inboard oil-immersed, self-adjusting; dual foot-operated boosted pedals.
	
	

	5.3
	Parking brake
	Mechanically applied hand lever, independent of service brake.
	
	


6. Standard and Required Equipment
	No.
	Category
	Requirement
	BIDDERS TO COMPLETE 
Status / Supplier Offer
	LRC TO COMPLETE

	6.1
	Loader safety brace
	Included.
	 
	 

	6.2
	Backhoe stick
	Included.
	 
	 

	6.3
	Backhoe transport lock – swing
	Included.
	 
	 

	6.4
	Backhoe transport lock – boom
	Included.
	 
	 

	6.5
	Hydraulic pump
	Approx. 132 L/min reference; supplier shall state actual capacity.
	 
	 

	6.6
	Hydraulic auxiliary quick disconnects
	Required for attachments where applicable; supplier shall confirm compatibility.
	 
	 

	6.7
	Side shift lock
	Electro-hydraulic; standard or equivalent.
	 
	 

	6.8
	Hydraulic oil cooler
	Included.
	 
	 

	6.9
	Loader kickout / float
	Included.
	 
	 

	6.10
	Parallel lift
	Included.
	 
	 

	6.11
	Reversing alarm
	Included.
	 
	 

	6.12
	Tires
	Front 12.5/80-18 AWD; rear 16.9-28 reference sizes or equivalent.
	 
	 

	6.13
	Transport tie-downs
	Included.
	 
	 

	6.14
	Tool storage box
	Included.
	 
	 

	6.15
	Rear license plate holder/light
	Included.
	 
	 



7. Cabin and Safety Features
The offered machine shall include the following features, with any exception clearly identified:
Beacon socket ×2
Cup holder
Differential lock button on loader control
Removable floor mat
Front and rear side-opening windows
Front headlights
Minimum six adjustable work lights
Gauge cluster
Front and rear horns
Internal power sockets ×2
Rear tail lights
Left and right opening doors
Left-hand storage console
Transmission safety lock
Mechanical suspension seat
Self-cancelling directional indicator
Front and rear window wipers
8. Supplier Technical Submission
The supplier shall submit all of the following with its quotation:
Completed Technical Compliance Matrix, with offered values and supporting references.
Official manufacturer technical datasheet for the exact proposed model.
Manufacturer, model, model year, country of manufacture and serial/chassis identification details.
Evidence of manufacturing origin.
Detailed description and datasheets for all proposed attachments.
Warranty terms and warranty coverage.
Evidence of local maintenance/service capability and spare-parts availability.
Estimated delivery lead time to Lebanon.
9. Warranty and After-Sales Support
The supplier shall provide a clear warranty covering the complete machine and supplied attachments. The quotation shall state the warranty period, commencement date, covered components, exclusions, response time and repair/replacement arrangements.
Minimum warranty period: 2 years 
Supplier shall provide local technical support and identify the service location and responsible contact.
Supplier shall state availability and expected lead time for critical spare parts.
Supplier shall state the maximum response time for warranty/service requests.
Warranty repairs and replacement parts shall be provided in accordance with the agreed warranty terms without additional cost to LRC where the defect is covered.
Supplier shall provide recommended preventive maintenance schedule and service intervals.
10. Training and Handover
The supplier shall provide practical operator familiarization and basic maintenance training at delivery, unless otherwise agreed. The supplier shall provide operating, maintenance and parts documentation in electronic format and, where available, hard copy.
11. Inspection, Testing and Acceptance
LRC reserves the right to inspect the equipment before delivery and/or upon delivery.
The supplier shall demonstrate the machine and attachments against the mandatory technical requirements.
Acceptance shall be subject to verification of the delivered model, specifications, accessories, serial/chassis identification and documentation.
Any missing, damaged, defective or non-compliant item shall be rectified/replaced by the supplier within an agreed period at no additional cost to LRC.
Payment and final acceptance shall be subject to the applicable LRC procurement and financial procedures and receipt of the required supporting documents.
12. Required Documentation at Delivery
Commercial invoice.
Delivery note.
Manufacturer certificate / certificate of origin as applicable.
Warranty certificate.
Manufacturer technical datasheet and manuals.
Parts catalogue, where available.
Maintenance/service schedule.
Serial/chassis and engine identification.
Conformity/safety certificates applicable to the offered equipment.
Any customs, import or registration documents required for delivery and use in Lebanon.
13. Supplier Qualification and Local Support
The supplier shall provide:
Company legal and registration details.
Evidence of authorization/distributorship from the manufacturer, where applicable.
Relevant experience supplying and servicing comparable heavy equipment.
Details of local workshop/service facilities and qualified technicians.
At least one relevant reference, where available.
Contact details for after-sales support.
14. Submission Checklist
	Document / Requirement
	Submitted (Yes/No)

	Completed technical compliance matrix
	

	Manufacturer technical datasheet
	

	Country of origin evidence
	

	Exact model / model year
	

	Attachment specifications
	

	Warranty terms
	

	Local after-sales/service details
	

	Spare-parts availability details
	

	Delivery lead time
	

	Supplier qualification / company documents
	

	Deviation schedule, if applicable
	

	Manufacturer authorization, if applicable
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