National tender application pack V0.3Lebanese Red Cross 

Tender reference: 2026-101
[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered.
· The contract will be awarded to the lowest-cost technically compliant complete lot or complete bid. 
· The quantities mentioned below are required unless there is a variation within a specified range with proper justification. The LRC reserves the right to increase or decrease the quantities.
· The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.  
· In the event of any discrepancy between the unit price and the total price, LRC reserves the right to rely on the unit price as stated in the financial bid, rather than the total price without go back to the supplier. The unit price must be provided with no more than two decimal places.
· Only one option is allowed for biding 
· The bidder shall price each of the three distribution-line schedules separately. All unit rates shall include labor, materials, equipment, transport, testing, permits, overheads, incidental works, and all obligations necessary for the complete execution and handover of the works.
LOT 1:  OMAR AL FAROKH SCHOOL -CERD: 40 - BEIRUT
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1.1
	Demolition
	LS
	1
	 
	 
	 
	 

	1.2
	Concrete block wall — 12 cm
	m²
	4
	 
	 
	 
	 

	1.3
	Internal Plastering
	m²
	70
	 
	 
	 
	 

	1.4
	Floor tiles (anti-slip ceramic)
	m²
	6
	 
	 
	 
	 

	1.5
	Wall tiles 20×60
	m²
	55
	 
	 
	 
	 

	1.6
	Ceiling & wall paint (with putty)
	m²
	15
	 
	 
	 
	 

	1.7
	Wooden door with frame (approx. 0.90 × 2.10 m)
	No.
	4
	 
	 
	 
	 

	1.8
	Soap dispenser
	No.
	3
	 
	 
	 
	 

	1.9
	Mirror
	No.
	3
	 
	 
	 
	 

	1.10
	Toilet paper holder
	No.
	1
	 
	 
	 
	 

	1.11
	Plexi sign board — wall-fixed (600 × 400 mm)
	No.
	4
	 
	 
	 
	 

	1.12
	Shelf under mirror
	No.
	2
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	1.13
	Lighting point — concealed (LED 40 W)
	No.
	7
	 
	 
	 
	 

	1.14
	Toilet exhaust fan
	No.
	4
	 
	 
	 
	 

	1.16
	Circuit breaker box (6-way, double-pole devices)
	No.
	3
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	1.16
	Wall-hung WC
	No.
	1
	 
	 
	 
	 

	1.17
	Hand-held bidet (shattaf)
	No.
	1
	 
	 
	 
	 

	1.18
	Sanitary napkin pedal bin (MHM)
	No.
	1
	 
	 
	 
	 

	1.19
	Paper-towel dispenser
	No.
	3
	 
	 
	 
	 

	1.20
	Kitchen sink – granite (with cabinet)
	No.
	3
	 
	 
	 
	 

	1.21
	Wash basin – granite round 50 cm (supply & install only)
	No.
	3
	 
	 
	 
	 

	1.22
	Water mixer – wash basin / sink
	No.
	3
	 
	 
	 
	 

	1.23
	Short push/self-close tap (basin)
	No.
	3
	 
	 
	 
	 

	1.24
	Stainless-steel P-trap
	No.
	3
	 
	 
	 
	 

	1.25
	PPR pipe ½″ (concealed)
	m
	20
	 
	 
	 
	 

	1.26
	PVC pipe 2″
	m
	14
	 
	 
	 
	 

	1.27
	Floor drain 15×15 (stainless)
	No.
	3
	 
	 
	 
	 

	1.28
	Cleanout 20×20 (stainless)
	No.
	2
	 
	 
	 
	 

	1.29
	Toilet ventilation (in-line duct fan)
	No.
	4
	 
	 
	 
	 

	1.30
	Pressure test
	LS
	2
	 
	 
	 
	 

	1.31
	Flow switch
	No.
	1
	 
	 
	 
	 

	
	Total Amount including VAT for Lot 1
	
	
	
	
	
	

	
	Lead time of Delivery 
	
	
	
	
	
	









LOT 2:  RAWDAT ABI HAIDAR SCHOOL- CERD: 20 – BEIRUT
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1.1
	RC slab — 25 MPa (T14, 125 kg/m³)
	m³
	2
	 
	 
	 
	 

	1.2
	Demolition
	Ls
	1
	 
	 
	 
	 

	1.3
	Excavation & Backfilling
	m3
	6
	 
	 
	 
	 

	1.4
	Sewer / drainage network jetting per manhole run
	U
	1
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.5
	Asphalt layer (new subbase + base + asphalt)
	m3
	5
	 
	 
	 
	 

	1.6
	Subbase material
	m3
	10
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.7
	PVC pipe 6″
	m
	12
	 
	 
	 
	 

	1.8
	Manhole 100×100×120 cm
	No.
	2
	 
	 
	 
	 

	
	Total Amount including VAT for Lot 2
	
	
	
	
	

	
	Lead time of Delivery
	
	
	
	
	








LOT 3:  MARJ EL ZOHOR SCHOOL -CERD: 1187 - HASBAYA
	LRC To Complete
	Bidder To Complete
	 

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1.1
	DEMOLITION
	m²
	100
	 
	 
	 
	 

	1.2
	Concrete block wall — 12 cm
	m²
	10
	 
	 
	 
	 

	1.3
	Internal Plastering
	m²
	130
	 
	 
	 
	 

	1.4
	Floor tiles (anti-slip ceramic)
	m²
	35
	 
	 
	 
	 

	1.5
	Wall tiles 20×60
	m²
	70
	 
	 
	 
	 

	1.6
	Ceiling & wall paint (with putty)
	m²
	35
	 
	 
	 
	 

	1.7
	Wooden door (with frame)
	No.
	5
	 
	 
	 
	 

	1.8
	Steel window — full repair (all hardware)
	No.
	6
	 
	 
	 
	 

	1.9
	Soap dispenser
	No.
	3
	 
	 
	 
	 

	1.10
	Mirror
	No.
	3
	 
	 
	 
	 

	1.11
	Toilet paper holder
	No.
	4
	 
	 
	 
	 

	1.12
	Plexi sign board — wall-fixed (600 × 400 mm)
	No.
	2
	 
	 
	 
	 

	1.13
	Shelf under mirror
	No.
	3
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.14
	Lighting point — concealed (LED 40 W)
	No.
	10
	 
	 
	 
	 

	1.15
	Toilet exhaust fan
	No.
	4
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.16
	Western sitting WC (porcelain)
	No.
	4
	 
	 
	 
	 

	1.17
	Hand-held bidet (shattaf)
	No.
	4
	 
	 
	 
	 

	1.18
	Paper-towel dispenser
	No.
	4
	 
	 
	 
	 

	1.19
	Kitchen sink – granite (with cabinet)
	No.
	1
	 
	 
	 
	 

	1.2
	Wash basin – ceramic (supply & install only)
	No.
	3
	 
	 
	 
	 

	1.21
	Water mixer – wash basin / sink
	No.
	1
	 
	 
	 
	 

	1.22
	Water mixer – shower
	No.
	2
	 
	 
	 
	 

	1.23
	Short push/self-close tap (basin)
	No.
	3
	 
	 
	 
	 

	1.24
	PPR pipe 1″ (concealed)
	m
	20
	 
	 
	 
	 

	1.25
	PPR pipe ½″ (concealed)
	m
	30
	 
	 
	 
	 

	1.26
	PVC pipe 2″
	m
	20
	 
	 
	 
	 

	1.27
	PVC pipe 4″
	m
	20
	 
	 
	 
	 

	1.28
	PEX pipe ½″ (16 mm) — concealed
	m
	10
	 
	 
	 
	 

	1.29
	Floor drain 15×15 (stainless)
	No.
	7
	 
	 
	 
	 

	1.30
	Cleanout 20×20 (stainless)
	No.
	2
	 
	 
	 
	 

	1.31
	Manhole 60×60×100 cm
	No.
	1
	 
	 
	 
	 

	1.32
	Gas water heater (instantaneous, LPG) — with flue
	No.
	1
	 
	 
	 
	 

	1.33
	Gas jar (LPG cylinder) for gas water heater — any capacity, measured per kg
	kg
	12
	 
	 
	 
	 

	1.34-
	Flow switch
	No.
	2
	 
	 
	 
	 

	1.35
	Pressure test
	LS
	2
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.36
	Water tank 2000 L (PE, 3-layer)
	No.
	2
	 
	 
	 
	 

	 
	Total Amount including VAT for Lot 3
	 
	 
	 
	 
	 
	 

	
	Lead time of Delivery
	
	
	
	
	
	





LOT 4:  AKKAR SHELTERS / SCHOOLS- PUBLIC BUILDINGS- MUNICIPALITY
	LRC To Complete
	Bidder To Complete

	Item number 
	Item/Milestone Required
	Required UOM
	Estimated Qty
	Unit Price in USD, Exclusive VAT 
	VAT (%)
	Unit Price in USD, inclusive VAT 
	Total Price in USD, inclusive VAT 

	1.1
	DEMOLITION
	Unit
	3
	 
	 
	 
	 

	1.2
	Wooden door — full repair (all components)
	No.
	20
	 
	 
	 
	 

	1.3
	European lock + handle
	No.
	10
	 
	 
	 
	 

	1.4
	New steel window (approx. 1.20 × 1.00 m)
	No.
	5
	 
	 
	 
	 

	1.5
	Steel window — full repair (all hardware)
	No.
	10
	 
	 
	 
	 

	1.6
	Aluminum door/window — full repair (all hardware)
	No.
	20
	 
	 
	 
	 

	1.7
	Soap dispenser
	No.
	15
	 
	 
	 
	 

	1.8
	Mirror
	No.
	10
	 
	 
	 
	 

	1.9
	Toilet paper holder
	No.
	30
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.1
	Lighting point — concealed (LED 40 W)
	No.
	20
	 
	 
	 
	 

	1.11
	Solar water boiler 300 L — thermal collector type
	No.
	2
	 
	 
	 
	 

	1.12
	Toilet exhaust fan
	No.
	20
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.13
	Western sitting WC (porcelain)
	No.
	10
	 
	 
	 
	 

	1.14
	Repair Western (floor-standing) WC — complete with all accessories
	No.
	20
	 
	 
	 
	 

	1.15
	Hand-held bidet (shattaf)
	No.
	30
	 
	 
	 
	 

	1.16
	Repair single-basin sink — complete with P-trap, tap and all accessories
	No.
	20
	 
	 
	 
	 

	1.17
	Wash basin – ceramic (supply & install only)
	No.
	10
	 
	 
	 
	 

	1.18
	Short push/self-close tap (basin)
	No.
	10
	 
	 
	 
	 

	1.19
	PPR pipe 1″ (concealed)
	m
	80
	 
	 
	 
	 

	1.2
	PPR pipe ½″ (concealed)
	m
	20
	 
	 
	 
	 

	1.21
	Floor drain 15×15 (stainless)
	No.
	10
	 
	 
	 
	 

	1.22
	Cleanout 20×20 (stainless)
	No.
	10
	 
	 
	 
	 

	1.23
	Flow switch
	No.
	13
	 
	 
	 
	 

	1.24
	Pressure test
	LS
	10
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 

	1.25
	Water tank 2000 L (PE, 3-layer)
	No.
	10
	 
	 
	 
	 

	1.26
	Water pump ¾ HP (SS)
	No.
	3
	 
	 
	 
	 

	
	Total Amount including VAT for Lot 4
	
	
	
	
	
	

	
	Lead time of Delivery
	
	
	
	
	
	













ANNEX 3: DETAILED SPECIFICATIONS 

As per: 2026-101Terms of Reference

LOT 1:  OMAR AL FAROKH SCHOOL -CERD: 40 - BEIRUT	
	Item No.
	Item Code
	BIM / MasterFormat
	Item / Title
	Standard
	Description (English)
	Type
	Loc.

	1.1
	SW-1.01
	02 41 (Demolition)
	Demolition
	 
	Supply, install, test and hand over Demolition. The works include all cutting, breaking-out and dismantling, loading, haulage and legal disposal of debris at an approved dump, and protection of adjacent works. Priced as a lump sum for the complete works.
	demoliton
	both

	1.2
	AR-2.02
	04 22 (Concrete unit masonry)
	Concrete block wall — 12 cm
	EN 771-3
	Supply, install, test and hand over Concrete block wall — 12 cm. The works include laying blocks in 1:4 sand-cement mortar, reinforcement and ties as required, and a plumb, level finish. Measured per square metre of completed work.
	Supply & Install
	Both

	1.3
	AR-4.02
	09 24 (Cement plaster)
	Internal Plastering
	EN 998-1
	Supply, install, test and hand over Internal Plastering. The works include removal of loose material, a rush/key coat then two coats of 1:4 mortar (350 kg cement/m³) to 20 mm, and scaffolding as needed. Measured per square metre of completed work.
	Supply & Install
	Interior

	1.4
	AR-5.02
	09 30 (Tiling)
	Floor tiles (anti-slip ceramic)
	EN 14411
	Supply, install, test and hand over Floor tiles (anti-slip ceramic). The works include substrate preparation, sand/mortar or adhesive bedding, cross spacers, grouting, PVC edge/coving trims, silicone sealing and slope to floor drains. Measured per square metre of completed work.
	Supply & Install
	Both

	1.5
	AR-5.03
	09 30 (Tiling)
	Wall tiles 20×60
	EN 14411
	Supply, install, test and hand over Wall tiles 20×60. The works include substrate preparation, sand/mortar or adhesive bedding, cross spacers, grouting, PVC edge/coving trims, silicone sealing and slope to floor drains. Measured per square metre of completed work.
	Supply & Install
	Both

	1.6
	AR-6.01
	09 91 (Painting)
	Ceiling & wall paint (with putty)
	EN 13300
	Supply, install, test and hand over Ceiling & wall paint (with putty). The works comprise: surface preparation — removal of loose or flaking material, scraping and sanding; ONE coat of alkali-resistant primer/sealer; TWO coats of putty (skim filler) applied and rubbed down between coats to a true, smooth surface; and TWO finishing coats of emulsion paint in the approved colour — i.e. FIVE applied coats in total (1 primer + 2 putty + 2 finish). Includes cutting in, protection of floors, joinery and fittings, scaffolding, and cleaning on completion. Measured per square metre of completed work.
	Supply & Install
	Both

	1.7
	AR-8.01
	08 14 (Wood doors)
	Wooden door with frame (approx. 0.90 × 2.10 m)
	EN 14351-1
	Supply, install, test and hand over a wooden door complete with frame, approximate leaf size 0.90 × 2.10 m × 45 mm thick — exact dimensions to be confirmed from site survey before fabrication. The works include a flush plywood/beech-framed leaf faced as specified, a galvanised or hardwood frame 100 × 50 mm anchored to the wall, architraves both sides, three hinges, mortice lockset and lever handles, door stop and threshold, and preparation for painting. Measured per unit, complete and serviceable; where the actual size differs from the stated approximate size by more than 15%, the rate is to be adjusted pro rata on area.
	Supply & Install
	Interior

	1.8
	AR-11.02
	10 28 (Toilet accessories)
	Soap dispenser
	ISO 21542
	Supply, install, test and hand over Soap dispenser. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.9
	AR-11.03
	10 28 (Toilet accessories)
	Mirror
	ISO 21542
	Supply, install, test and hand over Mirror. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.10
	AR-11.04
	10 28 (Toilet accessories)
	Toilet paper holder
	ISO 21542
	Supply, install, test and hand over Toilet paper holder. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.11
	AR-11.06
	10 14 (Signage)
	Plexi sign board — wall-fixed (600 × 400 mm)
	ISO 7010
	Supply, install, test and hand over a wall-fixed plexiglass (acrylic) sign board, nominal face size 600 × 400 mm × 5 mm thick, with UV-stable printed or engraved graphics to the approved design. The works include stainless-steel standoff fixings at four corners, wall plugs and anchors suitable for the substrate, protective film removal and cleaning on completion, and setting out at the approved height. No post or concrete base is required. A sample and artwork proof are to be approved before manufacture. Measured per unit, complete and serviceable.
	Supply & Install
	Both

	1.12
	AR-11.08
	10 28 (Toilet accessories)
	Shelf under mirror
	ISO 21542
	Supply, install, test and hand over Shelf under mirror. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	 
	 

	1.13
	EL-2.01
	26 51 (Interior lighting)
	Lighting point — concealed (LED 40 W)
	EN 12464-1 / EN 60598
	Supply, install, test and hand over Lighting point — concealed (LED 40 W). The works include luminaire, wiring, back-box, switch and socket, and all items for a complete working point. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.14
	EL-3.03
	23 34 (Fans)
	Toilet exhaust fan
	EN 13141
	Supply, install, test and hand over Toilet exhaust fan. The works include wiring, conduit, protection and ducting connection, tested and commissioned. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.16
	EL-3.04
	26 24 (Panelboards)
	Circuit breaker box (6-way, double-pole devices)
	IEC 61439
	Supply, install, test and hand over a 6-way circuit breaker box. The works include the enclosure and appropriately-rated breakers, wired, labelled and tested. ALL protective devices on single-phase circuits shall be DOUBLE-POLE (2P), switching both line and neutral, in accordance with the project standard for this section; single-pole devices are not acceptable. Measured per unit, complete and serviceable.
	Supply & Install
	Both

	 
	 

	1.16
	PL-1.03
	22 42 (Fixtures)
	Wall-hung WC
	EN 997 / EN 14688
	Supply, install, test and hand over Wall-hung WC. The works include triangle chrome stop valve, cistern and complete flush system, seat cover, concealed PPR water and PVC waste connections, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.17
	PL-1.04
	22 42 (Fixtures)
	Hand-held bidet (shattaf)
	EN 997 / EN 14688
	Supply, install, test and hand over Hand-held bidet (shattaf). The works include triangle chrome stop valve, cistern and complete flush system, seat cover, concealed PPR water and PVC waste connections, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.18
	PL-1.15
	10 28 (MHM)
	Sanitary napkin pedal bin (MHM)
	—
	Supply and install a lidded pedal-operated sanitary-waste bin in each female/accessible cubicle for menstrual-hygiene waste.
	Supply & Install
	Interior

	1.19
	PL-1.17
	10 28 (Hygiene)
	Paper-towel dispenser
	—
	Supply and install a wall-mounted paper-towel dispenser with fixings.
	Supply & Install
	Interior

	1.20
	PL-2.01
	22 42 (Sinks)
	Kitchen sink – granite (with cabinet)
	EN 997 / EN 14688
	Supply, install, test and hand over Kitchen sink – granite (with cabinet). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.21
	PL-2.04
	22 42 (Sinks)
	Wash basin – granite round 50 cm (supply & install only)
	EN 997 / EN 14688
	Supply and install one wall-mounted round granite wash basin (50 cm, European), including brackets and fixing only. Mixer, trap and connections priced separately.
	Component
	Interior

	1.22
	PL-3.01
	22 42 (Trim)
	Water mixer – wash basin / sink
	EN 997 / EN 14688
	Supply, install, test and hand over Water mixer – wash basin / sink. The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.23
	PL-3.04
	22 42 (Trim)
	Short push/self-close tap (basin)
	EN 997 / EN 14688
	Supply and install Short push/self-close tap (basin). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Component
	Interior

	1.24
	PL-5.04
	22 42 (Components)
	Stainless-steel P-trap
	EN 997 / EN 14688
	Supply and install Stainless-steel P-trap. The works include all fixings, sealing and connections to leave the part complete and serviceable. Measured per unit, complete and serviceable.
	Component
	Interior

	1.25
	PL-7.01
	22 11 (Water pipe)
	PPR pipe ½″ (concealed)
	EN ISO 15874 / EN 809
	Supply, install, test and hand over PPR pipe ½″ (concealed). The works include breaking/chasing and re-concreting after approval, foam thermal insulation on exposed runs, copper connections, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both

	1.26
	PL-7.04
	22 13 (Drain pipe)
	PVC pipe 2″
	EN 1401 / EN 1329
	Supply, install, test and hand over PVC pipe 2″. The works include breaking/chasing and re-concreting after approval, ventilation piping, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both

	1.27
	PL-8.05
	22 13 (Floor drains)
	Floor drain 15×15 (stainless)
	EN 1401 / EN 1329
	Supply, install, test and hand over Floor drain 15×15 (stainless). The works include secure, watertight and corrosion-resistant fixing to the drainage line. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.28
	PL-8.04
	22 13 (Cleanouts)
	Cleanout 20×20 (stainless)
	EN 1401 / EN 1329
	Supply, install, test and hand over Cleanout 20×20 (stainless). The works include secure, watertight and corrosion-resistant fixing to the drainage line. Measured per unit, complete and serviceable.
	Supply & Install
	Both

	1.29
	PL-10.01
	23 34 (Fans)
	Toilet ventilation (in-line duct fan)
	EN 13141
	Supply, install, test and hand over Toilet ventilation (in-line duct fan). The works include ductwork and flexible connections, dampers, isolators, control wiring, and testing and commissioning. Measured per unit, complete and serviceable.
	Supply & Install
	Interior

	1.30
	PL-10.02
	22 08 (Commissioning)
	Pressure test
	EN 806-4
	Carry out Pressure test. The works include pressurising the system, checking all joints for leaks and issuing results. Priced as a lump sum for the complete works.
	Service
	Both

	1.31
	PL-3.06
	22 05 (Valves)
	Flow switch
	EN 200 / EN 817
	Supply, install, test and hand over Flow switch. The works include concealed hot/cold PPR connections, flexible tails, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Both





















LOT 2:  RAWDAT ABI HAIDAR SCHOOL- CERD: 20 – BEIRUT
	Item No
	Item Code
	BIM / MasterFormat
	Item / Title
	Standard
	Description (English)
	Type
	Loc.
	Unit

	1.1
	AR-1.01
	03 30 (Cast-in-place conc.)
	RC slab — 25 MPa (T14, 125 kg/m³)
	EN 206 / ACI 318
	Supply, install, test and hand over RC slab — 25 MPa (T14, 125 kg/m³). The works include sulphate-resisting cement adjacent to soil, plywood formwork for a fair-faced finish, ribbed reinforcement, mechanical vibration and curing. Measured per cubic metre in place.
	Supply & Install
	Both
	m³

	1.2
	SW-1.01
	02 41 (Demolition)
	Demolition
	—
	Supply, install, test and hand over Demolition. The works include all cutting, breaking-out and dismantling, loading, haulage and legal disposal of debris at an approved dump, and protection of adjacent works. Priced as a lump sum for the complete works.
	Demolition
	Both
	Ls

	1.3
	SW-1.02 / SW-1.03
	31 20 (Earthwork)
	Excavation & Backfilling
	—
	Supply, execute, test and hand over Excavation works. The works include setting out, excavation in any material to the required lines and levels, shoring/sheet piling and dewatering as required, trimming and levelling of the formation, temporary protection of the open excavation, and loading, haulage and legal disposal of surplus excavated material at an approved dump. Backfilling is measured separately under SW-1.03. Measured per cubic metre of excavation in place.  Backfilling: Supply, execute, test and hand over Backfilling works. The works include supply of approved granular backfill material (or re-use of selected excavated material where approved), bedding and surround to services, placing and compaction in layers not exceeding 200 mm to 95–98% MDD, watering as required, field density testing, and making good to the existing surface level. Excavation is measured separately under SW-1.02. Measured per cubic metre of compacted backfill in place.
	Supply & Install
	Both
	m3

	1.4
	SW-1.09
	33 01 (Sewer cleaning)
	Sewer / drainage network jetting per manhole run
	—
	High-pressure jetting and unblocking of sewer/drainage line between two manholes, including rodding and flushing.
	Service
	Both
	U

	 
	 

	1.5
	SW-2.02
	32 12 (Flexible paving)
	Asphalt layer (new subbase + base + asphalt)
	EN 13108
	Supply, install, test and hand over Asphalt layer (new subbase + base + asphalt). The works include sub-base and base preparation, prime/tack coat, laying and compaction to 5 cm after rolling, and reinstatement to match existing. Measured per square metre of completed work.
	Supply & Install
	Exterior
	m3

	1.6
	SW-2.04
	32 11 (Base course)
	Subbase material
	EN 13285
	Supply, install, test and hand over Subbase material. The works include supply, spreading, grading to line and level, watering and compaction, and all required tests. Measured per square metre of completed work.
	Supply & Install
	Exterior
	m3

	 
	 

	1.7
	PL-7.06
	22 13 (Drain pipe)
	PVC pipe 6″
	EN 1401 / EN 1329
	Supply, install, test and hand over PVC pipe 6″. The works include breaking/chasing and re-concreting after approval, ventilation piping, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.8
	PL-8.03
	33 44 (Manholes)
	Manhole 100×100×120 cm
	EN 476
	Supply, install, test and hand over Manhole 100×100×120 cm. The works include block construction with concrete cover and medium-duty steel lid, and internal plastering. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.












LOT 3:  MARJ EL ZOHOR SCHOOL -CERD: 1187 - HASBAYA
	Item No
	Item Code
	BIM / MasterFormat
	Item / Title
	Standard
	Description (English)
	Type
	Loc.
	Unit

	1.1
	SW-1.01
	Demolition
	DEMOLITION
	 
	Supply, install, test and hand over Demolition. The works include all cutting, breaking-out and dismantling, loading, haulage and legal disposal of debris at an approved dump, and protection of adjacent works. Priced as a lump sum for the complete works.
	demoliton
	both
	m²

	1.2
	AR-2.02
	04 22 (Concrete unit masonry)
	Concrete block wall — 12 cm
	EN 771-3
	Supply, install, test and hand over Concrete block wall — 12 cm. The works include laying blocks in 1:4 sand-cement mortar, reinforcement and ties as required, and a plumb, level finish. Measured per square metre of completed work.
	Supply & Install
	Both
	m²

	1.3
	AR-4.02
	09 24 (Cement plaster)
	Internal Plastering
	EN 998-1
	Supply, install, test and hand over Internal Plastering. The works include removal of loose material, a rush/key coat then two coats of 1:4 mortar (350 kg cement/m³) to 20 mm, and scaffolding as needed. Measured per square metre of completed work.
	Supply & Install
	Interior
	m²

	1.4
	AR-5.02
	09 30 (Tiling)
	Floor tiles (anti-slip ceramic)
	EN 14411
	Supply, install, test and hand over Floor tiles (anti-slip ceramic). The works include substrate preparation, sand/mortar or adhesive bedding, cross spacers, grouting, PVC edge/coving trims, silicone sealing and slope to floor drains. Measured per square metre of completed work.
	Supply & Install
	Both
	m²

	1.5
	AR-5.03
	09 30 (Tiling)
	Wall tiles 20×60
	EN 14411
	Supply, install, test and hand over Wall tiles 20×60. The works include substrate preparation, sand/mortar or adhesive bedding, cross spacers, grouting, PVC edge/coving trims, silicone sealing and slope to floor drains. Measured per square metre of completed work.
	Supply & Install
	Both
	m²

	1.6
	AR-6.01
	09 91 (Painting)
	Ceiling & wall paint (with putty)
	EN 13300
	Supply, install, test and hand over Ceiling & wall paint (with putty). The works comprise: surface preparation — removal of loose or flaking material, scraping and sanding; ONE coat of alkali-resistant primer/sealer; TWO coats of putty (skim filler) applied and rubbed down between coats to a true, smooth surface; and TWO finishing coats of emulsion paint in the approved colour — i.e. FIVE applied coats in total (1 primer + 2 putty + 2 finish). Includes cutting in, protection of floors, joinery and fittings, scaffolding, and cleaning on completion. Measured per square metre of completed work.
	Supply & Install
	Both
	m²

	1.7
	AR-8.01
	08 14 (Wood doors)
	Wooden door (with frame)
	EN 14351-1
	Supply, install, test and hand over a wooden door complete with frame, approximate leaf size 0.80 × 2.00 m × 45 mm thick — exact dimensions to be confirmed from site survey before fabrication. The works include a flush plywood/beech-framed leaf faced as specified, a galvanised or hardwood frame 100 × 50 mm anchored to the wall, architraves both sides, three hinges, mortice lockset and lever handles, door stop and threshold, and preparation for painting. Measured per unit, complete and serviceable; where the actual size differs from the stated approximate size by more than 15%, the rate is to be adjusted pro rata on area.
	Supply & Install
	Interior
	No.

	1.8
	AR-10.04
	08 01 (Repair)
	Steel window — full repair (all hardware)
	EN 14351-1
	Full overhaul repair of a steel window: straighten/reweld frame and sash, replace hinges/handles/locks, treat corrosion, prime and repaint, reglaze as needed. Components itemised separately in AR-12.
	Repair
	Both
	No.

	1.9
	AR-11.02
	10 28 (Toilet accessories)
	Soap dispenser
	ISO 21542
	Supply, install, test and hand over Soap dispenser. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.10
	AR-11.03
	10 28 (Toilet accessories)
	Mirror
	ISO 21542
	Supply, install, test and hand over Mirror. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.11
	AR-11.04
	10 28 (Toilet accessories)
	Toilet paper holder
	ISO 21542
	Supply, install, test and hand over Toilet paper holder. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.12
	AR-11.05
	10 14 (Signage)
	Plexi sign board — wall-fixed (600 × 400 mm)
	ISO 7010
	Supply, install, test and hand over a wall-fixed plexiglass (acrylic) sign board, nominal face size 600 × 400 mm × 5 mm thick, with UV-stable printed or engraved graphics to the approved design. The works include stainless-steel standoff fixings at four corners, wall plugs and anchors suitable for the substrate, protective film removal and cleaning on completion, and setting out at the approved height. No post or concrete base is required. A sample and artwork proof are to be approved before manufacture. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.13
	AR-11.06
	10 28 (Toilet accessories)
	Shelf under mirror
	ISO 21542
	Supply, install, test and hand over Shelf under mirror. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	 
	 

	1.14
	EL-2.01
	26 51 (Interior lighting)
	Lighting point — concealed (LED 40 W)
	EN 12464-1 / EN 60598
	Supply, install, test and hand over Lighting point — concealed (LED 40 W). The works include luminaire, wiring, back-box, switch and socket, and all items for a complete working point. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.15
	EL-3.03
	23 34 (Fans)
	Toilet exhaust fan
	EN 13141
	Supply, install, test and hand over Toilet exhaust fan. The works include wiring, conduit, protection and ducting connection, tested and commissioned. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	 
	 

	1.16
	PL-1.02
	22 42 (Fixtures)
	Western sitting WC (porcelain)
	EN 997 / EN 14688
	Supply, install, test and hand over Western sitting WC (porcelain). The works include triangle chrome stop valve, cistern and complete flush system, seat cover, concealed PPR water and PVC waste connections, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.17
	PL-1.04
	22 42 (Fixtures)
	Hand-held bidet (shattaf)
	EN 997 / EN 14688
	Supply, install, test and hand over Hand-held bidet (shattaf). The works include triangle chrome stop valve, cistern and complete flush system, seat cover, concealed PPR water and PVC waste connections, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.18
	PL-1.17
	10 28 (Hygiene)
	Paper-towel dispenser
	—
	Supply and install a wall-mounted paper-towel dispenser with fixings.
	Supply & Install
	Interior
	No.

	1.19
	PL-2.01
	22 42 (Sinks)
	Kitchen sink – granite (with cabinet)
	EN 997 / EN 14688
	Supply, install, test and hand over Kitchen sink – granite (with cabinet). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.2
	PL-2.03
	22 42 (Sinks)
	Wash basin – ceramic (supply & install only)
	EN 997 / EN 14688
	Supply and install Wash basin – ceramic (supply & install only). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Component
	Interior
	No.

	1.21
	PL-3.01
	22 42 (Trim)
	Water mixer – wash basin / sink
	EN 997 / EN 14688
	Supply, install, test and hand over Water mixer – wash basin / sink. The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.22
	PL-3.02
	22 42 (Trim)
	Water mixer – shower
	EN 997 / EN 14688
	Supply, install, test and hand over a shower mixer VALVE ONLY. This item covers the mixing valve/tap body and its escutcheon; the shower head, riser rail, flexible hose and wall bracket are NOT included — for a complete shower assembly use PL-3.03. The works include concealed hot/cold PPR connections, flexible tails, sealing, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.23
	PL-3.03
	22 42 (Trim)
	Short push/self-close tap (basin)
	EN 997 / EN 14688
	Supply and install Short push/self-close tap (basin). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Component
	Interior
	No.

	1.24
	PL-7.03
	22 11 (Water pipe)
	PPR pipe 1″ (concealed)
	EN ISO 15874 / EN 809
	Supply, install, test and hand over PPR pipe 1″ (concealed). The works include breaking/chasing and re-concreting after approval, foam thermal insulation on exposed runs, copper connections, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.25
	PL-7.01
	22 11 (Water pipe)
	PPR pipe ½″ (concealed)
	EN ISO 15874 / EN 809
	Supply, install, test and hand over PPR pipe ½″ (concealed). The works include breaking/chasing and re-concreting after approval, foam thermal insulation on exposed runs, copper connections, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.26
	PL-7.04
	22 13 (Drain pipe)
	PVC pipe 2″
	EN 1401 / EN 1329
	Supply, install, test and hand over PVC pipe 2″. The works include breaking/chasing and re-concreting after approval, ventilation piping, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.27
	PL-7.05
	22 13 (Drain pipe)
	PVC pipe 4″
	EN 1401 / EN 1329
	Supply, install, test and hand over PVC pipe 4″. The works include breaking/chasing and re-concreting after approval, ventilation piping, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.28
	PL-7.09
	22 11 (Water pipe)
	PEX pipe ½″ (16 mm) — concealed
	EN ISO 15875
	Supply, install, test and hand over cross-linked polyethylene (PEX) water pipe, size ½″ (16 mm), PN10 rated for hot and cold potable water, with an oxygen barrier where connected to a heating circuit. The works include chasing/breaking and re-concreting after approval, laying in protective conduit where concealed in screed or slab, foam thermal insulation on exposed runs, press or compression fittings of the same manufacturer's system, brass manifolds and transition couplings to PPR or copper where required, fixing clips at the specified centres, and pressure testing. Measured per linear metre of pipe installed, fittings deemed included.
	Supply & Install
	Both
	m

	1.29
	PL-8.05
	22 13 (Floor drains)
	Floor drain 15×15 (stainless)
	EN 1401 / EN 1329
	Supply, install, test and hand over Floor drain 15×15 (stainless). The works include secure, watertight and corrosion-resistant fixing to the drainage line. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.30
	PL-8.04
	22 13 (Cleanouts)
	Cleanout 20×20 (stainless)
	EN 1401 / EN 1329
	Supply, install, test and hand over Cleanout 20×20 (stainless). The works include secure, watertight and corrosion-resistant fixing to the drainage line. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.31
	PL-8.03
	33 44 (Manholes)
	Manhole 60×60×100 cm
	EN 476
	Supply, install, test and hand over Manhole 60×60×100 cm. The works include block construction with concrete cover and medium-duty steel lid, and internal plastering. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.32
	PL-9.03
	22 33 (Water heaters — gas)
	Gas water heater (instantaneous, LPG) — with flue
	EN 26 / EN 30 / EN 1949
	Supply, install, test and hand over an LPG gas water heater. The works include a room-sealed or forced-draught (Type C / fan-flued) instantaneous gas water heater of 10–16 L/min output, with electronic ignition, flame-failure safety device, anti-frost and over-temperature protection; a stainless-steel flue with terminal, wall sleeve and weatherproofing discharging to open air; an LPG regulator, approved flexible or copper gas line with a manual shut-off valve and a leak test on completion; hot and cold water connections with isolating valves and a pressure-relief valve; electrical supply where required; and permanent room ventilation openings to the gas-appliance regulations. Open-flue heaters are NOT permitted in bathrooms or unventilated rooms. Commissioning, combustion check and user handover instruction are included. Gas cylinders are excluded. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.33
	PL-9.04
	23 11 (Fuel gas storage)
	Gas jar (LPG cylinder) for gas water heater — any capacity, measured per kg
	EN 1442 / ISO 4706 / EN 16129
	Supply and place a refillable LPG gas jar (gas cylinder) to serve the gas water heater under PL-9.03, complete with its first fill of gas. The cylinder shall be a certified, in-date steel LPG cylinder to EN 1442 / ISO 4706 bearing a legible manufacture and re-test date stamp, fitted with a compliant self-closing valve and protective cap, free of corrosion, dents or weld defects, and hydrostatically re-tested within the required interval. The works include delivery to site, a levelled and ventilated standing position outdoors or in a ventilated cylinder cabinet, a wall chain or strap restraint to prevent toppling, a compatible pressure regulator and approved hose or copper connection with a manual shut-off valve, a leak test with soap solution or a gas detector on completion, and hazard labelling. Storage location must comply with the gas-appliance regulations: not inside bathrooms, stairwells, basements or unventilated rooms, and clear of drains, heat sources and electrical equipment. THIS ITEM IS MEASURED PER KILOGRAM OF NOMINAL GAS CAPACITY, so that any cylinder size can be priced from a single rate — for example a 10 kg jar is measured as 10, a 12.5 kg jar as 12.5, and a 35 kg commercial jar as 35. Enter the total kg required across all cylinders in the quantity column. Subsequent gas refills during operation are excluded and are not part of this contract.
	Supply & Install
	Exterior
	kg

	1.34
	PL-3.06
	22 05 (Valves)
	Flow switch
	EN 200 / EN 817
	Supply, install, test and hand over Flow switch. The works include concealed hot/cold PPR connections, flexible tails, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.35
	PL-10.02
	22 08 (Commissioning)
	Pressure test
	EN 806-4
	Carry out Pressure test. The works include pressurising the system, checking all joints for leaks and issuing results. Priced as a lump sum for the complete works.
	Service
	Both
	LS

	 
	PW-1  WATER STORAGE TANKS

	1.36
	PW-1.03
	22 12 (Water tanks)
	Water tank 2000 L (PE, 3-layer)
	EN 12573
	Supply, install, test and hand over Water tank 2000 L (PE, 3-layer). The works include 3-layer polyethylene tank, all supply/outlet accessories and European valves for inlet and outlet. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.















LOT 4:  AKKAR SHELTERS / SCHOOLS- PUBLIC BUILDINGS- MUNICIPALITY
	Item No
	Item Code
	BIM / MasterFormat
	Item / Title
	Standard
	Description (English)
	Type
	Loc.
	Unit

	1.1
	SW-1.01
	Demolition
	DEMOLITION
	 
	Supply, install, test and hand over Demolition. The works include all cutting, breaking-out and dismantling, loading, haulage and legal disposal of debris at an approved dump, and protection of adjacent works. Priced as a lump sum for the complete works.
	demoliton
	both
	Unit

	1.2
	AR-8.03
	08 01 (Repair)
	Wooden door — full repair (all components)
	EN 14351-1
	Full overhaul repair of a wooden door: refix/replace leaf panels and beadings, renew frame joints, replace hinges, lock and handle, apply putty and prepare for painting. Individual components are itemised separately in division AR-12 — use this item only for a complete overhaul.
	Repair
	Interior
	No.

	1.3
	AR-8.12
	08 71 (Door hardware)
	European lock + handle
	EN 12209 / EN 1935
	Supply, install, test and hand over European lock + handle. The works include all screws, keeps and fixings, adjusted and left fully operable. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.4
	AR-10.02
	08 51 (Metal windows)
	New steel window (approx. 1.20 × 1.00 m)
	EN 14351-1
	Supply, install, test and hand over a new steel window, approximate size 1.20 × 1.00 m — exact dimensions to be confirmed from site survey before fabrication. The works include a hot-rolled or pressed steel frame and opening sash in sections not less than 1.5 mm thick, single or double glazing as specified, glazing beads, gaskets and silicone perimeter seal, an insect screen, handles, stays and locking hardware, galvanising or anti-corrosive priming with two finish coats in the approved colour, and making good to the reveal. Measured per unit, complete and serviceable; where the actual size differs from the stated approximate size by more than 15%, the rate is to be adjusted pro rata on area.
	Supply & Install
	Interior
	No.

	1.5
	AR-10.04
	08 01 (Repair)
	Steel window — full repair (all hardware)
	EN 14351-1
	Full overhaul repair of a steel window: straighten/reweld frame and sash, replace hinges/handles/locks, treat corrosion, prime and repaint, reglaze as needed. Components itemised separately in AR-12.
	Repair
	Both
	No.

	1.6
	AR-7.08
	08 01 (Repair)
	Aluminum door/window — full repair (all hardware)
	EN 14351-1
	Full overhaul repair of an aluminum door or window: realign and refix leaf/sash, replace worn hinges, rollers, locks and handles, renew gaskets and silicone, and make fully operable. Individual components are also itemised separately in division AR-12 — use this item only for a complete overhaul.
	Repair
	Both
	No.

	1.7
	AR-11.02
	10 28 (Toilet accessories)
	Soap dispenser
	ISO 21542
	Supply, install, test and hand over Soap dispenser. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.8
	AR-11.03
	10 28 (Toilet accessories)
	Mirror
	ISO 21542
	Supply, install, test and hand over Mirror. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.9
	AR-11.04
	10 28 (Toilet accessories)
	Toilet paper holder
	ISO 21542
	Supply, install, test and hand over Toilet paper holder. The works include all fixings and brackets, mounted at the correct height, level and secure. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	 
	 

	1.1
	EL-2.01
	26 51 (Interior lighting)
	Lighting point — concealed (LED 40 W)
	EN 12464-1 / EN 60598
	Supply, install, test and hand over Lighting point — concealed (LED 40 W). The works include luminaire, wiring, back-box, switch and socket, and all items for a complete working point. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.11
	EL-6.09
	48 14 (Solar thermal)
	Solar water boiler 300 L — thermal collector type
	 
	Supply, install, test and commission Solar water boiler 300 L. The works include solar collector for hot climates (≥50 °C), tank, check valve and all connections. Measured per unit, complete and serviceable.
	Assembly
	Exterior
	No.

	1.12
	EL-3.03
	23 34 (Fans)
	Toilet exhaust fan
	EN 13141
	Supply, install, test and hand over Toilet exhaust fan. The works include wiring, conduit, protection and ducting connection, tested and commissioned. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	 
	 

	1.13
	PL-1.02
	22 42 (Fixtures)
	Western sitting WC (porcelain)
	EN 997 / EN 14688
	Supply, install, test and hand over Western sitting WC (porcelain). The works include triangle chrome stop valve, cistern and complete flush system, seat cover, concealed PPR water and PVC waste connections, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.14
	PL-1.20
	22 05 (WC repair)
	Repair Western (floor-standing) WC — complete with all accessories
	EN 997 / EN 14055
	The Contractor shall inspect every fixture and accessory of the WC and repair or replace any component found faulty, leaking, damaged, missing or not working properly, so that the whole WC is handed over fully functional. Repair and restore to full working order an existing Western floor-standing (close-coupled or low-level) WC, re-using the serviceable pan and cistern. The works include supply and fitting of a new fill (float) valve and flush (outlet) valve set; new push-button or lever handle; new cistern-to-pan rubber gasket (doughnut) and cistern fixing bolts with washers; new pan connector / flexible WC pan manifold to the soil pipe; new floor fixing bolt kit and caps; new chrome angle stop valve and braided flexible hose; new heavy-duty seat cover (European, min 1 cm); re-bedding and sealing of the pan base with sanitary silicone; leak and flush testing. Measured per WC repaired, complete and serviceable.
	Repair/Replace
	Interior
	No.

	1.15
	PL-1.04
	22 42 (Fixtures)
	Hand-held bidet (shattaf)
	EN 997 / EN 14688
	Supply, install, test and hand over Hand-held bidet (shattaf). The works include triangle chrome stop valve, cistern and complete flush system, seat cover, concealed PPR water and PVC waste connections, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.16
	PL-2.08
	22 05 (Sink repair)
	Repair single-basin sink — complete with P-trap, tap and all accessories
	EN 997 / EN 200 / EN 817
	The Contractor shall inspect the complete single-basin sink / wash basin and all its fixtures and accessories, and repair or replace any component found faulty, leaking, damaged, missing or not working properly, so that the whole unit is handed over fully functional. Re-using the serviceable basin, the works include: new or repaired tap / single-lever mixer (including cartridge, aerator and washers); new stainless-steel or chrome P-trap with waste outlet, plug and chain or pop-up, and overflow seals; new trap connector / waste pipe connection to the drain; new chrome angle (triangle) stop valves and braided flexible hoses for hot and cold; replacement of damaged water and waste fittings (elbows, unions, adaptors, rubber seals); checking, re-fixing or replacing the basin brackets / fixings; re-sealing of the basin to the wall or counter with sanitary silicone; and leak and flow testing. Measured per sink repaired, complete and serviceable. Where the basin itself is broken, it is replaced under PL-2.06 instead.
	Repair/Replace
	Interior
	No.

	1.17
	PL-2.03
	22 42 (Sinks)
	Wash basin – ceramic (supply & install only)
	EN 997 / EN 14688
	Supply and install Wash basin – ceramic (supply & install only). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Component
	Interior
	No.

	1.18
	PL-3.03
	22 42 (Trim)
	Short push/self-close tap (basin)
	EN 997 / EN 14688
	Supply and install Short push/self-close tap (basin). The works include brackets/stands, concealed PPR water and PVC waste connections, stainless P-trap, sealing and removal of the defective unit. Measured per unit, complete and serviceable.
	Component
	Interior
	No.

	1.19
	PL-7.03
	22 11 (Water pipe)
	PPR pipe 1″ (concealed)
	EN ISO 15874 / EN 809
	Supply, install, test and hand over PPR pipe 1″ (concealed). The works include breaking/chasing and re-concreting after approval, foam thermal insulation on exposed runs, copper connections, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.2
	PL-7.01
	22 11 (Water pipe)
	PPR pipe ½″ (concealed)
	EN ISO 15874 / EN 809
	Supply, install, test and hand over PPR pipe ½″ (concealed). The works include breaking/chasing and re-concreting after approval, foam thermal insulation on exposed runs, copper connections, and all joints, elbows and sockets. Measured per linear metre completed.
	Supply & Install
	Both
	m

	1.21
	PL-8.05
	22 13 (Floor drains)
	Floor drain 15×15 (stainless)
	EN 1401 / EN 1329
	Supply, install, test and hand over Floor drain 15×15 (stainless). The works include secure, watertight and corrosion-resistant fixing to the drainage line. Measured per unit, complete and serviceable.
	Supply & Install
	Interior
	No.

	1.22
	PL-8.04
	22 13 (Cleanouts)
	Cleanout 20×20 (stainless)
	EN 1401 / EN 1329
	Supply, install, test and hand over Cleanout 20×20 (stainless). The works include secure, watertight and corrosion-resistant fixing to the drainage line. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.23
	PL-3.06
	22 05 (Valves)
	Flow switch
	EN 200 / EN 817
	Supply, install, test and hand over Flow switch. The works include concealed hot/cold PPR connections, flexible tails, and removal of the defective unit. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.24
	PL-10.02
	22 08 (Commissioning)
	Pressure test
	EN 806-4
	Carry out Pressure test. The works include pressurising the system, checking all joints for leaks and issuing results. Priced as a lump sum for the complete works.
	Service
	Both
	LS

	 
	PW-1  WATER STORAGE TANKS

	1.25
	PW-1.03
	22 12 (Water tanks)
	Water tank 2000 L (PE, 3-layer)
	EN 12573
	Supply, install, test and hand over Water tank 2000 L (PE, 3-layer). The works include 3-layer polyethylene tank, all supply/outlet accessories and European valves for inlet and outlet. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.

	1.26
	PW-2.02
	22 11 (Pumps)
	Water pump ¾ HP (SS)
	EN ISO 15874 / EN 809
	Supply, install, test and hand over Water pump ¾ HP (SS). The works include stainless-steel construction, automatic switch and pressure control, control panel and all accessories, with head/flow confirmed on site. Measured per unit, complete and serviceable.
	Supply & Install
	Both
	No.
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