[bookmark: _Toc459799307]Annex 2 – Bid Form completed signed and stamped
· All bids must be typed; handwritten bids will not be considered. 
· The contract will be awarded to the lowest-cost technically compliant bid 
· Under this Framework Agreement, the quantities indicated are estimates only and may vary depending on LRC operational requirements. Purchases will be executed through the issuance of Purchase Orders on an as-needed basis during the validity period of the agreement. LRC does not guarantee the procurement of the full estimated quantities.
· In the event of any discrepancy between the unit price and the total price, LRC shall rely on the unit price without requesting clarification from the bidder. The unit price must be provided with no more than two decimal places.
· The quoted unit prices shall include all costs related to manufacturing, labor, packaging, transportation, unloading, delivery to the designated LRC warehouse, customs duties (if applicable), and all bank transfer charges.
· The bidder is allowed to propose only one option for each item.
	Lot #1: Pallet  

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item #
	Item/Milestone Required

	Unit of Measurement (UOM)
	Estimated
QTY/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery
(in calendar days) from the date of each Purchase Order.

	1
	EU Wooden Pallet
	Pcs
	1500
	
	
	
	
	

	2
	US Wooden Pallet
	Pcs
	600
	
	
	
	
	

	3
	EU Plastic Pallet
	Pcs
	1000
	
	
	
	
	

	4
	EU Plastic Pallet, Open Deck
	Pcs
	600
	
	
	
	
	

	5
	US Plastic Pallet
	Pcs
	1000
	
	
	
	
	

	6
	US Plastic Pallet, Open Deck
	Pcs
	600
	
	
	
	
	

	7
	Plastic Pallet Container with Lid
Size:120x80x80
	Pcs
	150
	
	
	
	
	

	8
	Plastic Pallet Container with Lid
Size:120x100x80
	Pcs
	150
	
	
	
	
	




	Lot #2: Wrapping Rolls

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item #
	Item/Milestone Required
	Unit of Measurement (UOM)
	Estimated
QTY/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery
(in calendar days) from the date of each Purchase Order.

	1
	Nylon Roll for Wrapping Machine
	Roll
	1000
	
	
	
	
	

	2
	Nylon Roll for Wrapping Machine Pre-Stretch
	Roll
	100
	
	
	
	
	

	3
	Nylon Roll for Manual Wrapping
	Roll
	1500
	
	
	
	
	

	4
	Bubble Wrap Roll
	Roll
	500
	
	
	
	
	



	Lot #3: Carton Boxes  

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item #
	Item/Milestone Required
	Unit of Measurement (UOM)
	Estimated
QTY/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery
(in calendar days) from the date of each Purchase Order.

	1
	Carton Box – 32 × 26 × 31 cm
	Piece
	1500
	
	
	
	
	

	2
	Carton Box – 40 × 40 × 20 cm
	Piece
	1500
	
	
	
	
	

	3
	Carton Box – 40 × 40 × 40 cm
	Piece
	1500
	
	
	
	
	

	4
	Carton Box – 60 × 40 × 40 cm
	Piece
	1500
	
	
	
	
	

	5
	Carton Box – 80 × 60 × 40 cm
	Piece
	1500
	
	
	
	
	

	6
	Carton Box – 80 × 60 × 60 cm
	Piece
	1500
	
	
	
	
	

	7
	Corrugated Kraft Carton Box (C-Flute, 460 gsm ±5%) – 49 × 29.2 × 25 cm
	Piece
	500
	
	
	
	
	

	8
	Corrugated Kraft Carton Box (C-Flute, 460 gsm ±5%) – 25 × 15 × 12.5 cm
	Piece
	500
	
	
	
	
	

	9
	Carton Box with Separate Top and Bottom Covers – 120 × 80 × 80 cm
	Piece
	500
	
	
	
	
	


	
	Lot #4: Packaging Accessories  

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item #
	Item/Milestone Required
	Unit of Measurement (UOM)
	Estimated
QTY/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery
(in calendar days) from the date of each Purchase Order.

	1
	Nylon Bags
	Piece
	10000
	
	
	
	
	

	2
	Paper Bag
	Piece
	5000
	
	
	
	
	

	3
	Solid Cardboard Edge Protector
	Piece
	5000
	
	
	
	
	

	4
	Cardboard Sheets
Size (L*W) 120*80 cm
	Piece
	5000
	
	
	
	
	

	5
	Cardboard Sheets
Size (L*W) 120*100 cm
	Piece
	2500
	
	
	
	
	

	6
	Plastic Sheet Size (L*W) 120*80 cm
	Piece
	1000
	
	
	
	
	

	7
	Plastic Sheet Size (L*W) 120*100 cm
	Piece
	1000
	
	
	
	
	

	8
	Adhesive Packaging Tape
	Piece
	5000
	
	
	
	
	



	Lot #5: Strapping Accessories

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item #
	Item/Milestone Required
	Unit of Measurement (UOM)
	Estimated
QTY/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery
(in calendar days) from the date of each Purchase Order.

	1
	Heavy load Strapping Roll PET
	meter
	1,000,000 
	
	
	
	
	

	2
	Light Load Strapping Rolls PP
	meter
	1,000,000 
	
	
	
	
	

	3
	Strapping Rolls PP
	meter
	100,000 
	
	
	
	
	

	4
	Metal Clips for Strapping
	Piece
	10000
	
	
	
	
	

	5
	Zip Ties Size: 4.8 x 350 mm
	Piece
	10000
	
	
	
	
	

	6
	Zip Ties Size: 7.6 x 450 mm
	Piece
	10000
	
	
	
	
	

	7
	Strapping Roll Dispenser
	Piece
	15
	
	
	
	
	


	
	Lot #6: Angle Grinder Accessories

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item # 
	Item/Milestone Required
	Unit of Measurement (UOM)
	Estimated 
Quantity 
/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
 Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery 
(in calendar days) from the date of each Purchase Order.

	1
	Thin Cutting Disc
	Piece
	200
	
	
	
	
	

	2
	Grinding Disc
	Piece
	200
	
	
	
	
	

	3
	Sanding Disc
	Piece
	200
	
	
	
	
	

	4
	Diamond Cutting Disc
	Piece
	200
	
	
	
	
	



	Lot #7: Warehouse Equipment 

	LRC To Complete
The bidder is not permitted to alter the section labelled “LRC to complete” below. Bidder is not allowed to use any other template.
	Bidder to Complete 

	Item # 
	Item/Milestone Required
	Unit of Measurement (UOM)
	Estimated 
Quantity 
/ 2 Years
	Unit Price in USD
Exclusive of VAT
	VAT (%)
	Unit Price in USD
 Inclusive of VAT
	Total Price in USD
Inclusive of VAT
	Lead time of delivery 
(in calendar days) from the date of each Purchase Order.

	1
	Hand Pallet Truck
	Piece
	40
	
	
	
	
	

	2
	Electric Pedestrian Pallet Truck
	Piece
	2
	
	
	
	
	

	3
	Electric Pedestrian Stacker 
	Piece
	5
	
	
	
	
	

	4
	Electric Counterbalance Trucks 3 Wheels 
	Piece
	2
	
	
	
	
	

	5
	Electric Counterbalance Trucks 4 Wheels 
	Piece
	1
	
	
	
	
	

	6
	Counterbalance Diesel 2T
	Piece
	5
	
	
	
	
	

	7
	Counterbalance Diesel 3.5 T
	Piece
	1
	
	
	
	
	

	8
	Wrapping Machine
	Piece
	6
	
	
	
	
	

	9
	Electric Strapping Machine
	Piece
	25
	
	
	
	
	

	10
	Manual Strapping Machine
	Piece
	30
	
	
	
	
	

	11
	Compact Professional High-Pressure Cleaner
	Piece
	10
	
	
	
	
	

	12
	Industrial Professional High-Pressure Cleaner
	Piece
	10
	
	
	
	
	

	13
	Single Disk Scrubbing Machine
	Piece
	5
	
	
	
	
	

	14
	Vacuum Cleaner
	Piece
	5
	
	
	
	
	

	15
	Mechanical Sweeper
	Piece
	5
	
	
	
	
	

	16
	Mobile Ladder
	Piece
	15
	
	
	
	
	

	17
	Retractable Ladder
	Piece
	20
	
	
	
	
	

	18
	Tool Kit
	Piece
	25
	
	
	
	
	

	19
	Cordless Angle Grinder
	Piece
	25
	
	
	
	
	

	20
	Cordless Screwdriver
	Piece
	25
	
	
	
	
	

	21
	Packaging Tape Dispenser
	Piece
	100
	
	
	
	
	

	22
	Cordless Blower
	Piece
	20
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ANNEX 3: DETAILED SPECIFICATIONS 
	ITEM #
	ITEM NAME
	Technical Specifications 
	Picture
	QTY / UOM

	Lot #1: Pallet  
Submission of 1 physical sample + Data sheet for each item is mandatory

	1
	EU Wooden Pallet
	Size:120x80x15
Load Capacity: 2000 kg
Rackable
	[image: EUR-pallet - Wikipedia]
	1500

	2
	US Wooden Pallet
	Size:100x120x15
Load Capacity: 2000 kg
Rackable
	[image: Block pallet open heavy weight 80x120 cm used | Foresco]
	600

	3
	EU Plastic Pallet
	Size:120x80x15
Load Capacity: 2000 kg
Rackable
	[image: Euro Pallets - Euro Plastic Pallets | Go Plastic Pallets®]
	1000

	4
	EU Plastic Pallet
Open Deck
	Size:120x80x15
Load Capacity: 2000 kg
Rackable
	[image: FDA Blue Pharmaceutical New Pallets - Open Deck Stackable Rackable  Multi-Trip | Nelson Company]
	600

	5
	US Plastic Pallet
	Size:100x120x15
Load Capacity: 2000 kg
Rackable
	[image: 1200 x 1000 Polyethylene Heavy Duty Tall Plastic Rackable Pallets - Buy solid top plastic pallets, HDPE pallet, hygiene pallets Product on Chinese provider of commercial and industrial grade plastic pallets and]
	1000

	6
	US Plastic Pallet
Open Deck
	Size:100x120x15
Load Capacity: 2000 kg
Rackable
	[image: Open Deck Pallets]
	600

	7
	Plastic Pallet Container with Lid
Size:120x80x80
	Size:120x80x80
Load Capacity: 2000 kg
Rackable
	[image: ]
	150

	8
	Plastic Pallet Container with Lid
Size:120x100x80
	Size:120x100x80
Load Capacity: 2000 kg
Rackable
	[image: ]
	150

	Lot #2 : Wrapping Roll 
 Submission of 1 physical sample + Data sheet for each item is mandatory

	1
	Nylon Roll for Wrapping Machine
	Height: 50 cm 
Weight: 16 kg 
Durable
Thickness: 35 Microns
Color: White, Black, Transparent
	
	1000

	2
	Nylon Roll for Wrapping Machine Pre-Stretch
	Height: 50 cm 
Weight: 16 kg
Pre-Stretch 250%
Durable
Thickness: 35 Microns
Color: White, Black, Transparent
	
	100

	3
	Nylon Roll for Manual Wrapping
	Height: 50 cm 
Weight: 3 kg 
Durable
Thickness: 35 Microns
Color: White, Black, Transparent
	
	1500

	4
	Bubble Wrap Roll
	Height: 50 cm
Length: 100 m
Bubble Size: 4 mm
Durable
Thickness: 35 Microns
Color: White, Black, Transparent
	[image: Large Bubble Wrap 1500mm x 50m - William Hayes]
	500

	Lot #3: Carton Boxes 
Submission of 1 physical sample + Data sheet for each item is mandatory

	Needed Qualifications for all of the items in Lot 3 
Durable, 5 Layers, Color: White, Brown, 5 Layers and reinforced corners

	1
	Carton Box – 32 × 26 × 31 cm
	Size(L*W*H): 32*26*31 cm

	[image: ]
	1500

	2
	Carton Box – 40 × 40 × 20 cm
	Size(L*W*H): 40 *40 *20 cm
	[image: ]
	1500

	3
	Carton Box – 40 × 40 × 40 cm
	Size(L*W*H): 40 *40 *40 cm
	[image: ]
	1500

	4
	Carton Box – 60 × 40 × 40 cm
	Size(L*W*H): 60 *40 *40 cm
	[image: ]
	1500

	5
	Carton Box – 80 × 60 × 40 cm
	Size(L*W*H): 80 *60 *40 cm
	[image: ]
	1500

	6
	Carton Box – 80 × 60 × 60 cm
	Size(L*W*H): 80 *60 *60 cm
	[image: ]
	1500

	7
	Corrugated Kraft Carton Box (C-Flute, 460 gsm ±5%) – 49 × 29.2 × 25 cm
	Flute corrugated board composed of Kraft
outside liner then fluting medium and inside liner Kraft.
Size(L*W*H): 49*29.2*25 cm
Made from 460 gsm +/-5% C 
	[image: ]
	500

	8
	Corrugated Kraft Carton Box (C-Flute, 460 gsm ±5%) – 25 × 15 × 12.5 cm
	Flute corrugated board composed of Kraft
outside liner then fluting medium and inside liner Kraft.
Size(L*W*H): 25*15*12.5 cm
Made from 460 gsm +/-5% C 
	[image: ]
	500

	9
	Carton Box with Separate Top and Bottom Covers – 120 × 80 × 80 cm
	Size(L*W*H): 120*80*80 cm
With Separate Top and Bottom Covers
	[image: ]

	500

	Lot #4: Packaging Accessories 
 Submission of 1 physical sample + Data sheet for each item is mandatory

	1
	Nylon Bags
	Size (L*W*H) 45*45*15 cm
Thickness: 60 Microns 
Capacity: 15 kg
	[image: ]
	
10000

	2
	Paper Bag
	Size (L*W*H) 33*32*20 cm
Capacity: 10-15 kg 

	[image: Buy 250 Pieces Kraft Brown Paper Bag Twisted Handle in Qatar Online – hotpack.qa]
	5000

	3
	Solid Cardboard Edge Protector

	Length: 150 cm
Width of legs (L-shape): 3 cm x 3 cm
Thickness: 5mm
	[image: Kraft Paper L Shape Angle Edge Board, Packaging Type: Box at ₹ 25/piece in Coimbatore]
	5000

	4
	Cardboard Sheets
Size (L*W) 120*80 cm
	Size (L*W) 120*80 cm
Thickness: 6mm
Material: Corrugated Cardboard
	[image: A4 A3 A2 A1 Double Wall Cardboard Corrugated Sheets Pads Divider Art Craft  Board | Packaging Shack]
	5000

	5
	Cardboard Sheets
Size (L*W) 120*100 cm
	Size (L*W) 120*100 cm
Thickness: 6mm
Material: Corrugated Cardboard
	[image: A4 A3 A2 A1 Double Wall Cardboard Corrugated Sheets Pads Divider Art Craft  Board | Packaging Shack]
	2500

	6
	Plastic Sheet Size (L*W) 120*80 cm
	Size (L*W) 120*80 cm
Thickness: 6mm
Material: Corrugated Plastic
	[image: Polypropylene (PP) Sheet – 3mm x 1m x 2m – Blue | Durable & Lightweight –  TOOLMART]
	1000

	7
	Plastic Sheet Size (L*W) 120*100 cm
	Size (L*W) 120*100 cm
Thickness: 6mm
Material: Corrugated Plastic
	[image: Polypropylene (PP) Sheet – 3mm x 1m x 2m – Blue | Durable & Lightweight –  TOOLMART]
	1000

	8
	Adhesive Packaging Tape
	Width:	48 mm
Length: 50 m
Thickness: 40–45 microns
Adhesive Type: Acrylic / Hot Melt
Color: Transparent
	[image: Box Sealing Tapes | 3M]
	5000

	Lot #5: Strapping Accessories 
Submission of 1 physical sample + Data sheet for each item is mandatory

	1
	Heavy load Strapping Roll PET
	Width: 12 mm, Thickness: 0.6 mm, Length: 2000 m, Weight: 20 kg, Heavy Loads
	[image: IDL Packaging 3/4" x .050" x 2400' Polyester (PET) Strapping Roll of 16" x  6" Core Size, 2500 lbs Break Strength, Green - UV, Water, and Rust ...]
	1,000,000 m

	2
	Light Load Strapping Rolls PP
	Width: 12 mm, Thickness: 0.6 mm, Length: 2000 m, Weight: 20 kg, Light Loads
	[image: ]
	1,000,000 m

	3
	Strapping Rolls PP
	Width: 6 mm, Thickness: 0.6 mm, Length: 2000 m, Weight: 20 kg, Light Boxes
	[image: Safeguard® White 6mm Light Duty Polypropylene Machine Strap | Ruffles Packaging]
	100,000 m

	4
	Metal Clips for Strapping
	Galvanized Metal
12 mm Strap

	[image: Buy 1000 Metal Buckles For 12mm PP Hand Pallet Strapping]
	10000

	5
	Zip Ties Size: 4.8 x 350 mm
	Size: 4.8 x 350 mm
	[image: qqqqqqq]
	10000

	6
	Zip Ties Size: 7.6 x 450 mm
	Size: 7.6 x 450 mm
	[image: qqqqqqq]
	10000

	7
	Strapping Roll Dispenser
	Heavy-duty powder-coated steel construction 
Integrated storage tray for tools and accessories 
Two solid rubber wheels for easy mobility 
Compatible strap width: 12 mm 
Roll capacity: up to 25–30 kg 
Corrosion-resistant steel frame 
Built-in strap guide/brake system 
	[image: Heavy Duty Strapping Dispenser for Poly and Steel Strapping - Durable  Tubular Frame Deluxe Strapping Cart : Amazon.in: Office Products]
	15

	Lot #6: Angle Grinder Accessories 
Submission of 1 physical sample + Data sheet for each item is mandatory

	General Requirement
· Durable
· Made in EU, USA or Japan

	1
	Thin Cutting Disc
	Disc Diameter: 115 mm (4.5") 
Bore Size: 22.23 mm 
Thickness: 1.0–1.6 mm 
Material Compatibility: Steel - Stainless steel - Sheet metal 
Abrasive Material: Aluminum oxide 
Reinforcement: Fiberglass reinforced
	[image: 5" ULTRA THIN CUTTING DISCS 125x1x22.23MM 50 PACK METAL STEEL STAINLESS ALUMINUM. Pac Performance Racing NZ]
	200

	2
	Grinding Disc
	Disc Diameter: 115 mm (4.5") 
Thickness: 6 mm 
Material Compatibility: Mild steel - Structural steel - Weld seams 
Abrasive Material: Aluminum oxide 
	[image: Semi-Flexible Grinding Disc]
	200

	3
	Sanding Disc
	Disc Diameter: 115 mm (4.5") 
Sizes: 40 grit - 60 grit - 80 grit - 120 grit 
Backing Material: Fiberglass backing plate 
Abrasive Material: Zirconia alumina 
	[image: R444 Expert for Metal Sanding Disc - Bosch Professional]
	200

	4
	Diamond Cutting Disc
	Disc Diameter: 115 mm 
Bore Size: 22.23 mm 
Segment Type: Segmented rim 
Application: Concrete – Brick – Masonry – Stone – Tile  
	[image: SP-T Universal diamond blade - Diamond blades and cup wheels - Hilti USA] 
	200

	Lot #7: Warehouse Equipment 
Submission of Data sheet for each item is mandatory. Failure to comply will result in disqualification.

	Needed Qualifications  for all the items
Durable, Parts Availability, Made in USA, Japan, or EU, 1 Year Warranty.

	1
	Hand Pallet Truck
	Technical Feature	
Travel Distance:	Short
Max Capacity: 2000 kg
Steering Wheel Material	Solid Rubber
Lift: 130 mm
Safety Features
Neutral:	Yes
	[image: Record BF Hand Pallet Truck - 685mm Width | Langley]
	40

	2
	Electric Pedestrian Pallet Truck
	Technical Feature	
Engine	Electric
Max Capacity	1200 – 1600 kg
Battery	Lead Acid
Mode	Electric
Speed	Adjustable
Lift	130 mm
Safety Features	
Horns	Yes
Emergency Stop Button	Yes
	[image: Jungheinrich Electric pedestrian pallet truck EJE 114/116/118/120 1.4 -  2.0t | Compass Forklifts]
	2

	3
	Electric Pedestrian Stacker 
	Technical Feature	
Engine	Electric
Max Lift Height	4300 mm
Max Capacity	1200 kg
Mast Type	Three Stage Free Lift
Mode	Electric
Battery	Led Acid
Safety Features
Autobrake	Yes
Emergency Stop Button	Yes
Horn	Yes
Load Backrest	Yes
Speed Reduction & High Elevation Sensor Yes
	[image: Wholesale Wholesale China Electric Pedestrian Stacker Manufacturers Suppliers – electric stacker electric forklift electric forklift truck battery forklift – Andy Manufacturer and Supplier | Andy]
	5

	4
	Electric Counterbalance Trucks 3 Wheels 
	Technical Feature	
Engine	Electric
Wheels	3
Max Lift Height	5000 mm
Max Capacity	1500 kg
Type	Double Motor
Mast Type	Three Stage Free Lift
Battery	Lead Acid
Controls	Levers
Side Shifter	Hydraulic
Safety Features	
Seatbelt	Yes	
Overhead Guard	Yes
Horns and Lights	Yes
Load Backrest	Yes
Emergency Stop Button	Yes
Operator Presence Detection	Yes
Anti-Rollback System	Yes
	[image: 3-Wheel Electric Counterbalance Truck | EFG 213-220 | Jungheinrich]
	2

	5
	Electric Counterbalance Trucks 4 Wheels 
	Technical Feature	
Engine	Electric
	Wheels	4
	Max Lift Height	5000 mm
	Max Capacity	2000 kg
	Type	Double Motor
	Battery	Lead Acid
	Mast Type	Three Stage Free Lift
	Controls	Levers
	Side Shifter	Hydraulic
Safety Features
	Seatbelt	Yes
	Overhead Guard	Yes
	Horns and Lights	Yes
	Load Backrest	Yes
	Emergency Stop Button	Yes
	Operator Presence Detection	Yes
	Anti-Rollback System	Yes
	[image: Electric Four-Wheel Pneumatic Tire Lift Truck | EFG C20Q-C40Q | Jungheinrich]
	1

	6
	Counterbalance Diesel 2T
	Technical Feature	
Engine	Diesel
Max Lift Height	5000 mm
Max Capacity	2000 kg
Mast Type	Three Stage Free Lift
Controls	Levers
Transmission Type	Power Shift
Tank Capacity	50 L
Side Shifter	Hydraulic
Safety Features	
Brakes	Hydraulic	
Must Include: Seatbelt, Overhead Guard, Horns and Lights, Load Backrest and Emergency Stop Button	
	[image: ]
	5

	7
	Counterbalance Diesel 3.5 T
	Technical Feature	
Engine	Diesel
Max lift height	4500mm
Max capacity	3500kg
Controls	Levers
Transmission Type	Power Shift
Lift Type	Three Stage Free Lift
Tank Capacity	50 L
Side Shifter	Hydraulic
Brakes	Hydraulic
Safety Features	
Wheels	Double Rim
Seatbelt	, Overhead Guard, Horns and Lights, Load Backrest and Emergency stop button
	[image: ]
	1

	8
	Wrapping Machine
	Technical Features	
Turntable Diameter	1650 mm
Turntable Speed	Adjustable up to 12 RPM
Turntable Weight Capacity	2000 kg
Turntable Height	Low-profile, approx. 75 mm
Automatic Turntable Stop Positioning	Yes
Turntable Ramp	Pallet Jack Loading
Film Roll Width	500 mm
Film Thickness Compatibility	15–35 microns
Auto Film Cut	Yes
Max Pallet Height	Adjustable up to 2400 mm
Load Height Sensor	Automatic Photo-Eye Sensor
Control Options	Digital Programmable Control Panel
Wrapping Modes	Manual & Automatic
Adjustable Top and Bottom Wraps	Yes
Number of Film Rotations per Cycle
Adjustable
Speed Adjustment	Film Carriage & Turntable Adjustable
Pause / Reset / Auto-Restart	Yes
Ready-To-Wrap Profiles	Yes
Tension Control	Electronically Adjustable
Film Carriage Speed	Up to 3 m/s Adjustable
Safety Features
Emergency Stop	Yes
Electrical Specifications	
Voltage	230V, 50/60 Hz
	[image: Robopac® Masterplat Semi-Automatic Stretch Wrapper]
	6

	9
	Electric Strapping Machine
	Technical Features	
Material Type	Polyester PET/PP
Strap Width	12–15 mm
Strap Thickness	0.6 mm
Cycle Speed	2.5 seconds per strap cycle
Production Rate	40 cycles per minute
Tension Force	Adjustable up to 300 kg
Tension Method	Automatic Tensioning
Sealing Type	Friction Weld
Sealing Strength	75% of Strap Break Strength
Control Panel & Programming	
User Interface	Digital Control Panel with LCD Display
Programmable Settings	Stores up to 10 Strap Settings
Error Display	Low Strap, Miss Feed & Sealing Error Alerts
Additional Features	
Brake Mechanism and Built-in Tool Tray	
Durable
Parts Availability 
Made in USA, Japan, or EU
	[image: ]
	25

	10
	Manual Strapping Machine
	Technical Features	
Material Type	Polyester PET/PP
Strap Width	12–15 mm
Strap Thickness	0.6 mm
Tension Force	Adjustable up to 300 kg
Tension Method	Manual Tensioning
Sealing Type	Mechanical Buckle
Additional Features	
Strapping Dispenser	Portable Steel Trolley
Brake Mechanism and Built-in Tool Tray	
Durable
Made in USA, Japan, or EU
	[image: 32mm Cord Strapping Tool Manual Strapping Machine - Strapping Machine and Packing Machine]
	30

	11
	Compact Professional High-Pressure Cleaner
	Technical Feature	
Type	Cold Water High-Pressure Cleaner
Operation	Vertical and Horizontal
Flow Rate	500 l/h
Working Pressure	150 bar / 15 MPa
Max Pressure	200 bar / 20 MPa
Max Inlet Temperature	60 °C
Number of Simultaneous Users	1
Mobility	Ultra
Connection Load	2.8 kW
Weight	25.7 kg
Dimensions (L × W × H)	380 × 360 × 930 mm
Current Type	1 / 230 / 50 Ph/V/Hz
Spray Gun	Easy Force
High-Pressure Hose	10 m / DN 6 / 250 bar
Spray Lance	840 mm
Triple Nozzle	Manual (0°/25°/40°)
Pressure Relief	Automatic
Pressure Cut-Off	Yes
Carrying Handle	Integrated
Push Handle	Retractable
Cylinder Head	Brass
Safety Features
Stable Horizontal Operation, Automatic Pressure Relief and Durable Quick-Release Couplings
	[image: ]
	10

	12
	Industrial Professional High-Pressure Cleaner
	Technical Feature	
Type	High-Pressure Cleaner
Motor Type	4-Pole Low-Speed Electric Motor 220V
Pump Type	Crankshaft Pump
Cylinder Head	Brass
Frame Type	Tubular Steel Frame
Flow Rate	450 – 600 l/h
Working Pressure	70 – 150 bar
Max Pressure	190 bar
Inlet Temperature	Up to 60 °C
Supply Voltage	1 / 216 – 244 / 50 Phases/V/Hz
Connected Load	3.4 kW
Power Cable Length	5 m
Nozzle Size	036
Water Inlet	1″
Weight (with accessories)	51.6 kg
Weight incl. Packaging	64.62 kg
Dimensions (L × W × H)	740 × 528 × 952 mm
High-Pressure Hose Length	10 m
High-Pressure Hose Specification	ID 8 / 315 bar
Spray Lance	840 mm
Pressure Switch-Off	Yes
Variable Pressure & Water Flow Control	Yes
Water Filter	Integrated
Oil Level Inspection Glass	Yes
Safety Features
Reduced Motor Speed, Low Engine Vibrations, Easy Service Access, Tool-Free Water Filter Removal
	[image: ]
	10

	13
	Single Disk Scrubbing Machine
	Performance	
Coverage Capacity	1500 – 2000 sqm/hour
Battery Runtime	2.5 – 3 Hours
Working Width	17 – 20 Inches (43 – 50 cm)
Brush Speed	150 – 200 RPM
Solution Tank Capacity	15 – 20 L
Recovery Tank Capacity	15 – 20 L
Battery
Battery Type	Lithium-Ion or Maintenance-Free Gel
Voltage	24 V
Battery Capacity	80 – 120 Ah
Charging Time	4 – 6 Hours
Construction	
Weight	40 – 70 kg
Chassis Material	Heavy-Duty Plastic or Stainless Steel
Wheels	Non-Marking Large Wheels
Ergonomics & Controls	
Handle Type	Adjustable Ergonomic Handle
Controls	User-Friendly Controls
Adjustable Functions	Speed, Water Flow, Brush Pressure
Additional Features	
Cleaning Modes	Scrubbing, Polishing, Buffing
Water Saving Mode	Eco-Mode
Attachments	Hard and Soft Brushes
Safety Features	
Emergency Stop Button	Yes
Low Battery Indicator	Yes
	[image: ]
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	Vacuum Cleaner
	Technical Feature	
Type	Wet & Dry Vacuum Cleaner
Voltage	220 – 240 V
Frequency	50 – 60 Hz
Air Flow	2 × 74 l/s
Vacuum Pressure	254 mbar / 25.4 kPa
Container Capacity	65 L
Container Material	Heavy-Duty Plastic
Rated Power	Max. 2760 W
Standard Nominal Width	ID 40
Cable Length	10 m
Noise Level	73 dB(A)
Weight	20 kg
Dimensions	600 × 480 × 920 mm
Suction Hose Length	4 m
Suction Tube Quantity	2 pcs
Suction Tube Material	Stainless Steel
Filter Type	Flat Pleated Filter
Filter Material	Cellulose Fibre
Filter Cleaning System	Semi-Automatic Ap Filter Cleaning
Fill Level Detection	Electronic
Drain Hose	Oil-Resistant
Mobility	2 Fixed Wheels + 2 Guide Rolls
Push Handle	Ergonomic Push Handle
Hose Storage	Yes
Accessory Holder	Yes
On-Board Storage	Yes
Safety Features	
Automatic Cut-Out	Yes
Protection Class	Class II
Sturdy Bumper	Yes
Stop Swivel Castor	Yes
	[image: ]
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	Mechanical Sweeper
	Technical Feature	
Type	Manual Walk-Behind Sweeper
Drive Type	Manual
Max. Area Performance	3920 m²/h
Main Working Width	480 mm
Working Width with 1 Side Brush	700 mm
Working Width with 2 Side Brushes	980 mm
Container Capacity Gross/Net	45 L / 20 L
Dimensions (L × W × H)	989 × 800 × 416 mm
Sweeping System	Sweeping Roller + 2 Side Brushes
Sweeper Roller Adjustment	6-Step Adjustable
Side Brush Adjustment	Infinitely Adjustable
Filter Type	Fine Dust Filter
Dust Control	Virtually Dust-Free Sweeping
Push Handle	Foldable & Height Adjustable
Handle Positions	3 Adjustment Positions
Storage Type	Space-Saving Parking Position
Home Base System	Yes
Indoor Use	Yes
Outdoor Use	Yes
Dirt Container	Large Ergonomic Waste Container
Sweeper Principle	Dustpan Principle
Roller Drive System	Roller Driven by Both Wheels
Maneuverability	Compact & Easy Handling
Safety Features	
Dust Protection Filter, Ergonomic Operation, Foldable Handle Lock, Stable Parking Position
	[image: ]
	5

	16
	Mobile Ladder
	Technical Feature	
Construction Material	Welded Steel or Aluminum
Hand Rail Height	90 cm Above Platform
Locking System	Hand Lever Locking Bar
Mobility	Two Wheels
Feet Type	Rubber Covered
Step Width	50 – 60 cm
Step Rise	20 – 25 cm
Platform Size	50 – 60 cm × 40 – 50 cm
Ladder Height	3 m
Safety Features	Hand Rails	Both Sides
Rubber Covered Feet, Locking Bar, Stable Platform
	[image: Mobile Safety Ladder – Durable & Secure Access Solution - Koeberg Industrial]
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	Retractable Ladder
	Technical Feature	
Ladder Type	Telescopic Ladder
Material	Heavy-Duty Aluminum or Fiberglass
Load Capacity	150 kg Minimum
Open Height	4.1 m
Closed Height	1.2m
Number of Rungs	8 + 8
Rung Dimensions	30 x 30 x 1.5 mm
Locking System	Automatic Safety Hinge Locks
Feet Type	Non-Slip Industrial Rubber Feet
Stability	Reinforced Wide-Base Frame
Corrosion Resistance	Yes
Weather Resistance	Yes
Storage Type	Foldable Compact Design
Safety Features	
Finger-Safe Locks, Stabilizer Bars	, Reinforced Rails	, Anti-Slip Rungs, Non-Slip Rubber Feet
	[image: ECOMAX Folding Ladder, 13 ft Aluminum Extension Ladder, 300 lbs Load  Capacity, Portable Telescoping Ladder with Non-Slip Rubber, Multi-Position  Step Ladders, for Working Indoor/Outdoor EM4X3L2 - Amazon.com]
	20

	18
	Tool Kit
	Technical Feature	
Tool Set Type	Professional Ratchet Wrench Tool Set
Number of Pieces	256 pcs
Case Material	Aluminum
Tray Type	4 Removable Trays
Handle Type	Removable Handle
Mobility	Wheels for Easy Transport
Lock Type	Key Lock Included
Tool Material	Chrome Vanadium Steel (CR-V)
Case Dimensions	38 × 24 × 51 cm
Weight	Over 15 kg
Tools	
Ratchet Type	Low Degrees Ratchets
Socket Sizes	4 mm – 30 mm
Combination Wrench Sizes	8 mm – 17 mm
Spark Plug Socket Sizes	16 mm / 21 mm
Hex Key Sizes	1.5 mm – 10 mm
Extension Bars	4 pcs
Flexible Extension Bar	Yes
Included Tools	Ratchets, Sockets, Wrenches, Screwdrivers, Pliers, Hex Keys
Ergonomics	
Storage Type	Organized Multi-Layer Tool Storage
Portability	Portable Rolling Toolbox
Application	Mechanical, Workshop, Household & Automotive Use
Construction Type	Heavy-Duty Professional Grade
Carrying Style	Pull Handle with Wheels
Security Feature	Lockable Aluminum Case
Finish Type	Chrome / Gold Finish
Tool Organization	Removable Tray System
	[image: ]
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	Cordless Angle Grinder
	Technical Features	
Motor Type	Brushless Motor
Power Equivalent	1500 W Mains-Powered Tool
Switch Type	Paddle Switch with Dead Man Function
Brake System	Fast Brake System
Disc Stop Time	1.5 Seconds
Anti-Vibration System	Integrated Auto-Balancer
Disc Change System	Tool-Free Quick System
Adjustable Guard	Tool-Free, Twist-Proof
Battery Position	Rotatable in 90° Steps
Safety Clutch	S-Automatic Mechanical Safety Clutch
Protection Features	Electronic Overload Protection, Soft Start, Restart Protection
Dust Protection Filter	Detachable
Safety Features	
Dead Man Function, Fast Brake System, Anti-Vibration System, Safety Bracket for Strap Attachment, Safety Clutch, Overload Protection, Restart Protection, Dust Protection Filter
Additional Features	
Battery x 2	Included
Charger x 1	Included
Hard Case x 1	Included
	[image: ]
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	Cordless Screwdriver
	Technical Features	
Motor Type	Brushless Motor
Hammer Drill Function	Yes
Gear Housing Material	Aluminum Diecast
Torque Control	Electronic Precision Stop
Overload Protection	Yes
Euro Collar Size	Ø 43 mm
Electronic Safety Shutdown	Yes
LED Work Light	Integrated with Afterglow Function
Belt Hook and Bit Case	Yes
Safety Features	Overload Protection	Yes
Electronic Safety Shutdown	Yes
Kickback Protection	Yes
LED Work Light	Yes
Precision Torque Control	Yes
Additional Features	
Battery x 2	Included
Charger x 1	Included
Hard Case x 1	Included
	[image: Cordless Drill - Hire Pro]
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	Packaging Tape Dispenser
	Technical Features	
Tape Width	50 mm
Tape Roll Diameter	76 mm
Frame Material	Steel
Handle Design	Enclosed Full-Hand Grip
Hand Through Roll
Tension Method	Adjustable Brake Mechanism
Operation	
One-Hand Dispensing and Cutting
Additional Features	
Safety Feature	Integrated Blade guard
Tape Compatibility	BOPP, PP, PVC, Acrylic
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	Cordless Blower
	Technical Feature	
Motor Type	Brushless Motor
Battery System	Lithium-Ion
Air Speed	Min 190 km/h
Air Volume	Min 12 m³/min
Speed Control	Variable Speed Trigger
Runtime	Min 15 Minutes at Max Power
Additional Features	
Battery x 2	Included
Charger x 1	Included
Hard Case x 1	Included
	[image: ]
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